PROJECT & SITE: ANGELA AUSX-5134														
Hole ID:	APGT07			Depth To:	120.71 EOH									
Logger:	Martin Childs/Russell Bray			AZI TN:										
Date:	13/09/2009 + 13/10/09			Plunge:										
ORIENTED CORE GEOTECHNICAL LOG														
Depth m	Rock Code	Hard Code	Structure Code	Stick Top/Bot	Beta Degrees	Alpha Degrees	Rough Code	InfThick Code	InfType Code	InfHard Code	Orientated Y/N	Comments Core sizes; Faults and other major structures.		
0.00	SAND	R1	Unconsolidated								No ori lines	Topsoil/sand		
0.10	CORE LOSS		Unconsolidated								No ori lines	3.75m of core loss		
3.85	K4	R2	Unconsolidated								No ori lines	Kaolomite		
3.90	ROCK	R6	Unconsolidated								No ori lines	Large cobbles		
4.10	CORE LOSS		Unconsolidated								No ori lines	2.7m of core loss		
6.80	ROCK	R5	Unconsolidated								No ori lines	Mary stones		
6.90	ROCK	R6	Unconsolidated								No ori lines	Large cobble + small stones 1.85cm of core loss		
7.05	CORE LOSS		Unconsolidated								No ori lines	RWG sand		
8.90	SAND	R1	Unconsolidated								No ori lines	Clay sand CGL		
9.20	CGL	R3	Unconsolidated								No ori lines	River sand		
9.40	SAND	R1	Unconsolidated								No ori lines	30cm of core loss		
9.60	CORE LOSS		Unconsolidated								No ori lines	Consolidated river sand		
9.90	SAND	R2	Unconsolidated								No ori lines	Weathered SST		
10.05	WEATHERED SST	R2	B								No ori lines	Slightly weathered SST		
10.50	SST	R3	B				4	1			No ori lines	Slightly weathered SST		
10.62	SST	R3	B				3	1			No ori lines	Slightly weathered SST		
10.74	SST	R3	CB			85	4	1			No ori lines	Slightly weathered SST		
10.78	SST	R3	B			90	2	1			No ori lines	Slightly weathered SST		
10.86	SST	R3	B			85	3	1			No ori lines	Slightly weathered SST		
11.04	SST	R4	B			80	4	1			No ori lines	Slightly weathered SST		
11.16	SST	R4	B			85	3	1			No ori lines	Slightly weathered SST		
11.30	SST	R4	B			85	4	1			No ori lines	Slightly weathered SST		
11.42	SST	R4	B			85	3	1			No ori lines	Slightly weathered SST		
11.62	SST	R4	B			90	3	1			No ori lines	Slightly weathered SST		
11.67	SST	R4	CB			90	3	1			No ori lines	Slightly weathered SST		
11.74	CORE LOSS		B			-					No ori lines	Core loss		
12.00	SST	R3	B			90	3	1			No ori lines	Slightly weathered SST		
12.07	SST	R3	B			85	3	1			No ori lines	Slightly weathered SST		
12.33	PBL SST	R3	B			85	4	1			No ori lines	Slightly weathered SST		
12.59	CORE LOSS		CB			-	-				No ori lines	11cm core loss		
12.70	ROCK	R5	B			-	3	1			No ori lines	Large cobbles		
12.78	SST	R3	B			90	4	1			No ori lines	Slightly weathered SST		
12.90	ROCK SST	R5+R3	B			-	-	-			No ori lines	Rock and smashed SST. Rock in RS SST is R3		
13.40	SST	R4	B			-	-	-			No ori lines			
13.53	SST	R4	B			85	4	1			No ori lines			
13.90	SST	R4	CB			90	3	1			No ori lines	"Core break, flat break"		
14.08	SST	R4	B			75	3	1			No ori lines	NB		
14.22	SST	R4	B			75	4	1			No ori lines	NB		
14.63	SST	R4	B			70	3	1			No ori lines	NB		
14.90	SST	R4	CB			80	4	1			No ori lines	CB		
15.13	SST	R4	CB			-	3	1			No ori lines	Spun core		
15.23	SST	R4	CB			90	3	1			No ori lines	"Spun core, flat core"		
15.34	SST	R4	CB			80	4	1			No ori lines	NB		
15.44	ROCK SST	R5+R4	CB			-	-	-			No ori lines	"Smashed core, rock is R5, SST is R4"		
15.56	SST	R4	CB			90	4	1			No ori lines	Spun core		
15.62	CORE LOSS		B			-	-	-			No ori lines	Core loss		
15.90	SST	R4	CB			85	3	1			No ori lines	Core break 		
15.95	SST	R4	CB			90	3	1			No ori lines	HB		
16.15	SST	R4	B			90	2	1			No ori lines	Spun core		
16.27	SST	R4	B			90	3	1			No ori lines	Spun core		
16.35	SST	R4	B			90	2	1			No ori lines	"No ori, spun core"		
16.45	SST	R4	B			80	4	1			No ori lines	NB		
16.51	SST	R4	B			85	3	1			No ori lines	Spun core		
16.58	SST	R4	B			80	4	1			No ori lines	NB		
16.71	CORE LOSS		B			-	-	-			No ori lines	29cm core loss		
16.90	CORE LOSS		CB			-	-	-			No ori lines	1m core loss		
17.90	SST	R4	CB			-	3	1			No ori lines	"Core break, spun core"		
18.00	CORE LOSS		B			-	-				No ori lines	Core loss		
18.52	SST	R4	B			90	3	1			No ori lines	Spun core		
18.61	SST	R4	B			90	3	1			No ori lines	Spun core		
18.70	SST	R4	CB			90	3	1			No ori lines	Spun core		
18.80	SST	R4	B			-	5	-			No ori lines	Crushed core		
18.93	SST	R4	CB			85	3				No ori lines	Spun core		
19.01	ROCK+SST	R5+R4	B			-	-	-			No ori lines	"Crushed core, rock is R5, SST is R4"		
19.12	CORE LOSS		CB			-	-	-			No ori lines	38cm core loss		
19.50	SST	R4	CB			90	3	1			No ori lines	Spun core		
19.59	ROCK	R5	B			-	3	1			No ori lines	Large stone		
19.62	SST	R4	B			80	3	1			No ori lines	NB on stone		
19.71	SST	R4	CB			85	3	1			No ori lines	Spun core		
19.80	SST	R4	CB			90	3	1			No ori lines	"Core break, spun core"		
19.90	SST	R4	B			85	3	1			No ori lines	Spun core		
20.00	SST	R4	CB		150	75	4	1				Spun core		
20.08	CORE LOSS		CB			-	-	-				22cm core loss		
20.30	PBL SST	R4	B			-	5	1			No ori lines	Crushed core		
20.41	SST	R4	CB			90	3	1			No ori lines	Spun core		
20.67	SST	R4	CB			90	4	1			No ori lines	Spun core		
20.75	SST	R4	CB			90	3	1			No ori lines	Spun core		
20.80	SST	R4	CB			90	4	1			No ori lines	"Core break, spun core"		
20.95	SST	R4	CB			90	3	1			No ori lines	Spun core		
21.10	CORE LOSS		CB			-	-	-			No ori lines	"No ori, 20cm core loss"		
21.30	ROCK	R5	B			-	3	1			No ori lines	"No ori, cobble"		
21.34	PBL SST	R4	CB			90	4	1			No ori lines	Spun core		
21.42	SST	R4	CB			-	3	1			No ori lines	Spun core		
21.60	SST	R4	B			80	4	1			No ori lines	"No ori, NB"		
21.80	SST	R4	CB			90	3	1			No ori lines	"No ori, core break, spun core"		
21.96	SST	R4	CB			85	3	1			No ori lines	Spun core		
22.05	SST	R4	CB			85	4	1			No ori lines	Spun core		
22.11	SST	R4	CB			85	4	1			No ori lines	Spun core		
22.23	CORE LOSS		CB			-	-	-			No ori lines	7cm core loss		
22.30	SST	R4	CB			90	3	1				"Core break, spun core"		
22.45	SST	R4	B	T	195	80	4	1				Core break		
22.80	SST	R4	B	T	330	85	4	1				Core break		
23.07	SST	R4	CB	T	275	80	4	1				Slightly spun core		
23.30	SST	R4	CB			80	4	1				NB		
23.63	CGL	R4 R3	B			80	4	1				"NB, SST is R4, MDST is R3"		
23.73	CORE LOSS		B			-	-	-				7cm core loss		
23.80	SST	R4	CB			85	5	1				"Slightly spun core, broken on MDST"		
23.92	CGL	R4 + R3	CB			85	3	1				"Spun core, SST is R4, mud is R3"		
23.99	CGL	R4 + R3	B			65	4	1				"NB broken on mud, SST is R4 mud is R3"		
24.00	CGL	R4 + R3	B			85	5	1				"NB broken on mud, SST is R4 mud is R3"		
24.17	CGL	R4 + R3	B			85	4	1				"NB broken on mud, SST is R4 mud is R3"		
24.25	MUD	R3	CB			90	4	1				Spun core		
24.30	SST	R4	CB			90	4	1				"CB, spun core"		
24.71	SST	R4	CB		160	85	3	1				NB spun core		
24.80	SST	R4	CB		195	80	5	1				CB		
25.07	CGL	R3	B			80	4	1			N 	"Crumbly core, NB"		
25.10	SST	R4	CB			85	4	1				Spun core		
25.29	SST	R4	CB			90	3	1				Spun core		
25.48	SST	R4	CB			90	3	1				Spun core		
25.64	SST	R4	CB			90	3	1				Spun core		
25.70	CORE LOSS		-			-	-	-				-		
26.00	SST	R4	CB			90	3	1				Spun core		
26.18	SST	R4	CB	T		90	3	1				Spun core starting to crumble		
26.30	SST	R4	B			-	4	1				Bedding disrupted on stone		
26.80	SST	R4	CB			90	3	1				"Core break, spun core"		
26.85	SST	R4	CB			85	4	1			N			
26.94	SST	R4	CB			75	4	1				Slightly spun core		
27.10	SST	R4	CB			90	3	1				Spun core		
27.54	SST	R4	CB			90	3	1				Spun core		
27.69	SST	R4	CB		15	75	4	1				HB		
27.80	PBL SST	R4	CB			75	4	1			N	CB 		
28.00	SST	R4	CB			90	3	1				Spun core		
28.29	SST	R4	CB			90	3	1				Spun core		
28.55	SST	R4	CB			90	3	1				Spun core		
28.67	SST	R4	CB			90	3	1				Spun core		
28.80	SST	R4	CB			90	3	1				"Core break, spun core"		
28.90	SST	R4	CB			85	4	1			N	Core break		
29.01	SST	R4	CB			90	4	1				Spun core		
29.08	SST	R4	CB			80	4	1			N	Spun core		
29.12	SST	R4	CB			90	3	1				Spun core		
29.28	SST	R4	CB			90	3	1				Spun core		
29.52	CGL	R4	CB			90	3	1				Spun core		
29.79	CGL	R4	CB			90	3	1				Spun core		
29.95	CGL	R4	CB			90	3	1				Spun core		
30.09	CGL	R4	CB			90	4	1				Spun core		
30.27	CGL	R4	CB			90	5	1				Large cobble in section		
30.37	SST	R4	B			-	4	1				Re-drilled mishapen core		
30.43	SST	R4	CB			90	4	1				Spun core		
30.60	PBL SST	R4	CB			90	3	1				Spun core		
30.80	ROCK SST	R4	B			90	5	1				"Large cobble in SST section, core break"		
30.91	SST	R4	CB			90	3	1				Spun core		
31.08	SST	R4	CB			85	4	1			N	Spun core		
31.17	CORE LOSS		B			-	-	-				70cm core loss		
31.87	SST	R4	CB			90	4	1				Spun core		
32.08	SST	R4	CB			90	3	1				Spun core		
32.29	SST	R4	B			-	5	-				Crushed core		
32.37	SST	R4	CB			90	3	1				Spun core		
32.60	SST	R4	CB			90	3	1				Spun core		
32.70	SST	R4	B			-	5	-				Crushed core		
32.80	SST	R4	B			90	4	1				Spun core		
33.05	CORE LOSS		B			-	-	-				25cm core loss		
33.30	SST 	R4	CB			90	3	1				"Core break, spun core"		
33.37	ROCK	R5	B			-	5	1				Pebbly section		
33.40	SST	R4	B			90	4	1				Spun core		
33.63	SST	R4	CB			90	3	1				Spun core		
33.75	SST	R4	CB		10	80	3	1				Core break		
33.93	SST	R4	B		-	80	4	1			N	Core face crumbling		
34.04	SST	R4	CB	T	245	80	3	1				HB		
34.11	SST	R4	B	T	260	80	3	1				NB		
34.18	SST	R4	B	T	255	80	3	1				NB		
34.24	SST	R4	BB	T	280	80	3	1				NB		
34.65	SST	R4	BB	T	265	70	4	1				NB		
34.96	SST	R4	CB	T	240	80	4	1				HB		
35.06	SST	R4	B	T	250	70	5	2				"NB, GS band"		
35.30	SST	R4	CB	T	225	80	4	1				Core break		
35.56	SST	R4	B	T	245	70	4	1				"NB, crumbling"		
35.90	SST	R4	CB	T	85	80	4	1			N	HB unable to orientate		
36.44	SST	R4	B	T	60	80	4	1			N	NB unable to orientate		
36.80	SST	R4	CB	T	45	80	5	1				"Core break, stone disrupting bedding, spun core"		
36.97	SST	R4	B	T	65	80	3	1				NB		
37.03	SST	R4	B	T	50	80	3	1				NB		
37.10	SST	R4	B	T	55	80	3	1				NB		
37.39	SST	R4	B	T	55	80	3	1				NB		
37.62	SST	R4	B	T	35	80	4	1				NB		
37.76	SST	R4	CB	T	60	75	3	1				HB		
37.90	SST	R4	B	T	70	75	4	1				NB		
38.32	SST	R4	B	T	45	85	3	1				NB		
38.71	SST	R4	CB	T	110	80	3	1				HB		
38.88	SST	R4	CB	T	65	80	4	1				HB		
39.30	SST	R4	CB	T	90	85	4	1				Core break		
39.64	CGL	R4	CB	T	80	85	4	1				HB		
39.85	SST	R4	B	-	-	-	5	1				"Crushed, re-drilled core, 0.4cm core loss"		
40.76	SST	R4	B	T	190	85	4	1				NB		
40.95	SST	R4	CB	T	150	85	4	1				HB		
41.49	SST	R4	CB	T	210	80	4	1				HB		
41.90	SST	R4	CB	T	185	70	4	1				HB		
42.30	SST	R4	CB	T	160	80	5	1				Core break		
42.55	SST	R4	CB	T	185	85	4	1				Core break		
42.66	SST	R4	CB	T	200	75	4	1				HB		
43.21	SST	R4	B	T	125	85	5	1				NB broken on stones		
43.62	SST	R4	CB	T	130	85	4	1				HB		
43.69	SST	R4	B	T	185	80	4	1				NB broken on stones		
43.95	SST	R4	CB	-	-	90	4	1				"Core break, flat break"		
44.35	SST	R4	CB	T	140	85	4	1				HB		
44.57	SST	R4	CB	T	20	80	5	1				HB		
44.90	SST	R4	B	T	105	80	3	1				NB		
45.20	SST	R4	B	T	165	80	3	1				NB		
45.54	CGL	R4	B	-	-	85	5	1			N	"NB broken on MDST & pebbles,bedding disrupted, orientation discrepancy"		
45.62	SST	R4	B	T	230	80	5	1				NB		
45.80	SST	R4	CB	T	145	80	4	1				Core break		
46.40	SST	R4	CB	T	160	80	3	1				HB		
46.50	SST	R4	B	T	175	70	4	1				HB		
46.69	SST	R4	B	T	135	70	5	1				Broken on large stone & MDST		
47.30	SST	R4	CB	-	-	90	4	1				"Core break, flat break"		
47.51	SST	R4	B	T	325	65	5	1				NB bedding disrupted on stones		
48.20	SST	R4	B	T	310	75	5	1				NB broken on large stones		
48.28	SST	R4	B	-	-	90	5	1				"NB broken on stone, bedding disrupted"		
48.51	SST	R4	B	T	300	80	4	1				NB		
48.80	SST	R4	CB	T	295	85	5	1				Core break		
49.19	ROCK SST	R4	B	-	-	-	5	1			Unreadable	"Broken on stones, unable to read"		
49.32	SST	R4	CB	-	-	90	4	1				Spun core		
49.62	SST	R4	CB	-	-	90	3	1				Spun core		
49.86	PBL SST	R4	B	-	-	65	5	1			N	Broken on stones		
49.93	PBL SST	R4	B	-	-	80	4	1			N	Broken on stones		
50.01	PBL SST	R4	B	-	-	-	5	1			N	Broken on stones		
50.05	SST	R4	B	-	-	80	4	1			N	HB		
50.16	SST	R4	CB	-	-	90	3	1			N	Spun core		
50.30	SST	R4	CB	-	-	75	5	1			N	Core break		
50.51	SST	R4	B	-	-	80	5	1			N	Broken on stones		
50.90	SST	R4	CB	-	-	85	4	1			N	HB		
51.10	SST	R4	B	-	-	70	5	1			N	Broken on stones		
51.37	SST	R4	CB	-	-	90	3	1			N	Spun core		
51.56	ROCKS	R5	B	-	-	-	5	1			N	Rocks only in this section		
51.63	PBL SST	R4	B	-	-	-	5	1			N	"Broken on cobbles, unreadable"		
51.80	SST	R4	B	-	-	-	5	1			N	Broken on stones		
52.36	SST	R4	B	-	-	85	5	1			N	Broken on stone bands		
52.48	SST	R4	CB	-	-	90	3	1			N	Spun core		
52.66	SST	R4	CB	-	-	65	5	1			N	Spun/smashed core		
52.80	SST	R4	CB	-	-	85	4	1			N	Spun core		
52.93	SST	R4	CB	-	-	90	3	1			N	Spun core		
53.19	SST	R4	CB	-	-	90	3	1			N	Spun core		
53.30	SST	R4	CB	-	-	90	4	1			N	"Spun core, core break"		
53.56	SST	R4	CB	-	-	80	4	1			N	HB		
53.73	SST	R4	CB	-	-	80	5	1			N	Spun/smashed core		
54.13	CGL	R4	B	-	-	80	5	1			N	NB		
54.27	CGL	R4	CB	-	-	90	3	1			N	Spun core		
54.55	CORE LOSS		B	-	-	-	-	-			N	25cm core loss		
54.80	CGL	R4	CB	-	-	75	5	1			N	"Core break, broken on mudstone"		
55.22	SST	R4	CB	-	-	80	4	1			N	"Spun core, broken on quartzite"		
55.40	SST	R4	CB	-	-	90	3	1			N	Spun core		
55.77	SST	R4	CB	-	-	90	3	1			N	Spun core		
56.09	SST	R4	B	-	-	-	5	1			N	"Smashed /broken core, no orientation"		
56.30	SST	R4	CB	-	-	-	5	1			Unreadable	"Core break, broken on large stones, unreadable"		
56.51	SST	R4	B	T	35	80	4	1				NB		
56.83	SST	R4	B	T	330	80	5	1				"NB, broken on large stones, bedding disrupted on stones"		
57.34	SST	R4	B	T	325	80	5	1				NB surface crumbling		
57.45	SST	R4	B	T	325	80	4	1				NB		
57.60	CORE LOSS		B	-	-	-	-	-				20 cm core loss		
57.80	CORE TAKEN FOR GT SAMPLE		-	-	-	-	-	-				46cm core taken for GT sample		
58.26	SST	R4	CB	T	170	75	4	1				HB		
58.42	SST	R4	CB	T	160	80	4	1				HB		
58.78	SST	R4	CB	T	285	80	4	1				HB		
58.97	SST	R4	CB	T	185	75	4	1				HB		
59.17	SST	R4	CB	T	230	85	4	1				HB		
59.30	SST	R4	CB	T	250	80	4	1				Core break		
59.43	CORE TAKEN FOR GT SAMPLE		-	-	-	-	-	-				33cm core taken for GT sample		
59.76	PBL SST	R4	B	-	190	85	4	1				NB		
59.97	SST	R4	B	-	-	90	5	1				"Broken on stones, flat break"		
60.14	ROCKS	R5	B	-	-	-	5	1				Rocky band		
60.18	SST	R4	B	T	5	80	5	1				"NB, broken stones, reading unreliable"		
60.62	SST	R4	B	T	295	85	4	1				Cobble		
60.69	SST	R4	B	T	255	75	5	1				Bedding disrupted by stones		
60.80	SST	R4	B	T	200	80	5	1				Surface crumbling		
61.28	SST	R4	B	T	210	85	5	1				"Bedding unreliable, broken on stones, NB"		
61.76	SST	R4	CB	T	50	80	4	1				HB		
62.74	SST	R4	CB	T	135	80	4	1				HB		
62.95	CORE TAKEN FOR GT SAMPLE		-	-	-	-	-	-				32cm taken for GT sampling		
63.27	SST	R4	CB	T	120	75	4	1				Broken on stone		
63.56	SST	R4	CB	-	145	80	4	1				HB		
63.80	SST	R4	CB	-	160	75	5	1				"Core break, broken on pebbles and mudstone"		
64.38	CGL	R4	B	-	200	85	5	1				"NB, broken on mudstone"		
64.55	CGL	R3	B	-	-	-	5	-				Shattered mudstone and SST CGL		
64.60	CORE TAKEN FOR GT SAMPLE		-	-	-	-	-	-				28cm core taken for GT sampling		
64.88	CORE TAKEN FOR GT SAMPLE		-	-	-	-	-	-				31cm core taken for GT sampling		
65.19	SST	R4	B	T	140	85	4	1				HB		
65.38	CGL	R4	CB	-	-	90	4	1				"HB, flat break"		
65.80	CGL	R4	B	T	110	80	4	1				NB		
65.89	CGL	R4	B	-	-	-	-	-				Smashed CGL		
65.92	CGL	R4	B	-	-	80	5	1			N	"Unable to orientate, NB, broken on mudstone"		
66.10	SST	R4	B	-	-	85	4	1			N	HB unable to orientate		
66.32	SST	R4	B	-	-	80	4	1			N	HB unable to orientate		
66.51	SST	R4	CB	-	-	70	3	1				Spun core		
66.80	SST	R4	CB	T	140	75	4	1				Core break		
67.10	SST	R4	CB	T	55	85	4	1				HB		
67.45	SST	R4	B	T	5	85	3	1				NB		
67.81	SST	R4	B	T	265	80	4	1				NB		
67.96	SST	R4	CB	T	190	80	5	1				"HB, bedding disrupted on stones"		
68.16	SST	R4	CB	-	-	90	3	1				Spun core		
68.38	SST	R4	B	T	245	85	4	1				NB		
68.82	SST	R4	CB	-	-	90	4	1				"HB, flat break"		
68.95	SST	R4	CB	T	290	80	4	1				HB		
69.16	SST	R4	CB	T	240	75	4	1				HB		
69.45	SST	R4	B	T	265	80	3	1				NB		
69.77	CGL	R4	B	-	-	-	-	-				Smashed CGL core		
69.80	SST	R4	CB	-	-	90	2	1				"Core break, spun core"		
70.17	SST	R4	CB	T	10	80	3	1				NB		
70.46	SST	R4	CB	T	10	80	3	1				NB		
70.61	SST	R4	CB	-	-	90	4	1				"HB, flat break"		
70.92	SST	R4	CB	-	-	90	3	1				Spun core		
71.41	SST	R4	CB	-	-	85	4	1			No ori lines	HB		
71.56	SST	R4	CB	-	-	80	4	1			No ori lines	HB		
72.09	CORE LOSS		CB	-	-	-	-	-				15cm core loss		
72.24	SST	R4	CB	-	-	90	4	1				Spun core		
72.43	SST	R4	CB	-	95	75	4	1				NB		
72.63	SST	R4	CB	-	100	75	4	1				HB		
72.73	SST	R4	B	-	-	90	4	1				HB		
72.80	SST	R4	CB	T	80	85	4	1				Core break		
73.05	SST	R4	B	T	120	80	5	1				"NB, broken on MDST"		
73.55	PBL SST	R4	B	T	330	80	5	1				"NB, broken on large stones  "		
74.44	ROCK SST	R4 + R5	B	-	-	-	5	1				"NB, SST is R4, rock is R5. Embedded rock unreadable"		
74.59	PBL SST	R4	B	-	-	-	4	1				"NB broken on large cobble, unreadable"		
75.11	PBL SST	R4	CB	-	-	90	5	1				Spun core		
75.32	SST	R4	CB	T	80	80	4	1				HB		
75.42	SST	R4	CB	-	-	90	4	1				Spun core		
75.80	SST	R4	CB	T	285	85	4	1				Core break		
75.91	CGL	R4	B	T	265	70	5	1				Bumpy slickside section in break. Bedding distorted by stone		
76.07	CORE TAKEN FOR GT SAMPLE		-	-	-	-	-					118cm core taken for sampling		
77.25	SST	R4	B	T	215	85	4	1				NB		
77.93	SST	R4	CB	T	160	85	4	1				HB		
78.54	CGL	R4	CB	T	195	70	5	1				HB broken on mudstone		
78.69	SST	R4	CB	-	-	-	4	1				"Re-drill, mishapen core, unreadable"		
78.80	SST	R4	CB	T	-	90	4	1				Spun core		
79.61	CGL	R4	B	T	130	80	4	1				Broken on MDST		
79.75	SST	R4	CB	T	50	85	4	1				HB		
80.47	SST	R4	B	T	205	75	4	1				NB		
80.69	SST	R4	B	T	210	75	4	1				NB		
81.15	SST	R4	B	T	130	85	4	1				NB broken on stones		
81.46	SST	R4	CB	T	145	85	4	1				NB		
81.58	SST	R4	B	T	200	80	4	1				HB		
81.67	CGL	R4	CB	T	10	80	5	1				NB broken on stones and MDST		
81.80	SST	R4	CB	T	190	85	4	1				"CB, broken on MDST"		
82.50	SST	R4	CB	T	210	85	4	1				"HB, broken on MDST"		
83.49	SST	R4	CB	T	140	80	4	1				HB		
84.12	SST	R4	CB	-	-	90	3	1				Spun core		
84.26	SST	R4	B	-	-	85	5	1			N	"NB, broken on organic matter"		
84.42	SST	R4	CB	-	-	85	4	1			N	HB		
84.57	SST	R4	CB	-	-	90	3	1				Spun core		
84.80	CGL	R4	CB	-	-	85	4	1			N	Core break		
85.36	CGL	R3	CB	-	-	90	5	1				"HB, flat break on MDST"		
85.46	CORE TAKEN FOR GT SAMPLE		-	-	-	-	-	-				112cm taken for sampling		
86.58	SST	R4	CB	-	-	90	2	1				Sawn end		
87.12	SST	R4	B	T	275	65	4	1				NB 		
87.30	SST	R4	CB	T	235	75	4	1				HB		
87.80	CGL	R4	CB	T	165	85	4	1				Core break 		
88.20	SST	R4	CB	T	215	80	4	1				HB		
89.10	SST	R4	CB	T	290	85	4	1				HB		
89.54	SST	R4	B	T	185	80	5	1				"NB, core crumbling"		
89.64	SST	R4	B	T	160	85	4	1				"NB, surface crumbling"		
90.03	CGL	R4	B	-	-	-	3	1				Cobble obstructing reading		
90.46	CGL	R4	B	T	170	75	5	1				Broken on MDST		
90.65	PBL SST	R4	B	T	190	85	4	1				Broken on stone		
90.73	ROCK SST	R4 R5	B	-	-	-	-	-				"Cobble obstructing reading, rock is R5, SST is R4"		
90.80	PBL SST	R4	CB	-	-	90	5	1			N	"Core break, flat break"		
90.95	PBL SST	R3	B	-	-	80	5	1			N	Bedding disrupted on rocks		
91.06	PBL SST	R3	B	-	-	90	5	1			N	Bedding disrupted on cobble		
91.10	PBL SST	R4	B	-	-	80	5	1			N	Broken on stones		
91.55	PBL SST	R4	B	-	-	85	5	1			N	Broken on stones		
91.60	PBL SST	R4	CB	-	-	85	4	1			N	Slightly spun core		
91.82	PBL SST	R4	B	-	-	70	5	1			N	"Broken on cobble, surface crumbling, NB"		
92.07	SST	R4	B	-	-	75	5	1			N	"NB, surface crumbling"		
92.58	PBL SST	R4	CB	-	-	90	3	1			N	Spun core		
92.76	PBL CGL	R4	CB	-	-	80	5	1			N	"HB, broken on stones"		
92.85	PBL CGL	R4	CB	-	-	90	5	1			N	Spun core		
92.92	PBL CGL	R4	BB	-	-	75	5	1			N	"NB, broken on mudstone"		
93.34	SST	R4	CB	-	-	90	3	1			N	Spun core		
93.52	SST	R4	B	T	195	80	4	1				NB surface crumbling		
93.70	SST	R4	CB	T	145	85	4	1				HB		
93.80	SST	R4	CB	T	170	80	5	1				Core break		
93.99	PBL SST	R4	B	-	-	-	3	1				Reading obstructed by large cobble		
94.20	SST	R4	B	T	140	80	5	1				"Surface crumbling, HB, broken on mud"		
94.59	SST	R4	CB	T	165	85	4	1				"HB, surface crumbling"		
95.15	SST	R4	B	T	155	80	4	1				"NB, broken on pebbles"		
95.54	SST	R4	CB	T	210	80	4	1				HB		
95.70	SST	R4	B	-	-	-	-	-				"NB, broken on large stone, disrupting bedding reading"		
96.18	SST	R4	B	T	230	75	4	1				-		
96.44	SST	R4	CB	-	-	90	4	1				-		
96.67	SST	R4	B	T	310	75	4	-				-		
96.80	CORE TAKEN FOR GT SAMPLE		 	-	-	-	-	-				211cm of core taken for sampling		
98.91	SST	R4	B	T	260	75	5	1				Broken on mudstone		
99.28	SST	R4	B	-	-	-	5	1				Bedding disrupted on stone		
99.80	SST	R4	CB	T	215	85	4	1				Core break		
100.13	SST	R4	CB	T	230	75	4	1				HB		
100.65	SST	R4	B	T	260	70	5	2				"Broken on mudstone vein, NB"		
101.04	SST	R4	CB	T	265	80	4	1				HB		
101.63	SST	R4	B	T	290	80	4	1				NB		
102.05	SST	R4	CB	T	275	85	4	1				HB		
102.31	PBL SST	R4	CB	-	-	90	3	1				Spun core		
102.80	SST	R4	CB	-	-	90	4	1			N	"Core break, unable to orientate"		
102.93	SST	R4	CB	-	-	85	4	1				HB		
103.04	SST	R4	CB	-	-	90	2	1				Spun core		
103.50	SST	R4	CB	-	-	85	4	1			N	"Core break, no orientation"		
103.88	SST	R4	CB	-	-	85	4	1			N	HB		
104.38	SST	R4	B	-	-	80	4	1			N	NB		
104.85	SST	R4	CB	-	-	90	4	1			N	"HB, no orientation, flat break"		
105.00	SST	R4	CB	T	125	85	3	1				Core break		
105.35	SST	R4	CB	-	-	-	4	1				"Core break, broken on stone"		
105.55	SST	R4	B	T	310	80	4	1				NB		
105.69	SST	R4	CB	T	115	85	4	1				HB		
106.00	SST	R4	B	T	90	80	4	2				"NB, broken on mudstone, crumbly surface"		
106.64	SST	R4	CB	T	170	80	4	1				HB		
107.51	SST	R4	CB	T	340	75	4	1				HB		
107.78	CORE LOSS		-	-	-	-	-	1				Core loss		
107.91	SST	R4	CB	-	-	90	3	1				Spun core		
108.00	SST	R4	CB	T	5	80	4	1				Core break		
108.22	SST	R4	B	T	170	85	4	1				NB		
108.54	SST	R4	B	-	-	80	4	1			N	"HB, unable to orientate"		
108.85	SST	R4	B	-	-	70	5	1			N	"NB on stone, unable to orientate"		
109.25	SST	R4	B	-	-	-	-	-				3cm broken core		
109.26	SST	R4	CB	-	75	75	4	1				HB		
109.40	SST	R4	CB	-	-	85	4	1				Core break		
109.50	SST	R4	CB	-	-	90	4	1				Spun core		
109.87	SST	R4	B	T	340	80	4	1				NB		
110.40	SST	R4	CB	T	170	85	4	1				Core break		
111.02	SST	R4	CB	T	-	90	4	1				"HB, flat break"		
111.28	SST	R4	CB	T	155	80	4	1				HB		
111.37	SST	R4	CB	T	230	85	4	1				HB		
111.65	SST	R4	CB	T	130	80	4	1				"HB, broken on stone "		
111.80	SST	R4	CB	T	315	85	4	1				Core break		
112.14	SST	R4	B	T	305	80	5	1				"NB, broken on stone"		
112.82	CGL	R4	B	T	130	75	5	1				"NB, broken on MDST"		
112.89	SST	R4	CB	-	-	90	3	1				Spun core		
113.07	SST	R4	CB	T	160	85	3	1				HB		
114.01	SST	R4	CB	T	290	85	4	1				HB		
114.20	SST	R4	B	T	70	85	4	1				NB		
114.80	SST	R4	CB	-	-	90	4	1				"Core break, flat break"		
115.34	SST	R4	B	-	-	90	5	1				"NB, broken on stones, flat break"		
115.73	SST	R4	CB	T	140	80	5	1				"HB, broken on stones"		
116.68	SST	R4	B	T	175	70	4	1				HB		
117.43	SST	R4	B	-	-	90	4	1				NB		
117.80	PBL SST	R4	CB	-	-	90	4	1				Core break		
118.39	MUD CGL	R3	B	-	-	-	5	1				"NB, shattered mudstone"		
118.41	CGL	R4	B	T	195	80	3	1				"NB, broken on MDST"		
118.72	SST	R4	B	T	285	80	4	1				"NB, broken on stone"		
119.32	SST	R4	CB	T	170	80	4	1				HB broken on stone		
119.61	SST	R4	B	T	220	70	5	1				NB shattered on mudstone		
120.17	SST	R4	B	T	175	80	4	1				NB		
120.71	SST	R4	B	T	230	80	4	1				NB EOH		
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
														
