PROJECT & SITE: ANGELA AUSX-5134													
Hole ID:	APGT02			Depth To:	137.85 EOH								
Logger:	Russell Bray			AZI TN:									
Date:	07/10/09			Plunge:									
ORIENTED CORE GEOTECHNICAL LOG													
Depth m	Rock Code	Hard Code	Structure Code	Stick Top/Bot	Beta Degrees	Alpha Degrees	Rough Code	InfThick Code	InfType Code	InfHard Code	Comments Core sizes; Faults and other major structures.		
38.20	-										"Broken core, PQ core"		
40.96	SST	R4	J				3	1					
41.05	SST	R4	J				5	1					
45.80	BST	R4	B				3	1					
47.11	SST	R4	B	B	150	75	3	1					
47.23	SST	R4	B	T	330	75	3	1					
47.33	SST	R4	B	B	150	75	3	1					
47.38	SST	R4	B	T	330	75	3	1					
47.85	SST	R4	B	B	160	75	3	1					
48.10	SST	R4	B	T	340	70	3	1					
48.48	SST	R4	J	B	110	80	4	1					
49.10	CGL	R5	CO				5	1			Ground on cobbles		
49.25	SST	R4	CO				5	1					
50.90	CGL	R5	CO				5	1					
50.95	SST	R4	CO				5	1			Broken and ground on cobbles		
50.80	CGL	R5	CO				5	1			1 boulder		
52.90	SST	R4	CO				5	1					
53.76	CGL	R5	CO				5	1			Broken on cobbles		
57.30	SST	R4	CO	T	150		5	1			"Broken on cobbles, number of places"		
58.22	SST	R4	J	T		90	3	1			Ground + core axis		
58.65	SST	R4	B	T	215	90	3	1			Mica rich		
58.83	SST	R4	J	-		90	2	1			"CB, ground axis"		
59.08	SST	R4	J	-		90	2	1			"CB, ground axis"		
59.30	SST	R4	J	-		90	2	1			"CB, ground axis"		
59.50	SST	R4	J	-		90	2	1			"CB, ground axis"		
59.57	SST	R4	B	B	152	80	3				-		
59.80	SST	R4	B	T		80	3				No orientation		
60.15	SST	R4	B	T		75	3				No orientation		
60.25	SST	R4	B	T		70	3				No orientation		
61.05	SST	R4	BB	T		65	3	1			"Mica/SST, no orientation"		
61.31	SST	R4	CB	T		85	3				"End ground, spun core, no orientation"		
61.45	SST	R4	B	T		70	4				"Clay in break, no orientation"		
61.57	SST	R4	B	T		80	4	2			"Clay infill, no orientation"		
61.66	SST	R4	CB	T		90	3				"Spun core, no orientation"		
61.87	SST	R4	CB	T		80	4				"End crumbling, broken, no orientation"		
61.98	SST	R4	CB	T		90	2				"Spun core, no orientation"		
62.25	SST	R4	B	T		75	3				-		
62.92	SST	R4	B	T		85	3				"Weather damage, no orientation"		
63.15	SST	R4	B	T		80	3				"Weather damage, crumbling"		
63.39	SST	R4	B	T	274	80	3				-		
63.55	SST	R4	B	T		75	3				"Swollen, water damage"		
63.60	SST	R4	CB	B	165	80	3				-		
63.96	SST	R4	B	T	338	80	3				-		
64.30	SST	R4	B	T	342	85	3				HB		
64.46	SST	R4	CB	T		90	2				Spun core		
64.94	SST	R4	B	T		75	3				Broken on cobble		
65.27	SST	R4	CB	T		90	2				"Spun core, no orientation"		
65.73	SST	R4	B	T		75	3				No orientation		
65.93	SST	R4	B	T		85	3				-		
66.13	SST	R4	CB	T		90	2				Spun core		
66.60	SST	R4	CB	T		90	2				Spun core		
66.81	SST	R4	B	T		65	2	2			"Mud/mica infill, no ori"		
66.89	SST	R4	BB	T		65	3	2			"Mud/mica infill, no ori"		
69.03	SST	R4	B	T		90	3				"End crumbling, rounded"		
69.15	SST	R4	B	T		70	3				"Broken in clumps, no ori"		
69.20	SST	R4	CB	T		90	2				"Spun core, no orientation"		
69.29	SST	R4	CB	T		90	2				"Spun core, no orientation"		
69.60	SST	R4	CB	T		90	2				"End rounded, spun core, no ori"		
70.90	SST	R4	CB	T		90	2				"Spun core, no orientation"		
71.26	SST	R4	CB	T		90	2				"Spun core, no orientation"		
71.93	SST	R4	CB	T		90	2				"Spun core, no orientation"		
72.17	SST	R4	B	T		80	4				"Mud , no ori"		
72.27	SST	R4	CB	T		90	2				"Spun core, no orientation"		
72.49	SST	R4	B	T		90	2				"End rounded, spun core"		
72.50	SST	R4	CB	T		90	2				"End rounded, spun core"		
72.67	SST	R4	CB	T		90	2				"Spun core, no orientation"		
73.00	SST	R4	B	T		85	3				No orientation		
73.17	SST	R4	CB	T		90	2				"Spun core, no orientation"		
73.54	MDST	R4	CB	T		90	3				"Unreliable, spun core, no ori"		
73.66	MDST	R4	B	T	286	80	3				"Mica mud bedding, broken on stone"		
73.87	MDST	R4	CB	T		90	2				Spun core		
74.23	SST	R4	CB	T		90	2				"End rounded, spun core"		
74.65	SST	R4	CB	T		90	2				Spun core		
74.86	SST	R4	B	T		75	3				-		
74.94	SST	R4	CB	T		90	2				Spun core		
75.50	SST	R4	CB	T		90	2				Spun core		
77.00	SST	R4	B	T		85	4				Pebble content		
77.31	SST	R4	B	T		80	2				Broken on cobble		
78.06	SST	R4	B	T		70	4				-		
78.16	SST	R4	CB	T		90	2				Spun core		
78.27	SST	R4	B	T		85	3				-		
78.50	SST	R4	CB	T		90	2				Spun core		
79.03	SST	R4	CB	T		90	2				Spun core		
79.22	SST	R4	B	T		80	3				-		
79.53	SST	R4	CB	T		90	2				Spun core		
79.96	SST	R4	CB	T		90	2				Spun core		
80.18	SST	R4	B	T		80	3				-		
80.80	SST	R4	CB	T		90	2				Spun core		
81.09	SST	R4	CB	T		90	2				"End rounded, spun core"		
81.33	SST	R4	CB	T		90	2				Spun core		
83.20	SST	R4	CB	T		90	2				Spun core		
83.34	SST	R4	B	T		85	3				-		
83.57	SST	R4	CB	T		90	2				Spun core		
83.80	SST	R4	CB	T		90	2				"End rounded, spun core"		
83.87	SST	R4	CB	T		90	2				"End rounded, spun core"		
84.19	SST	R4	CB	T		90	2				Spun core		
84.34	SST	R4	CB	T		90	2				Spun core		
84.50	SST	R4	CB	T		90	2				Spun core		
84.70	SST	R4	CB	T		90	2				Spun core		
85.32	SST	R4	B	T		80	2				-		
85.50	SST	R4	B	T		80	3				-		
85.59	SST	R4	J	T		80	3				-		
85.73	SST	R4	CB	T		90	2				Spun core		
85.87	SST	R4	CB	T		90	2				"End rounded, spun core"		
86.05	SST	R4	CB	T		90	2				Spun core		
86.23	SST	R4	CB	T		90	2				"End rounded, spun core"		
86.50	SST	R4	CB	T		90	2				Spun core		
86.95	SST	R4	CB	T		90	2				Spun core		
87.07	SST	R4	B	T		65	3				HB		
87.34	SST	R4	CB	T		90	2				Spun core		
87.50	SST	R4	CB	T		90	2				Spun core		
88.50	SST	R4	CB	T		90	2				Spun core		
88.88	SST	R4	CB	T		90	2				Spun core		
89.12	SST	R4	CB	T		90	2				Spun core		
89.31	MDST	R4	BB	T		70	2				-		
89.50	SST	R4	CB	T		90	2				Spun core		
90.13	SST	R4	CB	T		85	2				Spun core		
91.50	SST	R4	CB	T		90	2				"End rounded, spun core"		
91.69	SST	R4	B	T		70	3				-		
91.77	SST	R4	CB	T		90	2				Spun core		
91.99	SST	R4	B	T		75	3				Broken on cobble		
92.97	SST	R4	B	T		80	3				Broken on stone		
93.13	SST	R4	CB	T		90	2				Spun core		
93.60	SST	R4	B	T		85	3				-		
93.79	SST	R4	B	T		80	3				-		
94.38	SST	R4	B	T		80	3				-		
94.60	SST	R4	B	T		80	3				Broken on stone		
94.72	SST	R4	B	T		75	3				Broken on stone		
95.37	SST	R4	B	T		85	3				Broken on cobble		
95.80	SST	R4	B	T		80	3				Broken on cobble		
96.15	SST	R4	B	T		70	3	1			Clay/mud infill		
96.60	SST	R4	B	T		75	3				End weathered		
96.75	MDST	R4	B	T		75	3				Broken on stone		
98.44	SST	R4	B	T		75	3				High clay content		
98.77	SST	R4	B	T		65	3	1			Clay infill		
99.00	SST	R4	B	T		85	3	1			Clay infill		
99.17	SST	R4	BB	T		65	3	1			MDST		
100.29	SST	R4	CB	T		90	3				Spun core		
100.54	SST	R4	B	T		85	3				Broken on stone		
100.95	SST	R4	B	T		85	3				-		
101.73	SST	R4	BB	T		75	4	2			Clay mica		
101.97	MDST	R4	BB	T		75	3				-		
102.15	MDST	R4	BB	T		75	3				-		
102.21	MDST	R4	BB	T		75	3				-		
102.31	MDST	R4	BB	T		75	3				-		
102.60	MDST	R4	B	T		80	3				-		
102.64	MUD	R4	BB	T		80	2				-		
102.67	MUD	R4	BB	T		80	2				-		
102.72	MUD	R4	BB	T		80	2				-		
102.79	MUD	R4	BB	T		80	2				-		
102.83	MUD	R4	BB	T		80	2				-		
102.90	MUD	R4	BB	T		80	2				-		
102.92	MDST	R4	B	T		80	3				-		
103.06	MDST	R4	B	T		80	3				-		
103.89	SST	R4	B	T		80	3				-		
103.92	SST	R4	B	T		80	3				Broken on stone		
104.07	SST	R4	BB	T		85	3				-		
104.42	SST	R4	B	T		90	3				-		
104.63	SST	R4	B	T		80	3				Broken on stone		
104.80	SST	R4	CB	T		85	3				HB		
105.10	SST	R4	CB	T		80	3				HB		
105.62	SST	R4	B	T		85	3				Broken on cobble		
106.57	SST	R4	CB	T		85	3				HB		
106.79	SST	R4	B	T		85	3				-		
107.31	SST	R4	B	T		85	3				Broken on stone		
107.42	SST	R4	B	T		80	3				-		
107.67	SST	R4	CB	T		90	2				-		
107.98	SST	R4	CB	T		90	2				-		
108.07	SST	R4	B	T		90	2				Broken on cobble		
108.33	SST	R4	B	T		80	2	1			Clay		
108.60	SST	R4	CB	T		85	3				HB		
108.83	SST	R4	BB	T		75	2				Mica bedding		
109.21	SST	R4	B	T		85	2				HB		
109.43	SST	R4	B	T		85	3				Broken on stone		
110.15	SST	R4	CB	T		80	3				HB		
110.46	SST	R4	BB	T		75	3				-		
111.01	SST	R4	BB	T		85	3				HB		
111.23	SST	R4	B	T		85	3				Broken on stone		
111.60	SST	R4	B	T		85	3				-		
111.97	SST	R4	B	T		80	3				-		
112.50	SST	R4	BB	T		80	2	1			Mudstone		
112.59	MDST	R3	BB	T		80	2				-		
112.95	SST	R4	CB	T		85	3				HB		
113.84	SST	R4	B	T		85	3				-		
113.94	SST	R4	B	T		80	3				Broken on stone		
114.60	SST	R4	CB	T		80	4				HB		
114.75	SST	R4	B	T		80	3				-		
115.67	SST	R4	B	T		80	3				Broken on stone		
116.65	SST	R4	CB	T		85	3				HB		
116.90	SST	R4	B	T		85	3				-		
117.60	SST	R4	CB	T		90	2				Spun core		
118.06	SST	R4	B	T		85	2				-		
118.50	SST	R4	B	T		85	2				-		
119.37	SST	R4	B	T		70	2				Broken on stone		
119.54	SST	R4	B	T		85	2				-		
120.33	SST	R4	B	T		85	2				-		
120.60	SST	R4	B	T		80	3				-		
121.23	SST	R4	B	T		80	3				-		
122.07	SST	R4	B	T		80	5				Broken on stone		
122.19	SST	R4	J	T		25	3				-		
122.89	SST	R4	CB	T		85	3				HB		
123.04	SST	R4	B	T		80	4	3			Organic infill		
123.16	SST	R4	B	T		75	3				-		
123.28	SST	R4	B	T		75	3				-		
123.40	SST	R4	B	T		75	3				-		
123.60	SST	R4	B	T		80	3				-		
123.72	SST	R4	CB	T		90	2				Spun core		
124.67	SST	R4	CB	T		85	3				HB		
124.85	SST	R4	CB	T		85	3				HB		
125.63	SST	R4	CB	T		70	3				HB		
126.60	SST	R4	CB	T		85	3				HB		
127.49	SST	R4	B	T		85	3				-		
127.99	SST	R4	B	T		80	3				Broken on cobble		
128.23	MDST	R4	BB	T		75	3				Mica		
128.44	SST	R4	B	T		80	3				-		
129.37	SST	R4	B	T		80	3				-		
129.60	SST	R4	CB	T		80	3				HB		
130.29	SST	R4	CB	T		80	3				HB		
130.98	SST	R4	B	T		80	3				Broken on stone		
131.24	SST	R4	CB	T		85	3				HB		
132.94	SST	R4	B	T		75	3				-		
133.17	SST	R4	B	T		80	3				-		
133.24	SST	R4	B	T		75	3				-		
133.40	SST	R4	B	T		75	3				-		
133.49	SST	R4	B	T		75	3				-		
132.60	SST	R4	CB	T		80	3				HB		
133.17	SST	R4	B	T		80	5				Broken on stone		
133.43	SST	R4	B	T		70	4				Broken on cobble		
134.04	SST	R4	CB	T		90	3	2			HB		
134.30	MDST	R4	BB	T		70	3	1			Mica		
135.01	MDST	R4	B	T		85	3				HB		
135.09	CLAY	R3	B	T		80	3				Clay		
135.22	CLAY	R3	B	T		80	3				MDST		
135.60	SST	R4	CB	T		85	3				Clay infill		
135.91	SST	R4	CB	T		85	3				HB		
136.85	SST	R4	B	T		80	3				-		
137.22	SST	R4	B	T		80	3				-		
137.48	SST	R4	B	T		80	4				Clay infill		
137.78	SST	R4	CB	T		85	3				HB		
137.85	SST	R4	B	T		85	3				EOH		
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
