PROJECT & SITE: ANGELA AUSX-5134													
Hole ID:	APGT09					Depth To:	258.45 to 399.9 EOH						
Logger:	Martin Childs/Russell Bray					AZI TN:							
Date:	18/09/2009 + 27/09/09 + 14/10/09					Plunge:							
ORIENTED CORE GEOTECHNICAL LOG													
Depth m	Rock Code	Hard Code	Structure Code	Stick Top/Bot	Beta Degrees	Alpha Degrees	Rough Code	InfThick Code	InfType Code	InfHard Code	Comments Core sizes; Faults and other major structures.		
258.45	SST	R4	CB	T	-	90	4	1			"No orientation, flat break"		
258.72	SST	R4	B	T	-	85	4	1			"Broken on stone, no orientation"		
259.25	SST	R4	CB	T	-	90	3	1			"Spun core, no orientation"		
259.40	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
259.50	SST	R4	CB	T	-	UNREADABLE		1			"Core break, smashed surface, no orientation"		
259.68	SST	R4	CB	T	-	90	3	1			"Spun core, no orientation"		
260.26	SST	R4	B	T	-	85	4	1			"NB on stone, no orientation"		
260.67	SST	R4	B	T	-	UNREADABLE		1			"Broken on stone, water damage, no orientation"		
261.15	SST	R4	B	T	-	75	4	1			"NB, no orientation"		
261.69	SST	R4	B	T	-	80	4	1			"Broken on MDST, no orientation"		
261.86	CGL	R4	B	T	-	90	5	1			"NB, broken on MDST, no orientation"		
262.07	CGL	R4	B	T	-	85	5	1			"NB, broken on MDST, no orientation"		
262.23	SST	R4	CB	T	-	90	3	1			"Spun core, no orientation"		
262.50	SST	R4	CB	T	-	90	4	1			"Core break, no orientation"		
262.96	SST	R4	CB	T	-	80	4	1			HB		
263.35	SST	R4	B	T	-	85	4	1			NB		
263.67	SST	R4	B	T	-	85	4	1			NB		
263.84	SST	R4	B	T	-	-	5	1			Core has been water damaged		
264.18	CGL	R4	B	T	-	-	5	1			Core has been water damaged		
264.58	SST	R4	B	T	-	70	5	1			"NB, crumbling surface"		
264.83	SST	R4	B	T	-	80	4	1			NB		
264.98	SST	R4	B	T	-	80	5	1			"NB, core surface crumbling"		
265.43	SST	R4	B	T	-	85	4	1			NB		
265.50	SST	R4	CB	T	-	75	4	1			Core break		
265.63	SST	R4	CB	T	-	85	4	1			HB		
266.21	SST	R4	CB	T	-	80	4	1			"HB, broken on MDST"		
266.51	SST	R4	CB	T	-	85	4	1			HB		
266.56	SST	R4	CB	T	-	85	4	1			HB		
266.64	SST	R4	CB	T	-	80	4	1			HB		
267.30	SST	R4	B	T	-	70	4	1			"NB, broken on stone"		
267.47	SST	R4	CB	T	-	85	4	1			HB		
268.18	MUD CGL	R3	CB	T	-	90	3	1			Spun on smashed MDST		
268.32	MUD	R3	B	T	235	75	5	1			NB		
268.39	MUD	R3	B	T	240	70	5	1			HB		
268.42	SST	R4	CB	T	255	75	4	1			"HB, broken on MDST"		
268.50	SST	R4	CB	T	150	85	5	1			"Core break, broken on stone"		
269.27	SST	R4	B	T	90	80	4	1			"HB, bedding disrupted on stone"		
269.39	SST	R4	B	T	70	65	4	1			"NB, broken stone and MDST"		
269.67	SST	R4	B	T	95	80	4	1			NB		
269.98	SST	R4	CB	T	260	85	4	1			HB		
270.13	SST	R4	CB	T	-	90	4	1			"HB, flat break"		
270.26	SST	R4	CB	T	-	90	4	1			"HB, flat break"		
270.33	SST	R4	CB	T	-	90	4	1			HB		
270.51	SST	R4	BB	T	155	85	4	1			"NB, broken on stone and MDST"		
270.85	SST	R4	B	T	130	80	4	1			Bedding disrupted on stone		
271.05	SST	R4	B	T	170	75	4	1			"NB, surface crumbling"		
271.20	SST	R4	CB	T	140	70	4	1			HB		
271.33	SST	R4	B	T	280	85	4	1			NB		
271.50	SST	R4	BB	T	-	75	4	1			"CB, broken on shattered mica SST, no orientation"		
272.10	SST	R4	CB	T	-	70	4	1			"HB, broken on stone, no orientation"		
272.40	SST	R4	B	T	-	75	4	1			"NB, broken on stone, no orientation"		
273.60	SST	R4	B	T	-	75	4	1			"NB, broken on stone, no orientation"		
272.81	SST	R4	B	T	-	85	4	1			"NB, crumbling section, no orientation"		
272.85	SST	R4	B	T	-	80	4	1			"NB, broken on MDST, no orientation"		
273.08	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
273.23	SST	R4	B	T	-	80	5	1			"NB, broken on large stone, surface curmbling, no orientation"		
273.46	SST	R4	B	T	-	-	5	1			"NB, bedding disrupted on large stones, no orientation"		
273.62	SST	R4	CB	T	-	90	5	1			"Spun core, surface crumbling, no orientation"		
273.89	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
274.06	SST	R4	CB	T	20	85	4	1			HB		
274.50	SST	R4	CB	T	130	85	4	1			CB 		
274.97	SST	R4	CB	T	195	80	4	1			HB		
275.38	SST	-	B	T	-	-	-	1			Damp water damaged section		
275.43	SST	R4	B	T	-	70	-	1			Crumbling  		
275.94	SST	R4	B	T	-	90	4	1			"Water damage, no orientation"		
276.52	SST	R4	B	T	-	60	4	1			"NB water damage, no orientation"		
276.63	SST	R4	B	T	-	75	4	1			"NB water damage, no orientation"		
276.92	SST	R4	CB	T	195	85	4	1			HB		
277.50	SST	R4	CB	T	245	90	4	1			CB		
278.01	SST	R4	CB	T	-	90	4	2			"HB, no orientation"		
278.21	SST	R4	B	T	-	70	5	2			"NB, MDST infill, no orientation"		
278.60	SST CGL	R4	BB	T	-	90	4	1			"NB, MDST CGL, no orientation"		
278.78	MUD	R3	BB	T	-	90	3	1			"NB, MDST, no orientation"		
278.87	MUD	R4	BB	T	-	90	3	1			"Water damage, no orientation"		
278.94	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
279.35	SST	R4	B	T	-	90	4	2			"NB on MDST, no orientation"		
279.54	SST	R4	B	T	-	90	4	1			"NB on MDST, no orientation"		
279.92	SST	R4	CB	T	-	70	4	1			"HB, no orientation"		
280.07	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
280.25	SST	R4	BB	T	-	85	3	1			"NB, no orientation"		
280.50	SST	R4	CB	T	-	90	3	1			"CB, no orientation"		
280.84	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
280.97	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
281.20	SST	R4	BB	T	-	90	3	1			"NB, no orientation"		
281.31	SST	R4	BB	T	-	90	3	1			"NB, no orientation"		
281.74	SST	R4	BB	T	-	70	4	1			"NB broken on MDST, no orientation"		
281.81	SST	R4	CB	T	-	85	5	1			"HB, no orientation"		
281.97	SST	R4	B	T	-	90	5	1			"NB broken on MDST, no orientation"		
282.02	SST	R4	B	T	-	90	5	1			"NB broken on MDST, no orientation"		
282.16	SST	R4	B	T	-	85	4	1			"NB, water damage, no orientation"		
282.59	SST	R4	B	T	-	65	5	1			"NB, broken on stone, no orientation"		
282.73	SST	R4	CB	T	-	75	4	1			"NB crumbly texture, no orientation"		
282.94	SST	R4	B	T	-	80	4	1			"NB, broken on stone, no orientation"		
283.50	SST	R4	CB	T	-	85	3	1			"HB, no orientation"		
284.15	SST	R4	B	T	-	80	4	1			"NB, broken on stone, no orientation"		
284.27	SST	R4	CB	T	-	70	3	1			"HB SST MDST, no orientation"		
284.41	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
285.09	SST	R4	B	T	-	75	4	1			"NB on stone, no orientation"		
285.37	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
285.48	SST	R4	B	T	-	85	5	1			"NB on stone, no orientation"		
285.76	SST	R4	B	T	-	80	5	1			"NB on stone, no orientation"		
286.13	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
286.29	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
286.46	SST	R4	B	T	330	85	4	1			NB		
286.50	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
287.20	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
288.08	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
288.94	SST	R4	B	T	-	65	4	1			"HB water damage, crumbling stone, no orientation"		
289.06	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
289.14	SST	R4	B	T	-	75	4	1			"NB but end rounded off, no orientation"		
289.34	SST	R4	B	T	190	80	4	1			NB		
289.50	SST	R4	CB	T	-	80	4	1			"CB, no orientation"		
289.90	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
290.09	SST	R4	B	T	-	75	4	1			"NB on MDST, no orientation"		
290.48	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
290.69	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
290.86	SST	R4	CB	T	-	70	4	1			"HB, no orientation"		
291.55	SST	R4	B	T	-	85	4	1			"NB on MDST, no orientation"		
291.65	SST	R4	B	T	-	80	5	1			"NB on MDST, no orientation"		
291.70	SST	R4	B	T	-	70	5	1			"NB on MDST, no orientation"		
291.78	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
291.85	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
291.93	SST	R4	CB	T	-	80	5	1			"HB crumbly, no orientation"		
292.32	SST	R4	BB	T	20	85	3	2			End rounded formica		
292.50	SST	R4	CB	T	-	80	4	1			"CB, no orientation"		
292.67	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
293.22	SST	R4	B	T	-	85	4	1			"HB, no orientation"		
293.50	MUD	R3	B	T	-	75	3	2			"NB, no orientation"		
293.63	MUD	R3	BB	T	-	70	3	1			"HB, no orientation"		
293.86	SST	R4	BB	T	-	60	3	1			"HB, no orientation"		
294.25	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
294.42	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
294.57	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
294.61	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
295.34	SST	R4	B	T	-	80	4	1			"HB, no orientation"		
295.39	SST	R4	B	T	190	75	5	1			NB		
295.50	SST	R4	B	T	-	90	4	1			"NB flat break, no orientation"		
296.28	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
296.44	SST	R4	BB	T	-	70	5	1			"NB on MDST, no orientation"		
296.50	SST	R4	BB	T	-	70	5	2			"NB on MDST and formica, no orientation"		
297.25	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
297.63	SST	R4	B	T	-	85	4	1			"NB broken on stone, no orientation"		
297.88	SST	R4	BB	T	-	80	4	1			"NB, no orientation"		
298.02	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
298.19	SST	R4	B	T	-	85	3	1			"NB water damage, no orientation"		
298.28	SST	R4	B	T	208	80	3	2			NB water damage		
298.50	SST	R4	B	T	-	90	4	1			"CB, no orientation"		
298.71	SST	R4	B	T	-	65	4	1			"NB water damage, no orientation"		
299.14	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
299.43	SST	R4	B	T	-	70	4	1			"NB, no orientation"		
300.11	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
300.22	SST	R4	CB	T	-	70	4	1			"HB, no orientation"		
301.08	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
301.22	SST	R4	B	T	-	70	4	1			"NB on mud/formica, no orientation"		
301.42	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
301.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
301.93	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
302.06	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
302.27	SST	R4	CB	T	-	75	5	1			"NB broken on stone, no orientation"		
302.90	SST	R4	B	T	-	70	5	1			"NB on stone, no orientation"		
303.09	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
303.94	SST	R4	B	T	-	85	5	1			"NB, no orientation"		
304.37	SST	R4	B	T	140	85	4	1			NB		
304.50	SST	R4	CB	T	-	80	4	1			"NB spun core, no orientation"		
305.95	SST	R4	B	T	-	80	4	1			"NB broken on stone, no orientation"		
306.18	SST	R4	B	T	-	75	5	1			"NB on stone, no orientation"		
306.79	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
306.89	SST	R4	CB	T	-	90	4	1			"Spun core, no orientation"		
307.29	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
307.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
307.79	SST	R4	B	T	-	75	5	1			"CB on stone, no orientation"		
307.98	SST	R4	B	T	-	65	5	1			"NB on stone, no orientation"		
308.31	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
308.61	SST	R4	B	T	-	80	4	1			"NB on stone, no orientation"		
308.79	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
309.21	SST	R4	B	T	-	85	5	1			"NB on stone, no orientation"		
309.53	SST	R4	B	T	-	80	5	1			"NB on stone, no orientation"		
309.70	SST	R4	B	T	-	90	4	1			"NB spun core, no orientation"		
310.41	SST	R4	B	T	-	90	5	1			"NB, no orientation"		
310.50	SST	R4	B	T	-	85	5	1			"CB, no orientation"		
311.00	SST	R4	B	T	-	80	5	5			"NB MDST, no orientation"		
311.48	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
312.30	SST	R4	B	T	-	75	5	3			"NB on mud, no orientation"		
312.38	SST	R4	B	T	-	75	4	4			"NB, no orientation"		
312.60	CGL	R4	B	T	-	55	5	4			"NB on mud, no orientation"		
312.83	CGL	R4	B	T	-	70	5	1			"NB on stone, no orientation"		
313.10	CGL	R4	B	T	-	70	5	1			NB on stone		
313.31	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
313.40	SST	R4	CB	T	-	90	4	1			"Spun core, no orientation"		
313.50	SST	R4	CB	T	-	90	4	1			"CB, no orientation"		
314.13	SST	R4	B	T	-	80	4	1			"NB on stone, no orientation"		
315.09	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
315.56	SST	R4	B	T	-	85	5	1			"NB, no orientation"		
315.99	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
316.19	SST	R4	B	T	-	80	4	1			"NB crumbly, no orientation"		
316.38	SST	R4	B	T	350	80	4	1			NB		
316.50	SST	R4	B	-	-	-	-	1			Too broken to measure		
316.65	SST	R4	B	T	-	90	4	1			"NB on stone, no orientation"		
316.90	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
317.62	SST	R4	B	T	-	90	5	1			"NB on MDST, no orientation"		
317.72	SST	R4	B	T	-	90	5	1			"NB on MDST, no orientation"		
317.77	SST	R4	B	T	-	85	5	1			"NB on stone, no orientation"		
317.84	SST	R4	CB	T	-	80	4	1			"CB, no orientation"		
318.78	SST	R4	B	T	190	85	4	1			NB		
319.21	SST	R4	B	T	136	90	4	1			NB		
319.35	SST	R4	B	T	290	75	4	1			NB		
319.50	SST	R4	CB	T	-	90	4	1			"CB crumbling MDST, no orientation"		
319.71	SST	R4	CB	T	-	50	4	1			"HB, no orientation"		
320.10	SST	R4	B	T	-	90	4	1			"NB water damage, no orientation"		
320.44	SST	R4	CB	T	-	75	4	1			"HB crumbly, no orientation"		
320.60	SST	R4	B	T	-	80	5	1			"HB, no orientation"		
320.70	SST	R4	B	T	-	85	4	1			"HB, no orientation"		
321.03	SST	R4	B	-	-	80	5	1			"NB on MDST, no orientation"		
321.36	SST	R4	B	-	-	75	5	2			NB on MDST		
321.53	MUD	R3	B	T	-	-	-	1			"Crumbling to 322m, no orientation"		
322.00	SST	R4	B	T	-	80	4	2			"NB, no orientation"		
322.07	SST	R4	B	T	-	85	4	1			"NB on MDST, no orientation"		
322.37	SST	R4	B	T	145	70	5	1			NB		
322.50	SST	R4	CB	T	-	90	4	1			"CB, no orientation"		
323.13	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
323.40	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
323.99	SST	R4	B	T	-	80	3	1			"NB, no orientation"		
324.26	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
324.41	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
324.48	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
324.68	SST	R4	B	T	-	90	3	1			"NB spun core, no orientation"		
324.95	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
325.10	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
325.13	SST	R4	CB	T	-	75	4	1			"HB, no orientation"		
325.22	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
325.50	SST	R4	CB	T	-	90	3	1			"Spun core, no orientation"		
325.58	SST	R4	CB	T	-	90	3	1			"Spun core, no orientation"		
326.04	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
326.28	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
326.67	SST	R4	B	T	-	75	4	1			"NB, no orientation"		
326.95	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
327.15	SST	R4	B	T	-	75	3	1			"NB, no orientation"		
327.56	SST	R4	B	T	178	80	5	1			NB		
327.94	SST	R4	B	T	172	75	4	2			NB on MDST and formica		
328.03	SST	R4	B	T	260	80	4	1			NB on stone		
328.50	SST	R4	CB	T	-	90	4	1			"CB chipped from hammer, no orientation"		
328.84	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
329.64	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
329.76	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
329.84	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
330.32	SST	R4	B	T	-	70	3	1			"NB on stone, no orientation"		
330.72	SST	R4	CB	T	116	85	4	1			HB		
331.06	SST	R4	B	T	220	80	5	1			NB on stone		
331.50	SST	R4	CB	T	-	90	4	1			"Spun core, no orientation"		
332.44	SST	R4	CB	-	-	80	4	1			"CB, no orientation"		
333.61	SST	R4	B	T	156	85	4	1			NB		
334.30	SST	R4	B	T	200	80	4	1			NB on MDST and formica		
334.40	SST	R4	B	T	162	85	4	1			NB		
334.50	SST	R4	B	T	-	90	4	1			"NB, no orientation"		
341.13	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
341.21	SST	R4	B	T	-	90	4	1			"NB, no orientation"		
341.35	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
341.89	SST	R4	B	T	-	75	-	1			"NB water damage, no orientation"		
342.59	SST	R4	B	T	-	75	-	1			"NB, no orientation"		
342.79	SST	R4	B	T	-	75	-	1			"NB on stone, no orientation"		
342.80	SST	R4	B	T	-	70	2	1			"NB on MDST, no orientation"		
343.34	SST	R4	B	T	-	80	-	1			"NB, no orientation"		
343.50	SST	R4	B	T	-	85	-	1			"NB on stone, no orientation"		
343.67	SST	R4	B	T	-	75	-	1			"NB on stone, no orientation"		
344.46	SST	R4	B	T	-	75	-	1			"NB, no orientation"		
344.66	SST	R4	B	T	-	75	5	1			"NB on stone, no orientation"		
345.02	SST	R4	B	T	-	85	5	1			"NB on stone, no orientation"		
345.39	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
345.99	SST	R4	B	T	-	85	5	1			"NB on stone, no orientation"		
346.29	SST	R4	B	T	-	70	5	1			"NB on mud, no orientation"		
346.37	SST	R4	B	T	220	75	5	1			NB on stone		
346.50	SST	R4	CB	T	-	80	2	1			"CB, no orientation"		
346.81	ROCK	R5	B	T	-	90	2	1			"NB on stone, no orientation"		
346.89	SST	R4	B	T	-	85	4	1			"NB on stone, no orientation"		
347.08	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
347.93	SST	R4	B	T	-	85	5	1			"NB on stone, no orientation"		
348.05	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
348.98	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
348.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
349.88	SST	R4	B	T	-	75	4	1			"NB, no orientation"		
350.30	SST	R4	CB	T	-	90	4	1			"Spun core, no orientation"		
350.85	SST	R4	CB	T	-	75	4	1			"CB crumbling, no orientation"		
351.06	SST	R4	B	T	-	90	4	1			"NB, no orientation"		
351.74	SST	R4	B	T	172	80	4	1			NB		
352.38	SST	R4	B	T	190	85	4	1			NB		
352.50	SST	R4	CB	T	-	80	4	1			"CB, no orientation"		
352.62	SST	R4	CB	T	-	85	5	1			"HB, no orientation"		
352.86	SST	R4	B	T	-	80	5	1			"NB, no orientation"		
353.44	SST	R4	CB	T	-	85	4	1			"NB on stone, no orientation"		
353.56	SST	R4	B	T	-	90	4	1			"NB, no orientation"		
353.96	SST	R4	B	T	-	80	5	1			"NB on mud, no orientation"		
354.39	SST	R4	CB	T	-	85	5	1			"HB, no orientation"		
354.55	SST	R4	CB	T	-	80	4	1			"CB, no orientation"		
354.63	SST	R4	B	T	4	55	4	1			NB on stone		
355.50	SST	R4	CB	T	-	90	4	1			"CB end rounded, no orientation"		
355.77	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
356.36	SST	R4	B	T	234	85	4	1			NB		
356.61	SST	R4	B	T	18	85	5	1			NB on stone		
357.29	SST	R4	B	T	260	85	4	1			NB		
358.08	SST	R4	B	T	34	90	4	1			NB		
358.30	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
358.45	SST MUD	R4	B	T	-	75	3	1			"NB, no orientation"		
358.61	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
359.01	SST	R4	B	T	-	75	4	1			"NB, no orientation"		
359.18	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
359.30	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
359.39	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
360.12	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
360.24	SST	R4	B	T	-	70	5	1			"NB on rock, no orientation"		
360.40	SST	R4	B	T	-	90	5	1			"NB on rock, no orientation"		
360.72	SST	R4	B	T	-	85	4	1			"NB on mud, no orientation"		
360.84	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
361.07	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
361.16	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
361.40	SST	R4	CB	T	-	90	4	1			"CB end rounded, no orientation"		
361.96	SST	R4	CB	T	-	90	4	1			"CB, no orientation"		
362.89	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
363.30	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
363.38	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
363.84	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
364.05	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
364.15	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
364.23	SST	R4	B	T	-	90	4	1			"NB, no orientation"		
364.30	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
364.37	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
364.50	SST	R4	CB	T	-	75	3	1			"CB, no orientation"		
364.70	SST	R4	CB	T	-	75	4	1			"HB, no orientation"		
364.79	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
364.96	SST	R4	B	T	-	55	4	1			"NB on mud, no orientation"		
365.63	SST	R4	B	T	-	80	5	1			"NB on stone, no orientation"		
365.71	SST	R4	CB	T	-	75	4	1			"CB, no orientation"		
366.67	SST	R4	B	T	146	80	4	1			NB		
366.85	SST	R4	B	T	170	80	4	1			NB on stone		
367.19	SST	R4	B	T	226	75	4	1			NB on stone		
367.37	SST	R4	B	T	176	80	4	1			NB		
367.50	SST	R4	CB	T	-	90	4	1			CB		
367.65	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
367.91	SST	R4	B	T	-	75	4	1			"NB, no orientation"		
368.27	SST	R4	B	T	-	75	4	1			"NB, no orientation"		
368.44	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
367.87	SST	R4	B	T	-	75	4	1			"NB on mud, no orientation"		
369.20	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
369.31	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
369.93	SST	R4	B	T	-	70	4	1			"NB, no orientation"		
370.28	SST	R4	CB	T	192	80	4	1			HB		
370.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
371.04	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
371.38	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
371.68	SST	R4	B	T	-	75	4	3			"NB on mud, no orientation"		
371.83	SST	R4	CB	T	-	80	4	1			"NB on stone, no orientation"		
371.99	SST	R4	CB	T	-	75	4	1			"HB, no orientation"		
372.05	SST	R4	B	T	-	80	4	1			"NB, no orientation"		
372.48	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
372.95	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
373.37	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
373.46	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
373.50	SST	R4	CB	T	-	80	4	1			"CB, no orientation"		
373.63	SST	R4	CB	T	-	90	4	1			"HB spun core, no orientation"		
373.79	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
374.56	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
375.42	SST	R4	CB	T	-	85	4	1			"NB, no orientation"		
375.73	MUD	R3	BB	T	-	85	4	1			"NB, no orientation"		
375.77	MUD	R3	BB	T	-	85	4	1			"NB, no orientation"		
375.84	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
376.20	MUD	R3	BB	T	-	75	4	1			"NB, no orientation"		
376.27	SST	R4	BB	T	-	70	4	1			"NB, no orientation"		
376.38	SST	R4	BB	T	-	85	4	2			"NB on mud, no orientation"		
376.50	SST	R4	CB	T	-	90	4	1			"CB, no orientation"		
377.24	SST	R4	CB	T	-	90	4	1			"HB, no orientation"		
378.09	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
378.54	SST	R4	B	T	270	85	4	1			NB		
378.84	SST	R4	CB	T	330	85	4	1			HB		
379.04	SST	R4	CB	T	3	85	4	1			HB		
379.16	SST	R4	CB	T	2	75	4	1			HB		
379.34	SST	R4	CB	T	300	85	4	1			HB		
379.50	SST	R4	CB	T	-	90	4	1			"CCB, no orientation"		
379.94	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
380.92	SST	R4	B	T	-	85	5	1			"NB, no orientation"		
381.18	SST	R4	B	T	-	90	4	1			"NB on stone, no orientation"		
381.88	SST	R4	CB	T	254	85	4	1			HB		
382.50	SST	R4	CB	T	-	90	4	1			"CB, no orientation"		
382.77	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
383.16	SST	R4	BB	-	-	75	4	1			"NB on mud, no orientation"		
383.64	SST	R4	CB	-	-	85	4	1			"HB, no orientation"		
384.52	SST	R4	CB	-	-	80	4	1			"HB, no orientation"		
385.36	SST	R4	CB	-	156	80	4	1			HB		
385.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
386.22	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
386.32	SST	R4	B	T	-	85	4	1			"NB, no orientation"		
387.01	MUD	R3	BB	T	-	85	4	1			"NB, no orientation"		
387.06	SST	R4	CB	T	-	85	4	1			"NB, no orientation"		
387.90	SST	R4	CB	T	140	85	3	1			HB		
388.06	SST	R4	BB	T	150	80	3	1			NB		
388.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
388.78	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
389.56	SST	R4	CB	T	-	75	4	1			"NB, no orientation"		
389.75	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
390.06	SST	R4	B	T	-	80	3	2			"NB on mud, no orientation"		
390.41	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
390.70	SST	R4	CB	T	112	85	4	1			HB		
391.27	SST	R4	CB	T	204	85	4	1			HB		
391.50	SST	R4	CB	T	56	80	4	1			HB		
391.66	SST	R4	CB	T	50	80	4	1			HB		
392.52	SST	R4	CB	T	-	80	5	1			"HB, no orientation"		
392.87	SST	R4	B	T	-	80	3	1			"NB on formica, no orientation"		
393.40	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
394.23	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
394.39	SST	R4	CB	T	18	90	4	1			HB		
394.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
395.24	SST	R4	CB	T	-	75	4	1			"HB stoney, no orientation"		
396.08	SST	R4	CB	T	-	80	3	1			"HB formica, no orientation"		
396.64	SST	R4	CB	T	-	80	3	1			"NB, no orientation"		
397.05	SST	R4	CB	T	-	80	4	1			"HB, no orientation"		
397.50	SST	R4	CB	T	-	85	4	1			"CB, no orientation"		
398.02	SST	R4	CB	T	-	85	4	1			"HB, no orientation"		
398.58	SST	R4	CB	T	180	85	4	1			HB		
398.96	SST	R4	CB	T	258	85	4	1			HB		
399.50	SST	R4	CB	T	180	80	4	1			HB		
399.90	SST	R4	CB	T	100	80	4	1			HB EOH		
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
													
