GENERAL SPECIFICATIONS
The following are the general specifications for the surveys:

Area:				Renner Springs 1, N.T.

Configuration:		Gradient array
Line Spacing:		200m
Line Direction:		E-W
A space:			25m
Geophysical Transmitter:	GDD
Tx Current			variable
Tx Frequency		0.125 Hz
Geophysical Receiver:	GDD 16
Rx Readings:		Minimum 2/station
Field Data:			GDD format files
Processed Data:		AMIRA format

Area:				Renner Springs 2, N.T.

Configuration:		Gradient array
Line Spacing:		200m
Line Direction:		E-W
A space:			25m
Geophysical Transmitter:	GDD
Tx Current			variable
Tx Frequency		0.125 Hz
Geophysical Receiver:	GDD 16
Rx Readings:		Minimum 2/station
Field Data:			GDD format files
Processed Data:		AMIRA format

 
Area:				Masai West, N.T.

Configuration:		Gradient array
Line Spacing:		50m
Line Direction:		E-W
A space:			25m
Geophysical Transmitter:	GDD
Tx Current			variable
Tx Frequency		0.125 Hz
Geophysical Receiver:	GDD 16
Rx Readings:		Minimum 2/station
Field Data:			GDD format files
Processed Data:		AMIRA format

Area:				Helen Springs, N.T.

Configuration:		Gradient array
Line Spacing:		200m
Line Direction:		NE-SW
A space:			25m
Geophysical Transmitter:	GDD
Tx Current			variable
Tx Frequency		0.125 Hz
Geophysical Receiver:	GDD 16
Rx Readings:		Minimum 2/station
Field Data:			GDD format files
Processed Data:		AMIRA format


Data 

Raw data is direct from the GDD

AMIRA Located Data has been editted and averaged

ASEG Final Data, data has been written out with a ASEG format,

Note: At this stage there is no formal ASEG format for IP data
