H0002	Version	4
H0003	Date_generated	1-May-2018
H0004	Reporting_period_end_date	23-Mar-2018
H0005	State	Northern Territory
H0100	Tenement_no/Combined_report_no	EL30042
H0101	Tenement_holder	Teck Australia
H0102	Project_name	Reward
H0106	Tenement_operator	Teck Australia
H0150	250K_map_sheet_number	SE5303
H0151	100K_map_sheet_number	Borrowloola 6165 & Batten 6064
H0152	50K_map_sheet_number	NA
H0153	25K_map_sheet_number	NA
H0200	Start_date_of_data_acquisition	24-Mar-2017
H0201	End_date_of_data_acquisition	23-Mar-2018
H0202	Data_format	DL4
H0203	Number_of_data_records	37
H0204	Date_of_metadata_update	1-May-2018
H0301	Location_data_file	EL30042_2018_A_02_CollarsDrillhole.txt
H0302	Lithology_data_file	EL30042_2018_A_03_LithologyLogs.txt
H0303	Assay_data_file	EL30042_2018_A_04_DownholeAssays.txt
H0304	Survey_data_file	EL30042_2018_A_05_DownholeSurvey.txt
H0307	Lithology_code_file	EL30042_2018_A_06_TeckLoggingCodesLookup.zip
H0308	File Verification List	EL30042_2018_A_07_FileListing.txt
H0310	Water_data_file	NA
H0313	Alteration_data_file	EL30042_2018_A_08_AlterationLogs.txt
H0314	Magsusc_data_file	EL30042_2018_A_09_MagSusData.txt
H0315	Vein_data_file	NA
H0316	Recovery_data_file	EL30042_2018_A_10_RecoveryData.txt
H0317	Weathering_data_file	NA
H0318	DHQAQC_data_file	EL30042_2018_A_11_DownholeQAQCChemistry.txt
H0319	Surface_QAQC_Data_file	NA
H0320	Stratigraphy_data_file	EL30042_2018_A_12_StratigraphyLogs.txt
H0321	Structure_Interval_data_file	EL30042_2018_A_13_StructureIntervalLogs.txt
H0322	Structure_Point_data_file	EL30042_2018_A_14_StructurePointLogs.txt
H0323	Mineralisation_data_file	EL30042_2018_A_15_MineralisationLogs.txt
H0324	GeotechDetails_data_file	EL30042_2018_A_16_GeotechDetailsLogs.txt
H0325	SG_data_file	EL30042_2018_A_17_SGData.txt
H0326	RQD_data_file	EL30042_2018_A_18_RQD.txt
H0327	Gamma_data_file	EL30042_2018_A_19_GammaData.txt
H0400	Drill Code	DDH
H0401	Drill_contractor	Titeline Drilling Pty Ltd	 Diverse Resources Group Pty Ltd
H0402	Drill_description	Diamond Drilling	 Water Bore Rotary Air
H0500	Feature_located	Drillhole Collar
H0501	Geodetic_datum	WGS 84
H0502	Vertical_datum	Nominal
H0503	Projection	NA
H0530	Coordinate_system	GEOGRAPHIC
H0531	Projection_zone	NA
H0532	Surface_Location_Survey_Instrument	NA
H0533	Surface_Location_Survey_Company	NA
H0900	Remarks	NA
H1000	Hole_id	Depth From	Depth To	Projectcode	PRIORITY	ALT_COMMENT	ALT_INT	ALT_STY	ALT_TYP	ALT_GSIZES	ALT_MIN1	ALT_LoggedBy
H1001		metres	metres									
H1004		0.001	0.001		0.00000001							
D	TNDD023	0	3.13	REW	1	Strong surface weathering of the top of hole. Generally "clay" with 13cm section of pervasively weathered compentent core.	atl	prvs			hem	N.McMillan
D	TNDD023	3.13	12.78	REW	1	Predominantly compentent drill core with tan/yellow discolouration (weathering) and minor intervals of significantly/pervasively weathered clay intervals.	aex	ptch			hem	N.McMillan
D	TNDD024a	0	66.5	REW	1	Strongly weathered/bleached rock. Little competent rock. Very few or no primary textures present.	atl	prvs			hem	N.McMillan
D	TNDD024a	66.5	109	REW	1	Strongly weathered broken/rubbly core and clay. Competent core increases and mre primary textures are noticeable.	atl	prvs			hem	N.McMillan
D	TNDD024a	109	139	REW	1	Weathering generally confined to fracture surfaces and some core discolouration.	aex	frac			hem	N.McMillan
D	TNDD025	0	13.7	REW	1	Strong surface wethering. Core pervasively leached and oxidised. Cavites developed throughout interval; some competent pieces of carbonate core	ain	prvs			goe,hem	D.Sully
D	TNDD025	13.7	16.96	REW	1	Pervasivly weathered rock. Small interval of clay rch material around 15.3m but predominantly saprock	ain	prvs			goe,hem	D.Sully
D	TNDD025	17.98	20.61	REW	1	Saprock; intensity of weathering decreases down interval. Several small zones of clay rich material. Iron staining common on weathered surfaces.	aex	prvs			goe,hem	D.Sully
D	TNDD025	70.05	71.3	REW	1	Oxidation of wallrock associated with an interpreted cavity. Clay and iron oxides on fracture surfaces	aex	prvs			goe,hem	D.Sully
D	TNDD025	85.64	86.74	REW	1	Patchy oxidation of wallrock associated with an interpreted cavity. Clay and iron oxides on fracture surfaces.	aex	ptch			goe,hem	D.Sully
D	TNDD025	97.8	98.19	REW	1	Oxidation of wallrock associated with an interpreted cavity. Clay and iron oxides on fracture surfaces	aex	ptch			goe,hem	D.Sully
D	TNDD025	762.42	769	REW	1	Variable pink (hem) dol alteration.	asl	prfr			hem	N.McMillan
D	TNDD025	769	780.84	REW	1	V thin lam pink  - dk pink silts adnd pale pink hem dol nod alteration. Pink discolouration decreases downhole.	amd	prfr			hem	N.McMillan
D	TNDD025	780.84	792.68	REW	1	Very pale pink crystalline dol.	aex	diff			hem	N.McMillan
D	TNDD025	798.7	814.2	REW	1	Lt pink - pink hem alt - variale replacement.	aex	ptch			hem	N.McMillan
D	TNDD025	814.2	824.85	REW	1	Pervasive pink - dk pink hem alt.	ain	prvs			hem	N.McMillan
D	TNDD025	824.85	829	REW	1	Minor intervals of very pale pink hematite alteration.	asl	ptch			hem	N.McMillan
D	TNDD026	0	6.1	REW	1	Significantly weathered interval at top of hole.	atl	prvs			hem	N.McMillan
D	TNDD026	6.1	19.55	REW	1	Some intervals of broken core. Weathering on fracture surfaces and patchy weathering.	aex	ptch			hem	N.McMillan
D	TNDD026	863.7	868.3	REW	1	Fault related hydrothermal dolomite. Intensity increases towards fault	amd	prvs			dol	M.Cawood
D	TNDD027	0	0.7	REW	1	Extremely weathered zone. Mainly lateritic clays	atl	prvs			hem	Contractor
D	TNDD027	0.7	2	REW	1	Highly weathered dololutite.	ain	prvs			hem	Contractor
D	TNDD027	2	10.5	REW	1	Moderately weathered dololutite. Highly weathered along fracture surfaces and in broken grounds.	ain	prvs			hem	Contractor
D	TNDD027	10.5	22.46	REW	1	Strongly - mod weathered.	ain	prvs			hem	Contractor
D	TNDD027	70.1	79.6	REW	1	Fractured/broken surfaces are highly weathered and surfaces have oxide staining. High clay content in the broken zone.	ain	prvs			hem	Contractor
D	TNDD027	79.6	93	REW	1	Minor weathering on fractured dol surfaces and some patchy alteration	asl	frac			hem	Contractor
D	TNDD027	728.24	735.52	REW	1	Pink dol alteration	asl	prfr			hem	Contractor
D	TNDD027	735.52	790.5	REW	1	Variable hem (pink) stained dol.	asl	diff			hem	Contractor
D	TNDD028	1.4	29.19	REW	1	Some pink/brown alteration/weathering within the unit.	amd	ptch			hem	N.McMillan
D	TNDD028	813.59	818.9	REW	1	Dol nods are stained a pale pink (hem)	asl	prfr			hem	N.McMillan
D	TNDD028	835.62	861.09	REW	1	Pink bedding parallel dol nods	asl	prfr			hem	N.McMillan
D	TNDD028	865.87	869.42	REW	1	Dol nods stained light pink (hem)	asl	prfr			hem	N.McMillan
D	TNDD028	871.73	873.64	REW	1	Pale pink dol nods (hem)	amd	prfr			hem	N.McMillan
D	TNDD028	874.97	882.55	REW	1	Pink dol nods (hem)	amd	prfr			hem	N.McMillan
D	TNDD028	1017.44	1029.34	REW	1	MFU - sections with pink hem alt.	asl	prfr			hem	N.McMillan
D	TNDD028	1057.14	1089.7	REW	1	MFU - variable sections discoloured with pink hem alt.	asl	prfr			hem	N.McMillan
D	TNDD028	1105.75	1135.48	REW	1	Rare pink to crayon red hem alt.	atr	prfr			hem	N.McMillan
EOF
