**Photos of Damaged Culvert & Bypass Track about 220m North of Mount Wells**

Washed out culvert at: -130 30’ 9.39” S / 1310 43’ 12.31” E



Mount Wells Road: official NT road ends just south of the washed-out culvert. Plan showing the partial straightening of the road, and cut back of banks to reduce the slopes entering and exiting the crossing.



View looking northerly along the culvert embankment, and showing the washed-out area where the culvert used to be. Plan is to push back the fill on the west side to partly straighten the road. But to leave open the creek so it drains.



View looking southerly along the bypass track, showing the planned push back of fill material and the cut back of the steep banks to reduce slopes, so large trucks and vehicles with caravans can cross the creek. The photograph does not accurately show the steepness of the slopes.