H0002	Version	4	
H0003	Date_generated	18-Dec-19	
H0004	Reporting_period_end_date	29-Nov-19	
H0005	State	NT	
H0100	Tenement_no or Combined_rept_no	[GR166]	
H0101	Tenement_holder	PRX	
H0102	Project_name	HYPERION	SUPPLEJACK
H0106	Tenement_operator	Prodigy Gold NL	
H0150	250K_map_sheet_number	SE5215_TANAMI																								
H0151	100K_map_sheet_number	4958_BUCK	
H0200	Start_date_of_data_acquisition	30-Nov-18	
H0201	End_date_of_data_acquisition	29-Nov-19	
H0202	Data_format	DL4	
H0203	Number_of_data_records	8	
H0204	Date_of_metadata_update	18-Dec-19	
H0301	Location_data_file	GR166_2019_GA_01_DHCollars.txt	
H0334	RegOverprint_Code(LIB)	GR166_2019_GA_27_LIBWeathering.txt	
H0900	Comments	N/A	
H1000	Code	Description	
D	CS	Silcrete	
D	CW	"Completely Weathered Rock exhibits soil-like properties (ie can be remoulded), some rock fragments may remain"	
D	EW	Extremelly Weathered	
D	FR	Fresh Rock No visible sign of rock material weathering	
D	HW	Highly Weathered >50% of the rock material is decomposed and/or disintegrated to soil. Fresh or discoloured rock is present as a discontinuos framework or as corestones.	
D	MW	Moderately Weathered <50% of the rock material is decomposed and/or disintegrated to soil. Fresh or discoloured rock is present either as a discontinuous framework or as corestones.	
D	PW	Partially Weathered	
D	SW	Slightly Weathered Discoloration indicates weathering of rock material on discontinuity surfaces. <5% of rock mass altered.	
EOF			
