Gulf Mines Ltd - Wollogorang Project																										Drill Hole #:									WGD08015																		
Prospect:				Nabunga P7						Drilling Type:					diamond																																	page ___ of ___		1			
																																																					
Location																														Surveys																							
UTM-E:			804891						Azimuth:			84						Drill Start Date:					03-Sep-08							Depth		Az		Dip		Type		Depth		Az		Dip		Type		Depth		Az		Dip		Type	
UTM-N:			8081143						Az. type:			mag						Finish Date:				05-Sep-08								85		84		60		mag																	
Elev.:			91						Dip:		-60							Logged By:				G Luketina								100.5		84		60		mag																	
Datum:									Casing Depth:					17.6				Logged On:				5-7 Sep 08																															
Grid E:									RC Depth:																																												
Grid N:									Total Depth:				100.5																																								
									Core Size:				"HQ, NQ"																																								
																																																					
																																																					
Meterage																																										Mineralisation %											
From			To			Rock Type				Formation					Rock Description																											Typ		%	Typ		%	Typ		%	Typ		%
0			1			"soil, wthd mat"									"highly weathered, red, sandy, surface gravels."																																						
1			5			"wthd snd, congl"									"highly weathered, broken core. Poorly consolidated red sstn (qtz fspar mica clay), conglom - med sand matrix, sstn clasts <3 cm, lots of white clay"																																						
																																																					
5			6			clay									white-grey laminated clay																																						
6			6.9			shale				Aquarium					vfgrd brown laminated shale																																						
6.9			7.2			shale				Aquarium					"vfgrd green, grey, red, brown laminated shale, "																																						
7.2			7.7			shale				Aquarium					broken red shale																																						
7.7			8.6			shale				Aquarium					"brown shale, occasional fgrd sstn layer"																																						
8.6			9.3			shale				Aquarium					"grey shale, some beds of fgrd red sstn"																																						
9.3			10.5			sstn				Aquarium					fgrd bedded red sstn. Qtz fspar mica. Mica aligned on bedding planes. Shaley layers																																						
										Aquarium																																											
10.5			11.3			"shale, sstn"				Aquarium					"grey shale-sstn - graded bedding - fgrd sand at base, (11.3) to shale at top (10.5)"																																						
10.8										Aquarium					orange sandy lenses																																						
11.3			12.9			sstn				Aquarium					"red, green & grey sstn. Bedded. Glauconite. A few beds of red/grey shale"																																						
12.2										Aquarium					"specs chpy, py on bedding plane"																											chpy 		<1	py		<1						
12.9			18.4			"sstn, shale"				Aquarium					"grey fgrd sstn, shale."																											chpy 		<1	py		<1						
17.6			17.9			sstn				Aquarium					hard white v qtz rich sstn. Broken																																						
18.05			18.15							Aquarium					grey clay																																						
18.4			21			"sstn, shale"				Aquarium					alternating layers grey fgrd sstn & green shale. High % sstn layers																																						
21			23.5			"shale, sstn"				Aquarium					alternating layers grey fgrd sstn & red & grey shale. High % shale layers																											py		<1									
23.5			33.2			"sstn, shale"				Aquarium					"alternating layers grey fgrd sstn & red & grey shale. High % sstn layers. From 24.7 m, sstn mgrd, lots of mica esp on bedding planes. Sstn layers have graded bedding - crs at base, fine at top."																																						
										Aquarium																																											
										Aquarium																																											
25.6										Aquarium					"cgrd sstn, large glauc & qtz grains, porous"																																						
33.2			41			"shale, sstn"				Aquarium					"alternating beds of green-grey mgrd bedded sstn (lots of glauc, mica), red shale & green shale. High % shale"																																						
										Aquarium																																											
38.5										Aquarium					cross bedding. Sstn v green (lots of glauc)																																						
39.1			39.6							Aquarium					sstn crgrd & porous																																						
																																																					
