Gulf Mines Ltd - Wollogorang Project																										Drill Hole #:									WGD08012																		
Prospect:				Nabunga (P5)						Drilling Type:					"Diamond (HQ, NQ)"																																	page ___ of ___		1			
																																																					
Location																														Surveys																							
UTM-E:			813897						Azimuth:			154-137						Drill Start Date:					23-Aug-08							Depth		Az		Dip		Type		Depth		Az		Dip		Type		Depth		Az		Dip		Type	
UTM-N:			8079999						Az. type:			mag						Finish Date:				26-Aug-08								51.4		154		89																			
Elev.:			89						Dip:		89							Logged By:				G Luketina								100		137		89																			
Datum:			GDA94						Casing Depth:					27				Logged On:				28-29 Aug 08																															
Grid E:									RC Depth:																																												
Grid N:									Total Depth:				100																																								
									Core Size:				"HQ, NQ"																																								
																																																					
																																																					
Meterage																																										Mineralisation %											
From			To			Rock Type				Formation					Rock Description																											Typ		%	Typ		%	Typ		%	Typ		%
0			2			"soil, weath seds"									"soil (10 cm), highly weathered seds, crushed, crumbly, clayey"																																						
2			3.6			"shale, sstn"				Aquarium Fm					weathered & broken shale & sstn																																						
3.6			4.9			"shale, sstn"				Aquarium Fm					"brown shale, laminated, vfgrd, micaceous, hematitic, up to 5 cm thick layers of bedded white fgrd sstn."																																						
										Aquarium Fm																																											
4.9			4.94			clay				Aquarium Fm					"laminated green, brown clay, weathered"																																						
4.94			8.9			shale				Aquarium Fm					"alternating layers of reddy brown hematitic micaceous shale, and green glauconitic shale. Vfgrd, laminated. Higher percentage of red-brown layers."																																						
										Aquarium Fm																																											
5.6			5.7			sstn				Aquarium Fm					"mgrd sandy layer, poorly consolidated, rounded grains qtz fspar glauconite"																																						
8.9			13			"shale, sstn"				Aquarium Fm					"alternating layers of sstn, red-brown hematitic shale & green glauconitic shale. Sstn layers f-mgrd qtz fspar glauc, some graded bedding crs at base, finer grd towards top of layers. The occasional 1 cm kaolinite layer"																																						
										Aquarium Fm																																											
										Aquarium Fm																																											
13			15.7			"shale, sstn"				Aquarium Fm					"same alternating red & green shales & sstn, but sstn layers becoming more frequent & larger (up to 30 cm)."																																						
										Aquarium Fm																																											
13.6										Aquarium Fm					<1 mm thick calcite vein within sstn layer. 																																						
15.7			16.6			"shale, sstn"				Aquarium Fm					"higher percentage of shale beds, bedding steepening slightly. Some shale layers undulating a little"																																						
										Aquarium Fm																																											
16.6			26.8			"shale, sstn"				Aquarium Fm					"sstn layers more frequent again, bedding steepening to 75 deg at 18 m. Large clasts of green shale in sstn, green shale in frac in sstn. "																																						
										Aquarium Fm																																											
19.8										Aquarium Fm					microcalcite vein within sstn layer. 																																						
21.1										Aquarium Fm					bedding slightly disturbed																																						
21.2										Aquarium Fm					layer of pyrite on bedding plane																											py		1									
21.8										Aquarium Fm					microcalcite vein within sstn layer. 																																						
22.3			22.6							Aquarium Fm					"frac zone, clay on frac walls, within red & green shale layers. Py coating frac"																											py		1									
23			24							Aquarium Fm					very few sstn layers - all red & green shale																																						
25.05										Aquarium Fm					cross bedding in sstn																																						
26.8			26.9			sstn (brecc)				Aquarium Fm					brecciated zone - angular clasts of red & green shale within cgrd sstn matrix																																						
26.9			36.5			"shale, sstn"				Aquarium Fm					alt layers fgrd red & green shale & cgrd sstn (coarser than above). Sstn layers have graded bedding - crs at base to fine at top																																						
										Aquarium Fm																																											
32.7										Aquarium Fm					undulating bedding in shale																																						
