				LEGEND			v 3.0			(Rock Codes)	
											
	Col 1	Col 2	Col 3	Description							
	M	B	P	Pillow Basalt				Stratigraphic Codes    (STRAT)			
	(Mafic)	(Basalt)	X	Autoclastic Basalt					QOO	Transported Alluvial Cover	
		A	V	Vesicular Basalt					CLA	Antrim Plataeu Volcanics	
		(Andesite)	C	Coarse Grained Massive 					KLO	Larranganni Beds	
		G	M	Amygdaloidal					PDK	Coomarie Sandstone	
		(Gabbro)	F	Fine Grained Massive					PDT	Talbot Wells Formation	
		D	T	Porphyritic					PDG	Gardiner Sandstone	
		(Diorite)	A	Aphanitic 					PLS	Supplejack Downs Sandstone	
		U	Y	Pyritic					PLW	Mt Winnecke Formation	
		(Ultramafic)	D	Medium Grained (Doleritic)					PFU	Felsic Rocks - Undifferentiated	
			K	Poikiloblastic					PLG	Pargee Sandstone	
			B	Porphyroblastic					PTH	Mt Charles Beds - Hangingwall Seq.	
			E	Equigranular					PTM	Mt Charles Beds - Mine Sequence	
									PTF	Mt Charles Beds - Footwall Seq			
	F	R	F	Flow Banded					PTC	Mt Charles Beds - Undifferentiated			
		(Rhyolites)	M	Massive					PTK	Killi Killi Beds			
	(Felsic)	D	G	Fragmental					PTW	Nanny Goat Creek Beds			
		(Dacite)	P	Porphyritic 					PTN	Nongra Creek Beds			
		A	D	Medium grained					PGG	Granites Complex - Undifferentiated			
		(Aplite)	V	Vesicular					PGC	Coomarie Dome			
		G	C	Coarse Grained					PGF	Frankenia Dome			
		(Granitoid)	L	Foliated					PGW	Mt Winnecke Granite			
		N	E	Equigranular					PGU	Granite Undifferentiated			
		(Granodiorite)	N	Fine grained									
		T											
		(Granite)						Abbreviated MM Codes in File Structure					
													
									Prospect		Drilling Area		
	S	C	P	Polymictic Conglomerate					Hole_nm		Hole Name		
	(Sedi-	(Conglomerate)	M	Monomictic Conglomerate					Geo		Geologist
	  mentary)	X	P	Polymictic Breccia					Smpl_No		Sample Number
		(Breccia)	M	Monomictic Breccia					From		From Metre
									To		To Metre
		S	F	Feldspathic					Rec		Recovery %
		(Sandstones)	Q	Quartzose					Hrd		Hardness
		L	H	Haematitic					Colour		Colour
		(Siltstones)	L	Lithic					Strat		Stratigraphic Name
		M	M	Micaceous					Reg		Regolith
		(Mudstones)	B	Carbonaceous					Rck		Rock Code
		U	O	Undifferentiated					Rck_Ql		Rock Qualifier
		(Sand-siltstone)	Y	Pyritic					Alt		Alteration
		V	P	Pale					Int		Alteration Intensity
		(Sand-mudstone)	T	Chert					Vn		Vein Code
		W	I	Hematitic-Feldspathic					Vn%		Vein %
		(Silt-Mudstone)	R	Quartz-Micaceous					Str		Structure
		B	D	Chert-Carbonaceous					Wtr		Water							
		(Carbonate)	E	Quartz-Hematitic					Mag_Sus		Magnetic Suseptibility (x10^-5)							
			J	Feldspathic-Micaceous														
			N	Hematitic-Micaceous				The Four Commandments										
			S	Quartz - Feldspathic														
			G	Lithic-Feldspathic (greywacke)				Thou shalt use the letter O as a filler when										
			C	Calcareous					only one or two characters are used in a 									
			V	Volcanic					three character code field.									
								Thou MUST have three characters within										
	Z	P	A	Amphibole					"Rock Codes, Alteration, Veining, Stucture"									
	(Meta-	(Phyllite)	T	Carbonate					and Regolith when data needs to be entered.									
	 morphics)	Z	C	Chlorite				Thou shalt not use any code that is not listed.										
		(Schist)	E	Epidote				Thou shalt discuss new coding requirements at 										
		G	G	Garnet					the monthly assembly.									
		(Gneiss)	N	Andalusite							                          JC.							
		A	M	Muscovite														
		(Amphibolite)	Q	Quartz		
		H	R	Graphite		
		(Hornfels)	B	Biotite		

LEGEND  				v. 3.0			(Descriptions)				Col 1			Col 2				Col 3												
	Colour			(COLOUR)							Regolith			(REG)																	
																															
		L		Light		D			Dark			R			T	Transported			C	Calcrete											
		BK		Black		MU			Mustard			(Regolith)			L	Laterite			D	Sand Dominant											
		BL		Blue		OR			Orange						M	Upper Saprolite			F	Ferricrete											
		BR		Brown		PI			Pink						S	Lower Saprolite			G	"Sands, Pisolites, Lithics"											
		CR		Cream		PU			Purple						C	Saprolite (Undifferentiated)			H	Silcrete											
		GR		Green		RE			Red						W	Weathered Bedrock			I	Lithic Fragments											
		GY		Grey		WH			White						B	Transitional Bedrock			L	Laterite Component											
		KH		Khaki		YE			Yellow						F	Fresh Bedrock			M	Mottled Clays											
		MA		Maroon															P	Pisolith Dominant											
																			Q	Pervassive Silica											
	Fabric and Structure																		S 	Saprolite Clay											
	Sedimentary						(RCK_QL)																								
		FS	Flame Structure																												
		BD	Bedding								Alteration				(ALT)																
		GB	Graded Bedding									A			C	Carbonate			D	Disseminated											
		LC	Load Clasts									(Alteration)				(cb+qz+py) (acid fizz)			F	Fracture 											
		PA	Parallel Laminations												G	Green Chloritisation			P	Pervasive											
		CR	Cross Bedding													(ch+cb+py+qz) (gr clays)			S	Selvedge											
		MS	Matrix Supported												B	Bleaching/Paling			O	Unknown											
		CS	Clast Supported													(illite/sericite+silica+py) (wh clays)															
		PO	Poorly Sorted												E	Sericite + Pyrite															
		MO	Moderately Sorted												S	Silicification															
		WE	Well Sorted													(qz+clay+py) (wh pervassive qz)															
		MA	Massive												F	Feruginous Silicification															
		AN	Angular Clasts													(FeO+qz+clay) (Red/Yellow/Brown)															
		SA	Sub-Angular Clasts																												
		SR	Sub-Rounded Clasts								Veining			(VN)																	
		RO	Rounded Clasts									V			C	Carbonate			B	Banded											
	Metamorphic											(Veining)				(Cb+Qz+Py+Ch)			C	Breccia											
		SP	Spotted												F	Ferruginous Carbonate			K	Crackly
		PK	Poikiloblastic													(Cb+Hm)			M	Milky
		PP	Porphyroblastic												H	Ferruginous Quartz			S	Stockwork
		EQ	Equigranular													(Hm+Qz+FeO)			T	Translucent
															Q	Quartz			X	Crystalline
	Minerals List					(RCK_QL)										(Qz+Cb+Py+Se+Ch)				
	Rock Forming														R	Chlorite				
		AD		Andalusite		SE		Sericite												
		AK		Ankerite		SI		Silica			Structure				(STR)					
		AM		Amphibole		TO		Tourmaline				T			U 	Unqualified			A	Alteration Front
		BT		Biotite								(Structure)							B	Boundary
		CB		Carbonate	Sulphides														C	Geological Contact
		CH		Chlorite		AS		Arsenopyrite											D	Bedding
		CL		Clay		CP		Chalcopyrite											P	Point
		EP		Epidote		PY		Pyrite												
		GT		Garnet		SU		Sulphides							S	Foliation			A	Axial
		KA		Kaolinite																		
		KS		K-Spar	Oxides										L	Linear Feature			M	Mineral Lineations		
		LX		Leucoxene		GO		Goethite											S	Strain/Rodding Lintn		
		MI		White Mica		HM		Haematite											H	Fold Hinge Lineation		
		NO		Nontronite		LM		Limonite														
		PL		Plagioclase		MH		Maghaemite							D	Folds			S	Slump Folds		
		PX		Pyroxene		MN		Manganese											D	Drag Folds		
		QZ		Quartz	 																	
															J	Joints			T	Stepped		
	Hardness				(HRD)										R	Fracture			H	Hackly		
																			P	Planar		
		1		Soft															S	Smooth		
		2		"Firm, broken by hand"															C	Clay filled 		
		3		Hard and Competent															D	Dilational		
		4		Rings and breaks																		
		5		Rings and breaks not											F	Faults			B	Brecciated		
																(Brittle)			G	Gauge
	Alteration Intensity					Water			(WTR)											
			(INT)				D	Dry Sample							K	Slickenlines			F	Frictional
		W		Weak			M	Moist Sample											B 	Fibrous
		M		Moderate			W	Wet Sample											T	Tensile Failure
		S		Strong			T	Water Table											D	Ductile
		I		Intense																
															Z	Shear Zone			M	Mylonite Fabric
	Sampling Number															(Ductile)			S	S-C Fabrics
		1		Transported																
		2		Unconformity											C	Cleavage			B	Bedding plane
		3		BOH - Residual															A	Axial Plane
		4		Saprolite Redox															P	Pencil
		5		Veining/Alteration																
		6		Calcrete/Silcrete																