

**Survey Report**

**Drill Hole Survey – Meta data**

**CLIENT:** Jinka Minerals

**JOB NUMBER: ASV11-0318**

**SURVEY COMMENCED:** 14 November 2011

**SURVEY COMPLETED:** 16November 2011

**SURVEYOR:** Luke Lorback

**Datum**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **STATION** | **MGA EAST** | **MGA NORTH** | **RL (AHD)** | **DESCRIPTION** |
| ASV01 | 629865.574 | 7492924.268 | 350.941 | Metal Spike |
| ASV02 | 630459.344 | 7495139.274 | 353.205 | Star Picket |
| ASV03 | 627197.121 | 7491949.100 | 367.402 | Star Picket |

All survey was conducted on MGA94 datum. Auspos Occupation of control ASV01, with GeoScience Australia post processing to establish corrected MGA94 datum and corrected AHD heights.

**Survey methodology**

All data was recorded by RTK GPS method.

**Survey**

All drill hole located were picked up at natural service level on the backside of collar. The holes drilled by Jinka mineral are recorded with the correct identifiers; the old collars located without a number are not numbered.

**Plans**

None

**Drill Hole Datum**

Magnetic (\_M) Azi

**Spatial Accuracy**

+/- 0.5m

Luke Lorback

Surveyor Ausurv Pty Ltd.

19/11/2011