H0002	Version	4
H0003	Date_generated	1-May-2018
H0004	Reporting_period_end_date	23-Mar-2018
H0005	State	Northern Territory
H0100	Tenement_no/Combined_report_no	EL30042
H0101	Tenement_holder	Teck Australia
H0102	Project_name	Reward
H0106	Tenement_operator	Teck Australia
H0150	250K_map_sheet_number	SE5303
H0151	100K_map_sheet_number	Borrowloola 6165 & Batten 6064
H0152	50K_map_sheet_number	NA
H0153	25K_map_sheet_number	NA
H0200	Start_date_of_data_acquisition	24-Mar-2017
H0201	End_date_of_data_acquisition	23-Mar-2018
H0202	Data_format	SL4
H0203	Number_of_data_records	8
H0204	Date_of_metadata_update	1-May-2018
H0301	Location_data_file	EL30042_2018_A_02_CollarsDrillhole.txt
H0302	Lithology_data_file	EL30042_2018_A_03_LithologyLogs.txt
H0303	Assay_data_file	EL30042_2018_A_04_DownholeAssays.txt
H0304	Survey_data_file	EL30042_2018_A_05_DownholeSurvey.txt
H0307	Lithology_code_file	EL30042_2018_A_06_TeckLoggingCodesLookup.zip
H0308	File Verification List	EL30042_2018_A_07_FileListing.txt
H0310	Water_data_file	NA
H0313	Alteration_data_file	EL30042_2018_A_08_AlterationLogs.txt
H0314	Magsusc_data_file	EL30042_2018_A_09_MagSusData.txt
H0315	Vein_data_file	NA
H0316	Recovery_data_file	EL30042_2018_A_10_RecoveryData.txt
H0317	Weathering_data_file	NA
H0318	DHQAQC_data_file	EL30042_2018_A_11_DownholeQAQCChemistry.txt
H0319	Surface_QAQC_Data_file	NA
H0320	Stratigraphy_data_file	EL30042_2018_A_12_StratigraphyLogs.txt
H0321	Structure_Interval_data_file	EL30042_2018_A_13_StructureIntervalLogs.txt
H0322	Structure_Point_data_file	EL30042_2018_A_14_StructurePointLogs.txt
H0323	Mineralisation_data_file	EL30042_2018_A_15_MineralisationLogs.txt
H0324	GeotechDetails_data_file	EL30042_2018_A_16_GeotechDetailsLogs.txt
H0325	SG_data_file	EL30042_2018_A_17_SGData.txt
H0326	RQD_data_file	EL30042_2018_A_18_RQD.txt
H0327	Gamma_data_file	EL30042_2018_A_19_GammaData.txt
H0400	Drill Code	DDH
H0401	Drill_contractor	Titeline Drilling Pty Ltd	 Diverse Resources Group Pty Ltd
H0402	Drill_description	Diamond Drilling	 Water Bore Rotary Air
H0500	Feature_located	Drillhole Collar
H0501	Geodetic_datum	WGS 84
H0502	Vertical_datum	Nominal
H0503	Projection	NA
H0530	Coordinate_system	GEOGRAPHIC
H0531	Projection_zone	NA
H0532	Surface_Location_Survey_Instrument	NA
H0533	Surface_Location_Survey_Company	NA
H0900	Remarks	NA
H1000	Hole_ID	Longitude	Lattitude	Elevation	Pre_Collar_Depth	Total Hole Depth	Drill Code	Dip	Azimuth_TRUE	Comments	Projectcode	GRIDNAME_DT_SRC	EAST_DT_SRC	NORTH_DT_SRC	RL_DT_SRC	PROSPECT	TENEMENTID	SITEID	SITEPREP_DATE	SITESIZE_HA	COMPANY	CONTRACTOR	DateCollarLoaded	STARTDATE	ENDDATE	RIG_NUMBER	RIG_TYPE	GRIDNAME	REF_SurveyMethod	HOLE_STATUS	HOLE_TYPE	WaterDepth	COMMENTS_COLL	REHAB_CODE	REHAB_DATE	REHAB_STATUS	SUMPDUG	SEDRECUNIT	COMMENTS_REHAB	DRILLTYPE1	DRILLTYPE1_DEPTH	DRILLTYPE2	DRILLTYPE2_DEPTH	PRECOLLAR_DEPTH	TYPE_PRECOLLAR	REG_EAST	REG_NORTH	REG_RL	REG_GRID_ID	SOURCE_FILE_COLL	PLANNED_AZ	PLANNED_DIP	PLANNED_DEPTH	TARGET_DEPTH	TARGET_EAST	TARGET_NORTH	TARGET_RL	WGS84_LL_cal_X	WGS84_LL_cal_Y	WGS84_LL_cal_Z
H1001		metres	metres	metres	metres	metres		degrees	degrees																																																			
H1004													0.00000001	0.00000001	0.00000001					0.00000001												0.00000001												0.00000001		0.00000001	0.00000001	0.00000001			0.00000001	0.00000001	0.00000001	0.00000001	0.00000001	0.00000001	0.00000001	0.00000001	0.00000001	0.00000001
D	TNDD023	136.01657865	-16.43977206	60		1321.1		-55.37	0.87		REW	MGA94_53	608529.0744	8182145.989	60	TEENA	EL30042	PAD_2017_B	11-May-2017	0.09	TA	TITELINE	7-Jun-2017	27-May-2017	23-Jun-2017	07	UDR1200	WGS84_LL	GPS	COMPLETED	DDH		PROP_2017_2 updated to TNDD023		10-Nov-2017	COMPLETE	Yes	No		HQ	0	NQ2	593.7			608529.0744	8182145.989	60	MGA94_53	2017_REW_TeckAusProposedDillholes.v5editedxlsx	0	-54.5	1350	1120	608592	8182747	-880	136.01657865	-16.43977206	60
D	TNDD024	136.01340505	-16.43116426	69.64		41.7		-62	177		REW	MGA94_53	608195	8183100	69.64	TEENA	EL30042	PAD_2017_C	11-May-2017	0.112	TA	TITELINE	7-Jun-2017	28-Jun-2017	28-Jun-2017	07	UDR1200	WGS84_LL	GPS	ABANDONED	DDH		PROP_2017_3 updated to TNDD024; abandonded hole; lost water at 40.7m snapped off 3m HQ and complete barrel EOH @ 41.7m		10-Nov-2017	COMPLETE	Yes	No		HQ	0	NQ2	41.7			608195	8183100	69.64	MGA94_53	2017_REW_TeckAusProposedDillholes.v5editedxlsx	177	-62	1250	943	608195	8182700	-787	136.01340505	-16.43116426	69.64
D	TNDD024a	136.01340486	-16.43112811	69.64		228.7		-62	180		REW	MGA94_53	608195	8183104	69.64	TEENA	EL30042	PAD_2017_C	11-May-2017	0	TA	TITELINE	7-Jun-2017	28-Jun-2017	3-Jul-2017	07	UDR1200	WGS84_LL	GPS	ABANDONED	DDH		PROP_2017_3 moved rig 4m forward (north) TNDD024a; abandoned hole due to bad ground conditions and cavities; rods parted breaking core; parted in cavity; an attempt to retrieve rods was made however drillers were unable to pass 97m		10-Nov-2017	COMPLETE	Yes	No		HQ	0	NQ2	228.7			608195	8183104	69.64	MGA94_53	2017_REW_TeckAusProposedDillholes.v5editedxlsx	177	-62	1250	943	608195	8182700	-787	136.01340486	-16.43112811	69.64
D	TNDD025	136.00778246	-16.43962459	72		882.9		-60.81	355.42		REW	MGA94_53	607590	8182167	72	TEENA	EL30042	PAD_2017_A	11-May-2017	0.1	TA	TITELINE	7-Jun-2017	4-Jul-2017	17-Jul-2017	07	UDR1200	WGS84_LL	GPS	COMPLETED	DDH		PROP_2017_1 updated to TNDD025; EOH depth 882.9m		10-Nov-2017	COMPLETE	Yes	Yes	Small pit/sump dug for SRU cuttings. Track not ripped, dozer not equipped with rippers	HQ	0	NQ2	311.4			607590	8182167	72	MGA94_53	2017_REW_TeckAusProposedDillholes.v5editedxlsx	358	-61	1100	790	607600	8182500	-635	136.00778246	-16.43962459	72
D	TNDD026	136.01387198	-16.43992969	72		1102.12		-54.07	348.88		REW	MGA94_53	608240	8182130	72	TEENA	EL30042	PAD_2017_G	11-May-2017	0.1	TA	TITELINE	12-Jul-2017	18-Jul-2017	12-Aug-2017	07	UDR1200	WGS84_LL	GPS	COMPLETED	DDH		PROP_2017_8 updated to TNDD026; EOH depth 1102.12m		10-Nov-2017	COMPLETE	Yes	Yes	Small pit/sump dug for SRU cuttings	HQ	0	NQ2	318.4			608240	8182130	72	MGA94_53	2017_REW_TeckAusProposedDillholes v6.xlsx	349	-54	1250	1034	608200	8182727	-767	136.01387198	-16.43992969	72
D	TNDD027	136.00604349	-16.44022951	60.7		896.5		-57	3		REW	MGA94_53	607404	8182101	60.7	TEENA	EL30042	PAD_2017_D	11-May-2017	0.12	TA	TITELINE	7-Jun-2017	1-Sep-2017	18-Sep-2017	07	UDR1200	WGS84_LL	GPS	COMPLETED	DDH		PROP_2017_4 updated to TNDD027		10-Nov-2017	COMPLETE	Yes	No	Sumps still contain water, contractor will return late Nov to complete	HQ	0	NQ2	389.5			607404	8182101	60.7	MGA94_53	2017_REW_TeckAusProposedDillholes.v5editedxlsx	0	-58	1000	714	607400	8182440	-567	136.00604349	-16.44022951	60.7
D	TNDD028	136.00977638	-16.44123296	67.3		1135.5		-72	360		REW	MGA94_53	607802	8181988	67.3	TEENA	EL30042	PAD_2017_E			TA	TITELINE	7-Jun-2017	20-Sep-2017	6-Oct-2017	07	UDR1200	WGS84_LL	GPS	COMPLETED	DDH		PROP_2017_6 updated to TNDD028		10-Nov-2017	COMPLETE	Yes	No	Dumps still contain water, contractor will return late Nov to complete	HQ	0	NQ2	290.7			607802	8181988	67.3	MGA94_53	2017_REW_TeckAusProposedDillholes.v5editedxlsx	0	-72	1100	750	607800	8182184	-657	136.00977638	-16.44123296	67.3
D	WB_REW04	135.99651561	-16.44340244	53.16		42		-90	0		REW	MGA94_53	606385	8181755	53.16	TEENA	EL30042	2			TA	DIVERSE	30-Aug-2017	10-Aug-2017	11-Aug-2017		UNKNOWN	WGS84_LL	GPS	COMPLETED	WB	12.5	Northing coordinate picked up in field does not equal the bore report coordinate;Casing has no end cap; Teck to install pump ASAP; water bearing beds 12.5-21m.			UNKNOWN				PR	0					606385	8181755	53.16	MGA94_53									135.99651561	-16.44340244	53.16
EOF
