H0002	Version	4
H0003	Date_generated	1-May-2018
H0004	Reporting_period_end_date	23-Mar-2018
H0005	State	Northern Territory
H0100	Tenement_no/Combined_report_no	EL30042
H0101	Tenement_holder	Teck Australia
H0102	Project_name	Reward
H0106	Tenement_operator	Teck Australia
H0150	250K_map_sheet_number	SE5303
H0151	100K_map_sheet_number	Borrowloola 6165 & Batten 6064
H0152	50K_map_sheet_number	NA
H0153	25K_map_sheet_number	NA
H0200	Start_date_of_data_acquisition	24-Mar-2017
H0201	End_date_of_data_acquisition	23-Mar-2018
H0202	Data_format	DL4
H0203	Number_of_data_records	673
H0204	Date_of_metadata_update	1-May-2018
H0301	Location_data_file	EL30042_2018_A_02_CollarsDrillhole.txt
H0302	Lithology_data_file	EL30042_2018_A_03_LithologyLogs.txt
H0303	Assay_data_file	EL30042_2018_A_04_DownholeAssays.txt
H0304	Survey_data_file	EL30042_2018_A_05_DownholeSurvey.txt
H0307	Lithology_code_file	EL30042_2018_A_06_TeckLoggingCodesLookup.zip
H0308	File Verification List	EL30042_2018_A_07_FileListing.txt
H0310	Water_data_file	NA
H0313	Alteration_data_file	EL30042_2018_A_08_AlterationLogs.txt
H0314	Magsusc_data_file	EL30042_2018_A_09_MagSusData.txt
H0315	Vein_data_file	NA
H0316	Recovery_data_file	EL30042_2018_A_10_RecoveryData.txt
H0317	Weathering_data_file	NA
H0318	DHQAQC_data_file	EL30042_2018_A_11_DownholeQAQCChemistry.txt
H0319	Surface_QAQC_Data_file	NA
H0320	Stratigraphy_data_file	EL30042_2018_A_12_StratigraphyLogs.txt
H0321	Structure_Interval_data_file	EL30042_2018_A_13_StructureIntervalLogs.txt
H0322	Structure_Point_data_file	EL30042_2018_A_14_StructurePointLogs.txt
H0323	Mineralisation_data_file	EL30042_2018_A_15_MineralisationLogs.txt
H0324	GeotechDetails_data_file	EL30042_2018_A_16_GeotechDetailsLogs.txt
H0325	SG_data_file	EL30042_2018_A_17_SGData.txt
H0326	RQD_data_file	EL30042_2018_A_18_RQD.txt
H0327	Gamma_data_file	EL30042_2018_A_19_GammaData.txt
H0400	Drill Code	DDH
H0401	Drill_contractor	Titeline Drilling Pty Ltd	 Diverse Resources Group Pty Ltd
H0402	Drill_description	Diamond Drilling	 Water Bore Rotary Air
H0500	Feature_located	Drillhole Collar
H0501	Geodetic_datum	WGS 84
H0502	Vertical_datum	Nominal
H0503	Projection	NA
H0530	Coordinate_system	GEOGRAPHIC
H0531	Projection_zone	NA
H0532	Surface_Location_Survey_Instrument	NA
H0533	Surface_Location_Survey_Company	NA
H0900	Remarks	NA
H1000	Hole_id	Depth From	Depth To	Projectcode	PRIORITY	GEOT_DINTERVAL	GEOT_HARDNESS	GEOT_TYPE	GEOT_TYPE2	GEOT_TYPE3	GEOT_FREQUENCY	GEOT_FREQUENCY2	GEOT_FREQUENCY3	GEOT_CAANGLE	GEOT_CAANGLE2	GEOT_CAANGLE3	GEOT_ALPHA	GEOT_ALPHA2	GEOT_ALPHA3	GEOT_BETA	GEOT_BETA2	GEOT_BETA3	GEOT_SHAPE	GEOT_SHAPE2	GEOT_SHAPE3	GEOT_ROUGHNESS	GEOT_ROUGHNESS2	GEOT_ROUGHNESS3	GEOT_CHARACTER	GEOT_CHARACTER2	GEOT_CHARACTER3	GEOT_INFILL	GEOT_INFILL2	GEOT_INFILL3	GEOT_INFILLTHICK	GEOT_INFILLTHICK2	GEOT_INFILLTHICK3	GEOT_LoggedBy	GEOTD_COMMENT
H1001		metres	metres																																				
H1004		0.001	0.001		0.00000001	0.00000001											0.00000001	0.00000001	0.00000001	0.00000001	0.00000001	0.00000001																	
D	TNDD023	3	5.24	REW	1	2.24	2	JN						0-30									Irregular			RO												N.McMillan	Some intervals of very wethered core - not competent and extremely soft rock.
D	TNDD023	5.24	16.95	REW	1	11.71	3	JN						0-30									Irregular			RO												N.McMillan	Some steeper fractures (60 - 90).
D	TNDD023	16.95	17.9	REW	1	0.95	3	JN						30-60									Irregular			VRO												N.McMillan	Some flatter fractures (0 - 30). Rare slickenfibres on fracture surface.
D	TNDD023	17.9	42.82	REW	1	24.92	3	JN						0-30									Irregular			RO												N.McMillan	.
D	TNDD023	42.82	45.82	REW	1	3	4	JN						0-30									Irregular			RO												N.McMillan	.
D	TNDD023	45.82	54.67	REW	1	8.85	3	JN						0-30									Irregular			RO												N.McMillan	Rare 30 - 60 planar smooth-rough bedding fractures.
D	TNDD023	54.67	62.15	REW	1	7.48	3	JN						0-30									Planar			SM												N.McMillan	Combination of bedding 30-60 bedding and 0-30 joint/fractures.
D	TNDD023	62.15	62.3	REW	1	0.15	3	FO						30-60									Planar			K												N.McMillan	Very smooth, likely slickensides.
D	TNDD023	62.3	72.36	REW	1	10.06	3	JN						30-60									Irregular			RO												N.McMillan	Rare stepped fracture shapes
D	TNDD023	72.36	72.45	REW	1	0.09	3	JN						30-60									Irregular			K												N.McMillan	
D	TNDD023	72.45	89.22	REW	1	16.77	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	89.22	91.75	REW	1	2.53	4	FO						30-60									Planar			RO												N.McMillan	Bedding
D	TNDD023	91.75	92.1	REW	1	0.35	3	FO						60-90									Undulating			K												N.McMillan	
D	TNDD023	92.1	96.3	REW	1	4.2	4	JN						0-30									Irregular			RO												N.McMillan	Combination of joint fractures and bedding. Probably a few more joints than bedding breaks.
D	TNDD023	96.3	96.4	REW	1	0.1	3	FO						30-60									Undulating			K												N.McMillan	Bedding
D	TNDD023	96.4	100.2	REW	1	3.8	4	JN						0-30									Irregular			RO												N.McMillan	Some bedding breaks.
D	TNDD023	100.2	111.6	REW	1	11.4	3	FO						30-60									Planar			SM												N.McMillan	
D	TNDD023	111.6	123	REW	1	11.4	3	FO						30-60									Planar			RO												N.McMillan	Joint breaks (predom 0-30) also increase during this section.
D	TNDD023	123	151.7	REW	1	28.7	3	JN						0-30									Irregular			RO												N.McMillan	Some bedding fractures in this zone - appear smooth and (30 - 60)
D	TNDD023	151.7	158.68	REW	1	6.98	2	JN						0-30									Irregular			RO												N.McMillan	Some very smooth (30-60) bedding planes.
D	TNDD023	158.68	170.4	REW	1	11.72	3	FO						30-60									Planar			SM												N.McMillan	Both smooth and rough bedding surfaces.
D	TNDD023	170.4	180.15	REW	1	9.75	3	JN						0-30									Irregular			RO												N.McMillan	Some bedding planes. Joint surfaces seem to break along mud infill stylolites. May also have smooth AND very rough surface.
D	TNDD023	180.15	184	REW	1	3.85	3	FO						30-60									Planar			SM												N.McMillan	
D	TNDD023	184	189	REW	1	5	3	JN						30-60									Irregular			RO												N.McMillan	
D	TNDD023	189	203.5	REW	1	14.5	3	FO						30-60									Planar			SM												N.McMillan	Bedding planes may also be more undulating and steeper (>60). Some faces can be very smooth.
D	TNDD023	203.5	204.6	REW	1	1.1	3	JN						0-30									Irregular			RO												N.McMillan	Also some smooth bedding features.
D	TNDD023	204.6	205.67	REW	1	1.07	3	FO						60-90									Planar			SM												N.McMillan	Bedding planes are both planar and undulating.
D	TNDD023	205.67	207	REW	1	1.33	3	FO						30-60									Planar			SM												N.McMillan	Bedding planes can also be rough. Some joint fracturing.
D	TNDD023	207	212.4	REW	1	5.4	3	JN						30-60									Irregular			RO												N.McMillan	An interpreted fault zone. Surfaces can be stepped and very rough.
D	TNDD023	212.4	215.95	REW	1	3.55	3	FO						30-60									Planar			RO												N.McMillan	
D	TNDD023	215.95	221.2	REW	1	5.25	4	FO						0-30									Planar			RO												N.McMillan	
D	TNDD023	221.2	237	REW	1	15.8	3	FO						60-90									Planar			SM												N.McMillan	Some flatter (0 - 30) joint breaks. Bedding surfaces may be very smooth.
D	TNDD023	237	250.3	REW	1	13.3	3	JN						0-30									Irregular			RO												N.McMillan	Joint breaks may be irregular or less commonly stepped. Rare steeper (30 - 60) smooth bedding breaks.
D	TNDD023	250.3	258.23	REW	1	7.93	3	FO						60-90									Planar			SM												N.McMillan	Some joint breaks - irregular or steppped
D	TNDD023	258.23	271.3	REW	1	13.07	3	FO						30-60									Planar			SM												N.McMillan	Joint breaks inconsistent - flat to more steep (60 - 90). May be planar, irregular or stepped. Generally relatively smooth.
D	TNDD023	271.3	278.78	REW	1	7.48	3	JN						30-60									Planar			RO												N.McMillan	
D	TNDD023	278.78	293.2	REW	1	14.42	2	JN						30-60									Planar			RO												N.McMillan	Some very smooth bedding (60 - 90)
D	TNDD023	293.2	305.3	REW	1	12.1	4	FO						30-60									Planar			SM												N.McMillan	
D	TNDD023	305.3	309.27	REW	1	3.97	3	FO						30-60									Undulating			SM												N.McMillan	
D	TNDD023	309.27	309.8	REW	1	0.53	3	FO						60-90									Undulating			SM												N.McMillan	Steep and shiny/smooth bedding surfaces associated with a fault.
D	TNDD023	309.8	324.1	REW	1	14.3	3	FO						30-60									Undulating			SM												N.McMillan	Some bedding surfaces are also rough. Some 0 - 30 joints.
D	TNDD023	324.1	325.37	REW	1	1.27	2	FO						60-90									Undulating			K												N.McMillan	Steep and shiny/smooth bedding surfaces associated with a fault.
D	TNDD023	325.37	328	REW	1	2.63	3	FO						60-90									Undulating			SM												N.McMillan	Some stepped/irregular joint breaks.
D	TNDD023	328	332.3	REW	1	4.3	3	FO						30-60									Planar			SM												N.McMillan	Bedding may be more undulating/irregular. Some stepped/irregular joint breaks.
D	TNDD023	332.3	338.1	REW	1	5.8	3	JN						0-30									Irregular			RO												N.McMillan	.
D	TNDD023	338.1	343	REW	1	4.9	3	FO						30-60									Planar			SM												N.McMillan	. Some irregular joints
D	TNDD023	343	351	REW	1	8	3	FO						60-90									Planar			SM												N.McMillan	Some more undulating bedding surfaces. Steeper beds likely associated with an interpreted fault @345m
D	TNDD023	351	363.21	REW	1	12.21	3	FO						30-60									Planar			SM												N.McMillan	Bedding both planar and undulating surfaces. Irregular and rough joint surfaces.
D	TNDD023	363.21	366.87	REW	1	3.66	2	FL						60-90									Planar			K												N.McMillan	Bedding is parallel to core axis. Broken and rubbley core in sections. Brecciated. Fracture surfaces are both smooth and have slickensides.
D	TNDD023	366.87	374.7	REW	1	7.83	3	FO						30-60									Irregular			RO												N.McMillan	Bedding faces may also contain smoother surfaces.
D	TNDD023	374.7	375.2	REW	1	0.5	2	SH						0-30									Irregular			SM												D.Sully	Low angle, graphitic
D	TNDD023	375.2	382.79	REW	1	7.59	3	FO						60-90									Irregular			RO												D.Sully	Some brecciation in core, irregular breaks, some graphitic surfaces
D	TNDD023	382.79	405.43	REW	1	22.64	3	FO						30-60									Planar			SM												D.Sully	Typically clean breaks typically along bedding planes
D	TNDD023	405.43	405.61	REW	1	0.18	3	SH						0-30									Planar			SM												D.Sully	Graphitic, very fine slickensides
D	TNDD023	405.61	431.6	REW	1	25.99	3	SH						30-60									Planar			SM												D.Sully	Generally clean breaks, parallel to bedding
D	TNDD023	431.6	433.7	REW	1	2.1	3	JN						30-60									Curved			RO												D.Sully	Rough breaks with minor amounts of clay on surface
D	TNDD023	433.7	438.61	REW	1	4.91	3	FO						30-60									Planar			SM												D.Sully	Graphitic breaks, generally parallel to bedding
D	TNDD023	438.61	440.07	REW	1	1.46	3	JN						60-90									Planar			VRO												D.Sully	Rough breaks, minor amounts of clay on surfaces
D	TNDD023	440.07	459.32	REW	1	19.25	3	FO						60-90									Planar			SM												D.Sully	Smooth graphitic breaks, typically bedding parallel
D	TNDD023	459.32	459.49	REW	1	0.17	3	BC						60-90									Irregular			RO												D.Sully	Small interval of broken rock
D	TNDD023	459.49	463.13	REW	1	3.64	3	FO						60-90									Planar			SM												D.Sully	Graphitic breaks, typically bedding parallel
D	TNDD023	463.13	469.23	REW	1	6.1	3	JN						30-60									Planar			RO												D.Sully	Clean surfaces along breaks, no graphite or clays observable
D	TNDD023	469.23	479.91	REW	1	10.68	3	FO						30-60									Planar			SM												D.Sully	Clean breaks; typically along bedding surfces; commonly graphitic
D	TNDD023	479.91	480.88	REW	1	0.97	3	BC						30-60									Irregular			SM												D.Sully	Broken core with numerous intersecting surfaces
D	TNDD023	480.88	504.25	REW	1	23.37	3	FO						30-60									Irregular			SM												D.Sully	Bedding parallel breaks; surfaces are commonly graphitic.
D	TNDD023	504.25	504.9	REW	1	0.65	3	JN						30-60									Irregular			RO												D.Sully	
D	TNDD023	504.9	512.11	REW	1	7.21	3	FO						30-60									Planar			SM												D.Sully	Bedding parallel
D	TNDD023	512.11	512.44	REW	1	0.33	3	JN						0-30									Planar			RO												D.Sully	Small amounts of clay and pyrite on broken surface
D	TNDD023	512.44	534.48	REW	1	22.04	3	FO						30-60									Planar			SM												D.Sully	Bedding parallel
D	TNDD023	534.48	535.12	REW	1	0.64	3	BC						0-30									Planar			SM												D.Sully	Fractured core; graphitic surfaces
D	TNDD023	535.12	538.48	REW	1	3.36	3	BC						30-60									Planar			SM												D.Sully	Bedding parallel
D	TNDD023	538.48	538.67	REW	1	0.19	2	JN						0-30									Planar			RO												D.Sully	Minot clay on fracture surface
D	TNDD023	538.67	544	REW	1	5.33	3	FO						30-60									Planar			SM												D.Sully	Bedding parallel
D	TNDD023	544	544.09	REW	1	0.09	3	JN						30-60									Planar			SM												D.Sully	Minor amounts of clay on surface
D	TNDD023	544.09	545.97	REW	1	1.88	3	FO						30-60									Planar			SM												D.Sully	Bedding parallel
D	TNDD023	545.97	547.85	REW	1	1.88	3	JN						30-60									Planar			SM												D.Sully	Minor amounts of clay, graphite and pyrite on fracture surface
D	TNDD023	547.85	558.25	REW	1	10.4	3	FO						30-60									Planar			SM												D.Sully	Bedding parallel
D	TNDD023	558.25	579.32	REW	1	21.07	3	FO						30-60									Planar			SM												D.Sully	Bedding parallel. Breaks commonly graphitic.
D	TNDD023	579.32	582.59	REW	1	3.27	3	BC						30-60									Planar			SM												D.Sully	Interval of broken core. Grpahite and clay common on surfaces
D	TNDD023	582.59	659.84	REW	1	77.25	2	FO						30-60									Planar			SM												D.Sully	Typically bedding parallel
D	TNDD023	659.84	660	REW	1	0.16	3	FL						30-60																								D.Sully	Cataclasite (?) and breccia interval. No obvious offsetting.
D	TNDD023	660	729	REW	1	69	2	FO						30-60									Planar			SM												N.McMillan	Some steeper and flat fracture breaks. Bedding fracture surfaces appear to be smoother than other.
D	TNDD023	729	786.6	REW	1	57.6	2	FO						0-30									Planar			SM												N.McMillan	Some flat joint breaks. Many of the bedding surfaces are very smooth.
D	TNDD023	786.6	815.4	REW	1	28.8	2	JN						0-30									Planar			RO												N.McMillan	Some flat joint breaks which may be more irregular. Also flat bedding breaks,
D	TNDD023	815.4	817.16	REW	1	1.76	1	BC																														N.McMillan	Interval of soft fissile/friable and broken core with dol silt. Softer core is broken.
D	TNDD023	817.16	828.86	REW	1	11.7	2	FO						0-30									Planar			SM												N.McMillan	Some flat fractures/breaks/joints. Rare/minor soft broken muds,
D	TNDD023	828.86	829.51	REW	1	0.65	1	FO						0-30																								N.McMillan	Interval of soft fissile/friable muds and softer dol silts. Breaks are generally "disking"
D	TNDD023	829.51	834.09	REW	1	4.58	2	FO						0-30									Planar			SM												N.McMillan	Some flat (0-30) joint fractures.
D	TNDD023	834.09	834.16	REW	1	0.07	2	FO																		SM												N.McMillan	Broken core. Some surfaces have slickensides.
D	TNDD023	834.16	838.57	REW	1	4.41	2	FO						0-30									Planar			SM												N.McMillan	
D	TNDD023	838.57	838.91	REW	1	0.34	1	FO						0-30									Planar			SM												N.McMillan	Interval of soft fissile/friable muds. Some surfaces are polished.
D	TNDD023	838.91	840.42	REW	1	1.51	2																															N.McMillan	
D	TNDD023	840.42	840.82	REW	1	0.4	1	BC																														N.McMillan	Interval of soft fissile/friable muds and softer dol silts.
D	TNDD023	840.82	852.8	REW	1	11.98	2	FO						0-30									Planar			SM												N.McMillan	Some flat joint fractures.
D	TNDD023	852.8	852.83	REW	1	0.03	1	BC																														N.McMillan	Broken core with polished surfaces.
D	TNDD023	852.83	854.55	REW	1	1.72	2	FO						0-30									Planar			SM												N.McMillan	
D	TNDD023	854.55	854.85	REW	1	0.3	1	BC																														N.McMillan	Interval of soft fissile/friable/broken muds and softer dol silts.
D	TNDD023	854.85	856.09	REW	1	1.24	2	FO						0-30									Planar			SM												N.McMillan	
D	TNDD023	856.09	856.97	REW	1	0.88	1	BC						0-30																								N.McMillan	Core tends to break along bedding planes although this also breaks. Some polishing on surfaces.
D	TNDD023	856.97	879.41	REW	1	22.44	2	FO						0-30									Planar			SM												N.McMillan	Most breaks are along bedding planes. Surfaces are generally flat with some roughness.
D	TNDD023	879.41	881.05	REW	1	1.64	1	FO						0-30									Planar			SM												N.McMillan	Intervals of soft fissile/friable muds and softer silts. Breaks are both along bedding planes and irregular breaks/crumbling.
D	TNDD023	881.05	908.05	REW	1	27	2	FO						0-30									Planar			SM												N.McMillan	Appears to be an even split between fracture breaks along bedding planes and flat fractures.  These may be flat and smooth or irregular.
D	TNDD023	908.05	912	REW	1	3.95	2	FO						0-30									Planar			K												N.McMillan	
D	TNDD023	912	915.75	REW	1	3.75	3	FO						0-30									Planar			SM												N.McMillan	Appears to be an even split between fracture breaks along bedding planes and flat fractures.  These may be flat and smooth or irregular.
D	TNDD023	915.75	916.06	REW	1	0.31	1	FO						0-30									Planar															N.McMillan	Interval of very soft rock with broken along bedding planes. Some polished surfaces.
D	TNDD023	916.06	927.27	REW	1	11.21	2	FO						0-30									Planar			SM												N.McMillan	Combination of flat joint breaks with rough surfaces and breaks along beddding planes
D	TNDD023	927.27	927.36	REW	1	0.09	0	BC																		SM												N.McMillan	Soft broken shards of core. Surfaces often polished.
D	TNDD023	934.96	935.02	REW	1	0.06	0	BC																		SM												N.McMillan	Soft broken shards of core. Surfaces often polished.
D	TNDD023	935.02	942.9	REW	1	7.88	2	FO						0-30									Planar			SM												N.McMillan	
D	TNDD023	942.9	943.12	REW	1	0.22	0	BC																														N.McMillan	Mostly soft broken and rubbly core with an interval of more competent core.
D	TNDD023	943.12	959.15	REW	1	16.03	2	FO						0-30									Planar			SM												N.McMillan	Generally smooth (or slightly rough) surfaces to flat breaks along interpreted bedding planes. Some other flat joint breaks with irregular surfaces.
D	TNDD023	959.15	965.5	REW	1	6.35	2	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	965.5	975.8	REW	1	10.3	2	JN						0-30									Irregular			SM												N.McMillan	Some breaks may also be in the 30 - 60 degree angle.  Faces can be irregular to more planar and smooth/rough.
D	TNDD023	975.8	975.85	REW	1	0.05	1	BC																														N.McMillan	Soft broken/crumbly rock associated with a fault. Some polished surfaces.
D	TNDD023	975.85	975.9	REW	1	0.05	0	BC																														N.McMillan	Soft broken/crumbly rock associated with a fault. Some polished surfaces.
D	TNDD023	975.9	988.53	REW	1	12.63	2	JN						0-30									Irregular			RO												N.McMillan	Generally flat lying breaks with variable surfaces - can be smooth and rough
D	TNDD023	988.53	988.62	REW	1	0.09	0	BC						0-30									Irregular			RO												N.McMillan	A combination of soft broken shards of core and more compentent core.
D	TNDD023	988.62	999.52	REW	1	10.9	2	JN						0-30									Planar			RO												N.McMillan	A combination of flat and more angled (30 - 60) joint breaks and can be more irregular. Beds surfaces range from smooth to rough.
D	TNDD023	999.52	999.8	REW	1	0.28	2	BC																														N.McMillan	
D	TNDD023	999.8	1008.63	REW	1	8.83	2	JN						30-60									Irregular			RO												N.McMillan	Joints surfaces of core fractures - some are irregular and others are flatter.
D	TNDD023	1008.63	1009	REW	1	0.37	2	JN						30-60									Irregular			RO												N.McMillan	Flat and steep breaks with soft/slick surfaces.
D	TNDD023	1009	1009.42	REW	1	0.42	3	JN															Irregular			RO												N.McMillan	
D	TNDD023	1009.42	1010.58	REW	1	1.16	2	JN						30-60									Planar			RO												N.McMillan	Some steeper fractures (60-90)
D	TNDD023	1010.58	1011.35	REW	1	0.77	3																															N.McMillan	
D	TNDD023	1011.35	1017.04	REW	1	5.69	2	JN																		SM												N.McMillan	A fault zone - minor amount of broken core and irregular fracture surfaces - often polished. No recognisable displacement.
D	TNDD023	1017.04	1017.21	REW	1	0.17	1																															N.McMillan	Appears to be a fault zone - soft rock.
D	TNDD023	1017.21	1019.81	REW	1	2.6	3	JN																		SM												N.McMillan	A fault zone - minor amount of broken core and irregular fracture surfaces - often polished. No recognisable displacement.
D	TNDD023	1019.81	1021.9	REW	1	2.09	2	FO						0-30									Planar			SM												N.McMillan	
D	TNDD023	1021.9	1023.92	REW	1	2.02	3	JN						0-30									Planar			RO												N.McMillan	
D	TNDD023	1023.92	1026.35	REW	1	2.43	2	JN						0-30									Planar			RO												N.McMillan	
D	TNDD023	1026.35	1029.6	REW	1	3.25	3	JN															Irregular															N.McMillan	A fault zone, fracture surfaces are irregular, flat, undulating and may be smooth or polished and rough/irregular.
D	TNDD023	1029.6	1030	REW	1	0.4	3	BC																														N.McMillan	
D	TNDD023	1030	1034.09	REW	1	4.09	3	FO						0-30									Undulating			SM												N.McMillan	Also some irregular fractures
D	TNDD023	1034.09	1035.23	REW	1	1.14	1	BC																														N.McMillan	Variably crumbled/broken core and some more compentent core.
D	TNDD023	1035.23	1040.26	REW	1	5.03	3	JN						0-30									Planar			SM												N.McMillan	May also break along bedding planes
D	TNDD023	1040.26	1040.37	REW	1	0.11	2	JN																														N.McMillan	Appears to be a fault - coherent rock
D	TNDD023	1040.37	1051.55	REW	1	11.18	2	FO						30-60									Undulating			SM												N.McMillan	Fracture surfaces may be flat and/or undulating.
D	TNDD023	1051.55	1053.77	REW	1	2.22	3	JN						0-30									Irregular			SM												N.McMillan	
D	TNDD023	1053.77	1063	REW	1	9.23	3	FO						60-90									Planar			RO												N.McMillan	Some fracture surfaces variably rough/smooth, fracture shape could be undulating. Some flatter (0 - 60) breaks.
D	TNDD023	1063	1069.89	REW	1	6.89	3	FO						60-90									Planar			RO												N.McMillan	Some minor intervals of broken core. Some fracture shapes can be more undulating.
D	TNDD023	1069.89	1070.51	REW	1	0.61	2	FO						60-90									Undulating			RO												N.McMillan	
D	TNDD023	1070.51	1080.73	REW	1	10.22	2	FO						0-30									Planar			SM												N.McMillan	A combination of flat smooth/rough bedding planes and flat irregular joint breaks.
D	TNDD023	1080.73	1081	REW	1	0.27	1	BC																														N.McMillan	Variably competent and flakey/broken chips.
D	TNDD023	1081	1084.23	REW	1	3.23	2	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1084.23	1084.38	REW	1	0.15	2	BC																														N.McMillan	Associated with fault
D	TNDD023	1084.38	1085.54	REW	1	1.16	1	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1085.54	1085.8	REW	1	0.26	2	BC																														N.McMillan	Associated with fault zone
D	TNDD023	1085.8	1089.16	REW	1	3.36	2	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1089.16	1089.2	REW	1	0.04	1	BC																														N.McMillan	Broken chips of fissile/friable muds.
D	TNDD023	1089.2	1089.52	REW	1	0.32	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1089.52	1089.56	REW	1	0.04	1	FO						0-30									Planar															N.McMillan	Disking
D	TNDD023	1089.56	1091.7	REW	1	2.14	2	JN						0-30									Planar															N.McMillan	Fraceture surfaces can be undulating and planar, range from smooth to rough.
D	TNDD023	1091.7	1093.53	REW	1	1.83	3	FO						30-60									Undulating			RO												N.McMillan	
D	TNDD023	1093.53	1097.43	REW	1	3.9	2	FO						0-30									Planar			SM												N.McMillan	Also some stepped/irregular fractures.
D	TNDD023	1097.43	1099.42	REW	1	1.99	3	FO						0-30									Planar			SM												N.McMillan	Fracture surfaces can be rough
D	TNDD023	1099.42	1102	REW	1	2.58	2	FO						0-30									Planar			SM												N.McMillan	Fracture surfaces can be smooth-rough
D	TNDD023	1102	1102.32	REW	1	0.32	3	FO						0-30									Planar			RO												N.McMillan	Fracture surfaces can be smooth-rough. Minor intervals of muds - softer.
D	TNDD023	1102.32	1109	REW	1	6.68	2	JN						0-30									Irregular			RO												N.McMillan	Some bedding breaks.
D	TNDD023	1109	1127.5	REW	1	18.5	2	FO						0-30									Planar			RO												N.McMillan	Bedding surfaces are generally rough-smooth.
D	TNDD023	1127.5	1128	REW	1	0.5	3	VN						30-60									Planar			RO												N.McMillan	
D	TNDD023	1128	1130	REW	1	2	2	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1130	1130.38	REW	1	0.38	3																															N.McMillan	
D	TNDD023	1130.38	1132.52	REW	1	2.14	2	JN						0-30									Undulating			RO												N.McMillan	
D	TNDD023	1132.52	1136.48	REW	1	3.96	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1136.48	1148.68	REW	1	12.2	3	FO						0-30									Undulating			RO												N.McMillan	
D	TNDD023	1148.68	1162.26	REW	1	13.58	4	JN						0-30									Irregular			RO												N.McMillan	Minor intervals of carb (+/- pyrite) silts is 2. Soft rock
D	TNDD023	1162.26	1164.94	REW	1	2.68	3	FO						0-30									Undulating			RO												N.McMillan	
D	TNDD023	1164.94	1167.15	REW	1	2.21	4	JN						0-30									Planar			RO												N.McMillan	
D	TNDD023	1167.15	1170.3	REW	1	3.15	3	FO						0-30									Planar			RO												N.McMillan	
D	TNDD023	1170.3	1170.85	REW	1	0.55	3	BC																														N.McMillan	
D	TNDD023	1170.85	1179.9	REW	1	9.05	3	JN						0-30									Irregular			RO												N.McMillan	A combination of fractures along bedding planes and joint fractures.
D	TNDD023	1179.9	1185.23	REW	1	5.33	3	FO						60-90									Undulating			SM												N.McMillan	Some fracture surfaces have smooth almost soapy surfaces. Likely associated with faulting.
D	TNDD023	1185.23	1185.39	REW	1	0.16	3	BC																														N.McMillan	
D	TNDD023	1185.39	1187.65	REW	1	2.26	3	JN						60-90									Irregular			SM												N.McMillan	Fracture surfaces may also be smooth/polished
D	TNDD023	1187.65	1189.24	REW	1	1.59	3	BC																														N.McMillan	Predominantly broken core with minor intervals of competent core.
D	TNDD023	1189.24	1193	REW	1	3.76	3	FO						60-90									Undulating			SM												N.McMillan	
D	TNDD023	1193	1195.47	REW	1	2.47	4	JN						0-30									Irregular			RO												N.McMillan	Both flat joints and bedding plane fractures.
D	TNDD023	1195.47	1196.9	REW	1	1.43	3	FO						60-90									Undulating			SM												N.McMillan	Fracture  surfaces may be irregular and rough.
D	TNDD023	1196.9	1220	REW	1	23.1	4	FO						0-30									Irregular			RO												N.McMillan	Combination of flat joints and breaks along veins.
D	TNDD023	1220	1220.25	REW	1	0.25	4	BC																														N.McMillan	
D	TNDD023	1220.25	1221.5	REW	1	1.25	4	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1221.5	1221.98	REW	1	0.48	4	BC																														N.McMillan	
D	TNDD023	1221.98	1225	REW	1	3.02	3	JN															Irregular			RO												N.McMillan	Increased fractures and minor intervals of broken core. Surfaces may be smooth or rough. Generally irregular. Some bedding breaks bur generally joint fractures.
D	TNDD023	1225	1245.4	REW	1	20.4	4	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1245.4	1247	REW	1	1.6	3	FO						60-90									Irregular			RO												N.McMillan	
D	TNDD023	1247	1248.03	REW	1	1.03	1	BC																														N.McMillan	
D	TNDD023	1248.03	1248.88	REW	1	0.85	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1248.88	1253.12	REW	1	4.24	4	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD023	1253.12	1254.5	REW	1	1.38	4	FO						60-90									Irregular			SM												N.McMillan	
D	TNDD023	1254.5	1260.89	REW	1	6.39	3	FO						60-90									Irregular			SM												N.McMillan	
D	TNDD023	1260.89	1263.03	REW	1	2.14	3	FO						0-30									Planar			RO												N.McMillan	
D	TNDD023	1263.03	1263.24	REW	1	0.21	3	BC																														N.McMillan	
D	TNDD023	1263.24	1266.15	REW	1	2.91	3	FO						60-90									Undulating			SM												N.McMillan	A combination of flat and steep bedding breaks.
D	TNDD023	1266.15	1298.75	REW	1	32.6	4	JN						0-30									Irregular			RO												N.McMillan	A combination of flat and irregular fracture surfaces.
D	TNDD023	1298.75	1298.89	REW	1	0.14	4	BC																														N.McMillan	
D	TNDD023	1298.89	1321.09	REW	1	22.2	4	JN						0-30									Irregular			RO												N.McMillan	A combination of flat and irregular fracture surfaces - both joint and rare bedding fractures.
D	TNDD024a	0	9.3	REW	1	9.3	0	BC																														N.McMillan	Strongly weathered
D	TNDD024a	9.3	11.95	REW	1	2.65	1	BC																														N.McMillan	Strongly weathered
D	TNDD024a	11.95	14.6	REW	1	2.65	0	BC																														N.McMillan	Strongly weathered
D	TNDD024a	14.6	16	REW	1	1.4	1																															N.McMillan	Strongly weathered
D	TNDD024a	16	28.17	REW	1	12.17	0	BC																														N.McMillan	Strongly weathered
D	TNDD024a	28.17	34.7	REW	1	6.53	1	BC																														N.McMillan	Strongly weathered
D	TNDD024a	34.7	41.3	REW	1	6.6	0	BC																														N.McMillan	Strongly weathered
D	TNDD024a	41.3	44.95	REW	1	3.65	1	BC																														N.McMillan	Strongly weathered
D	TNDD024a	44.95	49.7	REW	1	4.75	2	BC																														N.McMillan	Strongly weathered
D	TNDD024a	49.7	50.6	REW	1	0.9	1	BC																														N.McMillan	Strongly weathered. Some irregular fractures.
D	TNDD024a	50.6	56.4	REW	1	5.8	3	BC																														N.McMillan	Strongly weathered. Variably both competent and broken core.
D	TNDD024a	56.4	58.4	REW	1	2	2	BC																														N.McMillan	Strongly weathered. Variably both competent and broken core.
D	TNDD024a	58.4	64.4	REW	1	6	3	BC																														N.McMillan	Strongly weathered. Predominantly compentent core with some broken sections.
D	TNDD024a	64.4	64.65	REW	1	0.25	0																															N.McMillan	Strongly weathered.
D	TNDD024a	64.65	71.8	REW	1	7.15	3																															N.McMillan	Strongly weathered. Split between compentent and broken core.
D	TNDD024a	71.8	84.7	REW	1	12.9	3	BC																														N.McMillan	Strongly weathered. Predominantly broken core with intervals of competent core. Core hardness is generally average wth some soft and very soft broken core.
D	TNDD024a	84.7	88.2	REW	1	3.5	0	BC																														N.McMillan	Strongly weathered. Very soft, regularly crumbly/broken
D	TNDD024a	88.2	89.3	REW	1	1.1	3	JN															Irregular			RO												N.McMillan	Strongly weathered.
D	TNDD024a	89.3	90.8	REW	1	1.5	0	JN																														N.McMillan	Strongly weathered. Crumbly broken rock.
D	TNDD024a	90.8	91.08	REW	1	0.28	3	JN						0-30									Irregular			RO												N.McMillan	Weathered.
D	TNDD024a	91.08	92.2	REW	1	1.12	0																															N.McMillan	Strongly weathered. Crumbly core.
D	TNDD024a	92.2	103.6	REW	1	11.4	3	BC																														N.McMillan	Strongly weathered. Broken and competent core.
D	TNDD024a	103.6	104	REW	1	0.4	0																															N.McMillan	Strongly weathered. Soft clay.
D	TNDD024a	104	108.82	REW	1	4.82	3	BC																														N.McMillan	Weathered. Split between broken and competent core.
D	TNDD024a	108.82	117.7	REW	1	8.88	3	JN															Irregular			RO												N.McMillan	Some fractures are along beeding planes but generally irregular and not consistently oriented.
D	TNDD024a	117.7	118.1	REW	1	0.4	3	BC																														N.McMillan	
D	TNDD024a	118.1	119.4	REW	1	1.3	3	JN															Irregular			RO												N.McMillan	Generally fractured and along bedding planes.
D	TNDD024a	119.4	124.9	REW	1	5.5	3	BC																														N.McMillan	Dominated by broken core
D	TNDD024a	124.9	129.35	REW	1	4.45	3	JN															Irregular			RO												N.McMillan	Generally fractured and  also along bedding planes.
D	TNDD024a	129.35	130.9	REW	1	1.55	3	BC																														N.McMillan	Dominated by broken core.
D	TNDD024a	130.9	137.85	REW	1	6.95	3	JN						30-60									Irregular			RO												N.McMillan	Generally fractured and  also along some bedding planes.
D	TNDD024a	137.85	141.4	REW	1	3.55	3	JN						30-60									Irregular			RO												N.McMillan	Intervals of competent and broken core - interpreted to be associated wth fault.
D	TNDD024a	141.4	191.5	REW	1	50.1	3	FO						30-60									Planar			RO												N.McMillan	Breaks predominantly along bedding planes - generally 30-60 with some flatter breaks. Surfaces are variably smooth to rough/irregular.
D	TNDD024a	191.5	201.75	REW	1	10.25	3	JN						0-30									Planar			RO												N.McMillan	Fracture and bedding breaks generally flatter and planar/rough.
D	TNDD024a	201.75	201.83	REW	1	0.08	1	BC						60-90									Irregular			RO												N.McMillan	Short interval filled with clay
D	TNDD024a	201.83	211.76	REW	1	9.93	3	JN						30-60									Planar			SM												N.McMillan	Breaks that are typically along beddng planes. Some fracture surfaces are pyritic and slightly rough.
D	TNDD024a	211.76	212.99	REW	1	1.23	3	BC						60-90									Irregular			SM												N.McMillan	Zone of strongly broken and rubbly core.
D	TNDD024a	212.99	225.7	REW	1	12.71	3	JN						30-60									Planar			SM												N.McMillan	Typically bedding parallel breaks. Pyrite commonly on fracture surfaces.
D	TNDD025	0	20.16	REW	1	20.16	1	BC															Irregular			RO												D.Sully	Strongly weathered and rubbly core. Some zones of more competent rock that have a hardness of two but overall interval is very soft and strongly fragmented.
D	TNDD025	20.16	36.57	REW	1	16.41	3	FO						30-60									Planar			SM												D.Sully	Typically bedding parallel fractures. Iron oxides on some surfaces at top of interval due to weathering.
D	TNDD025	36.57	37.7	REW	1	1.13	2	BC															Irregular			SM												D.Sully	Small zone of brecciation; interpreted fault zone characterised by rubbly and broken core. Some graphitisation of fracture surfaces.
D	TNDD025	37.7	48.31	REW	1	10.61	3	JN						60-90									Irregular			RO												D.Sully	Sharp irregular breaks in core; typically at a steep angle to core axis. Minor bedding parallel fractures. Iron oxides on some fracture surfaces due to weathering.
D	TNDD025	48.31	51.01	REW	1	2.7	3	BC															Irregular			RO												D.Sully	Interpreted fault zone. Rubbly core with some competent sections. Minor amounts of clay on fracture surfaces.
D	TNDD025	51.01	70.05	REW	1	19.04	3	JN						60-90									Irregular			RO												D.Sully	Sharp irregular breaks in core; typically at a steep angle to core axis.
D	TNDD025	70.05	71.3	REW	1	1.25	3	BC															Irregular			RO												D.Sully	Zone of oxidised and weathered core. Traces of clay on rock fragments. Possibly a cavity,
D	TNDD025	71.3	85.76	REW	1	14.46	3	JN						60-90									Irregular			RO												D.Sully	Sharp irregular breaks in core; typically at a steep angle to core axis.
D	TNDD025	85.76	86.45	REW	1	0.69	3	BC															Irregular			RO												D.Sully	Zone of oxidised and weathered core. Traces of clay on rock fragments. Possibly a cavity,
D	TNDD025	86.45	97.81	REW	1	11.36	3	JN						60-90									Irregular			RO												D.Sully	Sharp irregular breaks in core; typically at a steep angle to core axis.
D	TNDD025	97.81	98.18	REW	1	0.37	2	BC															Irregular			RO												D.Sully	Zone of oxidised and weathered core. Traces of clay on rock fragments. Possibly a cavity,
D	TNDD025	98.18	109.08	REW	1	10.9	3	FO						30-60									Planar			SM												D.Sully	Typically bedding parallel fractures
D	TNDD025	109.08	131.02	REW	1	21.94	3	JN						60-90									Irregular			RO												D.Sully	Rough breaks, typically at a steep angle to core axis. Iron oxides common on broken surfaces. Some bedding parallel fractures but these are relatively minor compared to jointing.
D	TNDD025	131.02	131.41	REW	1	0.39	3	BC						60-90									Irregular			RO												D.Sully	Narrow zone of broken core; possible faults zone. Iron oxides and clay on fracture surfaces. Core is slightly oxidised.
D	TNDD025	131.41	146.4	REW	1	14.99	3	FO						60-90									Planar			SM												D.Sully	Typically bedding parallel fractures. Trace iron oxides on some surfaces.
D	TNDD025	146.4	146.51	REW	1	0.11	3	BC						60-90									Irregular			RO												D.Sully	Narrow zone of broken core. Minor amounts of graphite and clay on fracture surfaces; no iron oxides apparent.
D	TNDD025	146.51	149.37	REW	1	2.86	3	FO						60-90									Planar			SM												D.Sully	Typically bedding parallel fractures
D	TNDD025	149.37	149.64	REW	1	0.27	3	BC						60-90									Irregular			RO												D.Sully	Possibly a small fault zone; trace amounts of clay on fracture surfaces
D	TNDD025	149.64	163.92	REW	1	14.28	3	FO						60-90									Planar			SM												D.Sully	Typically bedding parallel fractures
D	TNDD025	163.92	163.99	REW	1	0.07	3	BC						60-90									Irregular			RO												D.Sully	Narrow zone of broken core; possible fault zone. Minor amounts of graphite on rock fragments
D	TNDD025	163.99	178.92	REW	1	14.93	3	FO						60-90									Planar			SM												D.Sully	Predominantly bedding parallel fractures
D	TNDD025	178.92	182.01	REW	1	3.09	3	JN						60-90									Irregular			RO												D.Sully	Irregular fracturing and jointing above an interpreted fault zone. Trace amounts of clay on fracture surfaces.
D	TNDD025	182.01	182.41	REW	1	0.4	2	FL						60-90									Irregular			SM												D.Sully	Interpreted fault zone; extensive carbonate flooding. Fracture surfaces are smooth and graphitic; slickensides developed on some surfaces. Small voids in carbonate infill.
D	TNDD025	182.41	188.13	REW	1	5.72	3	FL						60-90									Irregular			SM												D.Sully	Interpreted fault zone; slickensides on graphitic fractures surfaces;
D	TNDD025	188.13	200.99	REW	1	12.86	3	FO						60-90									Curved			SM												D.Sully	Bedding parallel fractures
D	TNDD025	200.99	210.13	REW	1	9.14	3	JN						60-90									Irregular			RO												D.Sully	Jointing typically perpindicular to core axis; irregular and rough fracture surfaces
D	TNDD025	210.13	210.68	REW	1	0.55	3	FL						60-90									Irregular			RO												D.Sully	Strongly brecciated interval; core is competent but clay rich carbonaceous(?) infill between clasts.
D	TNDD025	210.68	212.89	REW	1	2.21	3	SH						60-90									Planar			SM												D.Sully	Bedding parallel graphitic fracture surfaces. Slickensides developed on some fracture surfaces; probably related to underlying and overlying fault zones
D	TNDD025	212.89	217.87	REW	1	4.98	3	FL						60-90									Irregular			RO												D.Sully	Fault zone; fracture surfaces are commonly graphitic and have slickensides; some bedding parallel fractures
D	TNDD025	217.87	236.92	REW	1	19.05	3	FO						60-90									Planar			SM												D.Sully	Bedding parallel fractures; surfaces are commonly graphitic
D	TNDD025	236.92	243.34	REW	1	6.42	3	JN						60-90									Planar			RO												D.Sully	Jointing at a shallow angle to core axis; some bedding parallel fractures in interval
D	TNDD025	243.34	253.18	REW	1	9.84	3	FO						60-90									Planar			RO												D.Sully	Bedding parallel fractures; commonly graphitic fracture surfaces
D	TNDD025	253.18	253.85	REW	1	0.67	3	BC						60-90									Irregular			RO												D.Sully	Zone of strongly fractured core; no significant movement apparent
D	TNDD025	253.85	284.7	REW	1	30.85	3	FO						60-90									Planar			RO												D.Sully	Bedding parallel fractures. Frequent breaks down interval with rough to smooth knobbly fracture surfaces that are commonly graphitic
D	TNDD025	284.7	285.03	REW	1	0.33	3	BC															Irregular			RO												D.Sully	Small interval of broken core. Small amounts of pyrite coating some fracture surfaces
D	TNDD025	285.03	302.92	REW	1	17.89	3	FO						60-90									Planar			SM												D.Sully	Bedding parallel fracturing. Two 1cm thick clay rich carbonaceous intervals at 287.05 and 287.31m
D	TNDD025	302.92	304.06	REW	1	1.14	3	JN						60-90									Irregular			RO												D.Sully	
D	TNDD025	304.06	318.45	REW	1	14.39	3	FO						60-90									Planar			SM												D.Sully	Bedding parallel fractures. Rubbly rock from 311.4 to 312.2m; interpreted as re-drill when casing off from HQ down to NQ
D	TNDD025	318.45	318.95	REW	1	0.5	3	BC															Irregular			RO												D.Sully	Interval of broken core. No evidence of significant movement.
D	TNDD025	318.95	320.94	REW	1	1.99	3	FO						60-90									Planar			SM												D.Sully	Typically bedding parallel fractures
D	TNDD025	320.94	321.1	REW	1	0.16	3	SH						60-90									Planar			SM												D.Sully	Small shear zone with slickensides developed. No major displacement apparent
D	TNDD025	321.1	340.41	REW	1	19.31	3	FO						60-90									Planar			SM												D.Sully	Typically bedding parallel fractures. Fractures running parallel to stylolites between 335.49 to 337.64m
D	TNDD025	340.41	341.87	REW	1	1.46	3	JN						60-90									Irregular			RO												D.Sully	Interval of strongly fractured core. No slickensides observed on fracture surfaces
D	TNDD025	341.87	353.59	REW	1	11.72	3	FO						60-90									Planar			SM												D.Sully	Bedding parallel fractures
D	TNDD025	353.59	353.77	REW	1	0.18	3	JN						60-90									Planar			RO												D.Sully	Joint running at a shallow angle to core axis
D	TNDD025	353.77	359.51	REW	1	5.74	3	FO						60-90									Planar			SM												D.Sully	Bedding parallel fractures
D	TNDD025	359.51	360.76	REW	1	1.25	3	FL						60-90									Irregular			RO												D.Sully	Small fault zone; slickensides evident on fragments of broken core
D	TNDD025	360.76	377.72	REW	1	16.96	3	FO						60-90									Planar			SM												D.Sully	Bedding parallel fractures
D	TNDD025	377.72	378.16	REW	1	0.44	3	JN						60-90									Planar			RO												D.Sully	Joint running at a shallow angle to core axis
D	TNDD025	378.16	384.21	REW	1	6.05	3	FO						60-90									Planar			SM												D.Sully	Bedding parallel fractures
D	TNDD025	384.21	384.46	REW	1	0.25	3	BC						60-90									Irregular			RO												D.Sully	Interval of strongly broken core; probable fault zone.
D	TNDD025	384.46	403.64	REW	1	19.18	2	FO						60-90									Planar			SM												D.Sully	Typically bedding parallel fractures. Interval contains harder dolulutite of average strength (3); however given frequency of softer carbonaceous beds/laminatons an overall hardness of 2 has been assumed.
D	TNDD025	403.64	405.49	REW	1	1.85	2	JN						0-30									Planar			RO												D.Sully	Weak jointing developed at a shallow angle to core axis. Some bedding parallel fractures in interval
D	TNDD025	405.49	496.75	REW	1	91.26	2	FO						0-30									Planar			SM												D.Sully	Bedding parallel fractures. Interval contains minor harder dolulutite of average strength (3); however given frequency of softer carbonaceous beds/laminatons an overall hardness of 2 has been assumed. Fracture surfaces may be smooth-rough.
D	TNDD025	496.75	496.95	REW	1	0.2	1	BC																														N.McMillan	Minor interval of broken/fissile core and soft carbonaceous siltstone.
D	TNDD025	496.95	502.06	REW	1	5.11	3	JN						0-30									Irregular			SM												N.McMillan	Irregular fracture surfaces. May be broken along stylolite surfaces. Surfaces may be smooth to smooth-rough.
D	TNDD025	502.06	512.47	REW	1	10.41	2	FO						0-30									Planar			RO												N.McMillan	Some fractures along veins - still associated with bedding planes.
D	TNDD025	512.47	512.54	REW	1	0.07	1	JN						0-30									Planar															N.McMillan	Fissile/broken core.
D	TNDD025	512.54	575.34	REW	1	62.8	2	JN						0-30									Planar			RO												N.McMillan	Breaks along bedding planes and flat joint breaks. Fracture surfaces are often irregular.
D	TNDD025	575.34	575.45	REW	1	0.11	2	SH						60-90									Planar			K												N.McMillan	
D	TNDD025	575.45	582.05	REW	1	6.6	2	FO						0-30									Planar			RO												N.McMillan	Breaks along bedding planes and flat joint breaks. Fracture surfaces are often planar-irregular.
D	TNDD025	582.05	582.09	REW	1	0.04	1	BC																														N.McMillan	
D	TNDD025	582.09	602.1	REW	1	20.01	2	JN						0-30									Planar			RO												N.McMillan	Breaks along bedding planes and flat joint breaks. Fracture surfaces are often irregular
D	TNDD025	602.1	603.15	REW	1	1.05	2	JN						60-90									Irregular			RO												N.McMillan	
D	TNDD025	603.15	629	REW	1	25.85	2	FO						0-30									Planar			RO												N.McMillan	Breaks along bedding planes and flat joint breaks. Fracture surfaces are often irregular-planar.
D	TNDD025	629	638.3	REW	1	9.3	2	JN						0-30									Planar			RO												N.McMillan	Irregular and steeper joint breaks start to increase. Breaks along bedding planes and flat joint breaks. Fracture surfaces are often irregular-planar.
D	TNDD025	638.3	671.43	REW	1	33.13	2	FO						0-30									Planar			RO												N.McMillan	Irregular and steeper joint breaks start to increase. Breaks along bedding planes and flat joint breaks. Fracture surfaces are often irregular-planar and range from smooth to rough.
D	TNDD025	671.43	685.12	REW	1	13.69	2	FO						0-30									Planar			RO												N.McMillan	Minor silt and dol intervals/nods increase but the overall rock strength is soft rock. Fracture surfaces are rough-smooth and planar-irregular.
D	TNDD025	685.12	687.75	REW	1	2.63	3	JN						0-30									Irregular			SM												N.McMillan	Fractures both irregular and planar.
D	TNDD025	687.75	687.85	REW	1	0.1	2	SH						60-90									Planar			K												N.McMillan	
D	TNDD025	687.85	692.15	REW	1	4.3	2	FO						0-30									Planar			RO												N.McMillan	Broken along bedding planes. Fracture surfaces are generallly smooth-rough.
D	TNDD025	692.15	692.84	REW	1	0.69	2	JN															Planar			RO												N.McMillan	Variable broken fractures.
D	TNDD025	692.84	703.82	REW	1	10.98	2	FO						0-30									Planar			RO												N.McMillan	Broken along bedding planes - rough-smooth planar fractures.
D	TNDD025	703.82	708.8	REW	1	4.98	2	JN						0-30									Planar			RO												N.McMillan	Some steeper fractures. Generally not along bedding planes.
D	TNDD025	708.8	709	REW	1	0.2	3	JN						30-60																								N.McMillan	
D	TNDD025	709	710.46	REW	1	1.46	2	FO						0-30									Planar			SM												N.McMillan	Both bedding breaks and joint fractures.
D	TNDD025	710.46	710.69	REW	1	0.23	2	BC																														N.McMillan	
D	TNDD025	710.69	717.49	REW	1	6.8	2	FO						0-30									Planar			RO												N.McMillan	Some fractures not along bedding planes.
D	TNDD025	717.49	721.05	REW	1	3.56	3	FO						0-30									Planar			RO												N.McMillan	Breaks generally along bedding planes
D	TNDD025	721.05	724.68	REW	1	3.63	2	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD025	724.68	724.82	REW	1	0.14	2	BC																														N.McMillan	
D	TNDD025	724.82	728.86	REW	1	4.04	2	FO						0-30									Planar			RO												N.McMillan	Rough-smooth planar fracture surfaces.
D	TNDD025	728.86	729.49	REW	1	0.63	3	FO						0-30									Planar			RO												N.McMillan	
D	TNDD025	729.49	731.6	REW	1	2.11	2	FO						0-30									Planar			RO												N.McMillan	
D	TNDD025	731.6	752.52	REW	1	20.92	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD025	752.52	754.09	REW	1	1.57	3	FO						0-30									Planar			RO												N.McMillan	Rough-smooth planar fracture surfaces.
D	TNDD025	754.09	758.2	REW	1	4.11	3	JN						30-60									Irregular			RO												N.McMillan	
D	TNDD025	758.2	769	REW	1	10.8	3	FO						30-60									Planar			RO												N.McMillan	Fracture surfaces may also be more irregular.
D	TNDD025	769	780.3	REW	1	11.3	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD025	780.3	780.57	REW	1	0.27	3	BC																														N.McMillan	
D	TNDD025	780.57	812.12	REW	1	31.55	3	JN						0-30									Irregular			RO												N.McMillan	Also 30-60 degrees.
D	TNDD025	812.12	812.25	REW	1	0.13	1																															N.McMillan	Also 30-60 degrees.
D	TNDD025	812.25	829.7	REW	1	17.45	3	FO						0-30									Planar			RO												N.McMillan	A combination of joint breaks and bedding fracture breaks. Fracture shape can be more irregular.
D	TNDD025	829.7	848.6	REW	1	18.9	3	FO						0-30									Planar			RO												N.McMillan	
D	TNDD025	848.6	851.48	REW	1	2.88	3	BC																														N.McMillan	Fault zone: a combinaton of competent and broken core. Broken surfaces may be smooth/polished.
D	TNDD025	851.48	857.4	REW	1	5.92	3	JN						0-30									Irregular			RO												N.McMillan	Planar/irregular fracture surfaces.
D	TNDD025	857.4	869.46	REW	1	12.06	3	FO						60-90									Irregular			RO												N.McMillan	Planar/irregular fracture surfaces.
D	TNDD025	869.46	870	REW	1	0.54	2	BC																														N.McMillan	Some broken peices of core can be crumbled in hand.
D	TNDD025	870	871.9	REW	1	1.9	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD025	871.9	872.23	REW	1	0.33	2	BC																														N.McMillan	
D	TNDD025	872.23	872.44	REW	1	0.21	3																															N.McMillan	
D	TNDD025	872.44	872.49	REW	1	0.05	3	BC																														N.McMillan	
D	TNDD025	872.49	873.14	REW	1	0.65	3	JN						30-60									Stepped			RO												N.McMillan	
D	TNDD025	873.14	873.88	REW	1	0.74	3	BC																														N.McMillan	
D	TNDD025	873.88	875.17	REW	1	1.29	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD025	875.17	875.37	REW	1	0.2	3	BC																														N.McMillan	
D	TNDD025	875.37	876.11	REW	1	0.74	3	JN						0-30									Planar			RO												N.McMillan	
D	TNDD025	876.11	876.5	REW	1	0.39	2	BC																														N.McMillan	
D	TNDD025	876.5	882.9	REW	1	6.4	3	JN						0-30									Irregular			RO												N.McMillan	Also breaks along bedding fractures.
D	TNDD026	0	0.57	REW	1	0.57	0																															N.McMillan	
D	TNDD026	0.57	5.07	REW	1	4.5	1	FO																														N.McMillan	Strongly weathered core. A minor interval of broken core. Possibly bedding breaks.
D	TNDD026	5.07	5.6	REW	1	0.53	2	FO						0-30									Planar															N.McMillan	
D	TNDD026	5.6	5.8	REW	1	0.2	1	FO						0-30									Planar															N.McMillan	
D	TNDD026	5.8	6.32	REW	1	0.52	1	BC																														N.McMillan	Strongly weathered broken core.
D	TNDD026	6.32	13.83	REW	1	7.51	3	JN						30-60									Irregular			RO												N.McMillan	Weathered core.
D	TNDD026	13.83	13.94	REW	1	0.11	2	BC																														N.McMillan	Weathered core.
D	TNDD026	13.94	17.17	REW	1	3.23	3	JN						30-60									Irregular			RO												N.McMillan	
D	TNDD026	17.17	17.36	REW	1	0.19	1	BC																														N.McMillan	Strongly weathered and broken core.
D	TNDD026	17.36	83.02	REW	1	65.66	3	JN						0-30									Irregular			RO												N.McMillan	Joint fractures predominantly 0-30 degreee, but also some 30 - 90 degrees
D	TNDD026	83.02	83.13	REW	1	0.11	0	BC																														N.McMillan	
D	TNDD026	83.13	163.18	REW	1	80.05	3																															N.McMillan	
D	TNDD026	163.18	192.65	REW	1	29.47	2	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD026	192.65	209.5	REW	1	16.85	3	FO						60-90									Irregular			RO												N.McMillan	Predominantly breaking on bedding planes.
D	TNDD026	209.5	216	REW	1	6.5	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD026	216	234	REW	1	18	3	FO						30-60									Irregular			RO												N.McMillan	Predominantly breaking on bedding planes. Rare smoother fracture surfaces. Rarer 60-90 degree
D	TNDD026	234	241.5	REW	1	7.5	3	FO						60-90									Irregular			RO												N.McMillan	Predominantly breaking on bedding planes. Rare smoother fracture surfaces. Rarer 30-60 degree
D	TNDD026	241.5	249	REW	1	7.5	3	FO						30-60									Planar			RO												N.McMillan	Predominantly breaking on bedding planes.
D	TNDD026	249	255.9	REW	1	6.9	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD026	255.9	304.02	REW	1	48.12	3	FO						30-60									Planar			RO												N.McMillan	Predominantly breaking on bedding planes - generally planar.  Some 30-60 degree breaks. Rare breaks along veins - 0-30 degrees.
D	TNDD026	304.02	312.28	REW	1	8.26	2	FO						30-60									Planar			RO												N.McMillan	Predominantly breaking on bedding planes - generally planar.  Some irregular 0-30 JN breaks.
D	TNDD026	312.28	320.54	REW	1	8.26	3	FO						30-60									Planar			RO												N.McMillan	LOWER CONTACT NOT COMPLETE. Predominantly breaking on bedding planes - generally planar.  Some irregular 0-30 JN breaks.
D	TNDD026	320.54	333.1	REW	1	12.56	3	FO						30-60									Planar			RO												N.McMillan	LOWER CONTACT NOT COMPLETE. Predominantly breaking on bedding planes - generally planar.  Some irregular 0-30 JN breaks.
D	TNDD026	333.1	340	REW	1	6.9	3	JN						60-90									Irregular			VRO												N.McMillan	
D	TNDD026	340	367.9	REW	1	27.9	3	JN						60-90									Undulating			SM												N.McMillan	Fracture surface can be rough or smooth
D	TNDD026	367.9	368.1	REW	1	0.2	2	FL						30-60									Undulating			K												N.McMillan	
D	TNDD026	368.1	376.6	REW	1	8.5	3	FO						30-60									Planar			SM												N.McMillan	
D	TNDD026	376.6	383.1	REW	1	6.5	3	FO						60-90									Irregular			RO												N.McMillan	
D	TNDD026	383.1	383.7	REW	1	0.6	2	FL																		K												N.McMillan	Predom broken core
D	TNDD026	383.7	391.5	REW	1	7.8	3	FO						60-90									Irregular			RO												N.McMillan	
D	TNDD026	391.5	391.55	REW	1	0.05	2	FL						30-60									Stepped			K												N.McMillan	Minor fault zone
D	TNDD026	391.55	402.6	REW	1	11.05	3	JN						60-90									Irregular			RO												N.McMillan	Some breaks along bedding planes.
D	TNDD026	402.6	404.35	REW	1	1.75	3	JN						0-30									Irregular			RO												N.McMillan	
D	TNDD026	404.35	412.2	REW	1	7.85	3	JN						60-90									Irregular			RO												N.McMillan	Fracture surfaces may be smooth or irregular.
D	TNDD026	412.2	416.6	REW	1	4.4	3	FO						30-60									Planar			SM												N.McMillan	
D	TNDD026	416.6	491.7	REW	1	75.1	3	FO						30-60									Planar			RO												N.McMillan	Some fracture surfaces are smooth. About 10% are 30-60 fractures.
D	TNDD026	491.7	526.85	REW	1	35.15	3	FO						60-90									Planar			SM												N.McMillan	
D	TNDD026	526.85	678	REW	1	151.15	3	FO						60-90									Planar			SM												M.Cawood	Minor high angle bedding parallel natural breaks. Generally very competent core
D	TNDD026	678	679.9	REW	1	1.9	2	FO						60-90									Planar			SM												M.Cawood	Minor high angle bedding parallel natural breaks. Drilling has created minor pitting of core
D	TNDD026	679.9	695.9	REW	1	16	3	FO						60-90									Planar			SM												M.Cawood	One rough fracture follwing vein at 685.6. Dolomite infill, rough surface 45 degrees LCA
D	TNDD026	695.9	696.7	REW	1	0.8	1	BC						60-90									Irregular			RO												M.Cawood	Discing of core particularly betwwen 696.5 and 696.7. Clay infill. Soft to very soft
D	TNDD026	696.7	709.5	REW	1	12.8	3	FO						60-90									Planar			SM												M.Cawood	
D	TNDD026	709.5	709.6	REW	1	0.1	1	FO						60-90									Stepped			SM												M.Cawood	Soft mudstone with sub cm breaks along foliaton
D	TNDD026	709.6	710.3	REW	1	0.7	3																															M.Cawood	No natural breaks
D	TNDD026	710.3	710.4	REW	1	0.1	2	FO						60-90									Undulating			SM												M.Cawood	1cm partings along mud infill planes
D	TNDD026	710.4	719.4	REW	1	9	3	FO						60-90									Planar			SM												M.Cawood	Rare breaks
D	TNDD026	719.4	719.65	REW	1	0.25	1	BC						60-90									Irregular			SM												M.Cawood	Broken core associated with mudstone unit
D	TNDD026	719.65	721.2	REW	1	1.55	3	JN						30-60									Planar			SM												M.Cawood	
D	TNDD026	721.2	721.3	REW	1	0.1	2	BC						60-90									Irregular			SM												M.Cawood	Broken core associated with mudstone unit. Breaks  parallel to bedding
D	TNDD026	721.3	735.4	REW	1	14.1	3	FO						60-90									Planar			SM												M.Cawood	Generally competent core
D	TNDD026	735.4	735.7	REW	1	0.3	2	FO						60-90									Irregular			RO												M.Cawood	cm scale breaks associated with mudstone unit
D	TNDD026	735.7	736.9	REW	1	1.2	3	FO						60-90									Planar			SM												M.Cawood	Generally competent core
D	TNDD026	736.9	737.5	REW	1	0.6	2	FO						60-90									Irregular			RO												M.Cawood	Strongly disced core associated with mudstone unit
D	TNDD026	737.5	760.1	REW	1	22.6	3	FO						60-90									Planar			SM												M.Cawood	Generally competent core. Minor natural breaks
D	TNDD026	760.1	760.2	REW	1	0.1	1	FO						60-90									Irregular			SM												M.Cawood	Friable muddy unit. Multiple breaks. Very soft
D	TNDD026	760.2	760.9	REW	1	0.7	3	FO						60-90									Irregular			SM												M.Cawood	Generally competent core but minor zone of friable muddy unit.
D	TNDD026	760.9	761.1	REW	1	0.2	1	FO						60-90									Irregular			SM												M.Cawood	Friable muddy unit. Multiple breaks. Very soft
D	TNDD026	761.1	762.1	REW	1	1	3	FO						60-90									Irregular			SM												M.Cawood	Generally competent but 2 minor intervals of friable muddy rock. These unites contain multiple breaks.
D	TNDD026	762.1	778.9	REW	1	16.8	3	FO						60-90									Planar			SM												M.Cawood	Generally competent. Few natural breaks
D	TNDD026	778.9	779.4	REW	1	0.5	1	FO						60-90									Irregular			SM												M.Cawood	Two soft muddy units with no inherent strength. Multiple breaks along foliation parallel to bedding. 10cm units separated by competent sediments
D	TNDD026	779.4	795.4	REW	1	16	3	FO						60-90									Planar			SM												M.Cawood	Generally competent core. Few natural breaks
D	TNDD026	795.4	795.5	REW	1	0.1	1	FL						60-90									Irregular			RO												M.Cawood	Potentially a minor fault but no slicks. Narrow zone of broken core but not strongly fractures either side
D	TNDD026	795.5	803.5	REW	1	8	3	FO						60-90									Planar			SM												M.Cawood	Generally competent core with minor natural breaks
D	TNDD026	803.5	803.55	REW	1	0.05	1	FO						60-90									Irregular			SM												M.Cawood	Strongly friable muddy? unit. No strength
D	TNDD026	803.55	813.15	REW	1	9.6	3	FO						60-90									Planar			SM												M.Cawood	Generally competent but one 2cm zone around 806.7 which has minor muddy infill
D	TNDD026	813.15	813.35	REW	1	0.2	1	FO						60-90									Irregular			RO												M.Cawood	Extremely broken friable zones - rubble. No inherent rock strength
D	TNDD026	813.35	815.4	REW	1	2.05	3	JN						0-30									Planar			SM												M.Cawood	One joint parallel to veining
D	TNDD026	815.4	815.65	REW	1	0.25	1	FO						60-90									Irregular			SM												M.Cawood	2 muddy very soft friable zones separated by a 20cm zone of competent rock
D	TNDD026	815.65	819.95	REW	1	4.3	3	FO						60-90									Planar			SM												M.Cawood	Competent core. Few natural breaks
D	TNDD026	819.95	820.3	REW	1	0.35	1	FO						60-90									Irregular			SM												M.Cawood	Highly friable muddy zones. No strength
D	TNDD026	820.3	824.05	REW	1	3.75	3	FO						60-90									Planar			SM												M.Cawood	Competent core. Few natural breaks
D	TNDD026	824.05	824.1	REW	1	0.05	1	FO						60-90									Irregular			SM												M.Cawood	Narrow zone  strongly broken - along foliation
D	TNDD026	824.1	840.6	REW	1	16.5	3	FO						60-90									Planar			SM												M.Cawood	Competent core. Few natural breaks
D	TNDD026	840.6	840.65	REW	1	0.05	0	FL						60-90																								M.Cawood	Narrow puggy fault zone
D	TNDD026	840.65	846.7	REW	1	6.05	3	FO						60-90									Planar			SM												M.Cawood	Competent core
D	TNDD026	846.7	850.9	REW	1	4.2	3	JN						60-90									Irregular			RO												M.Cawood	Short runs with broken core at the start and end of run potentially relatd to muddy partings
D	TNDD026	850.9	864	REW	1	13.1	3	FO						60-90									Planar			SM												M.Cawood	Numerous natural breaks. Core competency becoming lower down hole
D	TNDD026	864	865.25	REW	1	1.25	3	JN						60-90									Irregular			RO												M.Cawood	Increasingly broken core approaching fault
D	TNDD026	865.25	866.3	REW	1	1.05	0	FL						60-90									Irregular			K												M.Cawood	Very puggy narrow fault zone
D	TNDD026	866.3	868.25	REW	1	1.95	3	BC						60-90									Irregular			RO												M.Cawood	Broken core between 2 fault zones
D	TNDD026	868.25	868.3	REW	1	0.05	0	FL						60-90									Irregular			K												M.Cawood	Puggy narrow fault zone
D	TNDD026	868.3	883.2	REW	1	14.9	3	FO						60-90									Planar			SM												M.Cawood	Multiple zones of 5cm broken core associted with muddy zones. Core between in generally competent breaking along bedding plane
D	TNDD026	883.2	900.9	REW	1	17.7	3	FO						60-90									Planar			SM												M.Cawood	Generally competent core. Some breaks wrap around dolomite nodules
D	TNDD026	900.9	906.4	REW	1	5.5	3	FO						60-90									Irregular			RO												M.Cawood	Bedding parallel breaks but rough and irregulkar in character
D	TNDD026	906.4	915.5	REW	1	9.1	3	FO						60-90									Planar			SM												M.Cawood	Moderate amoun t of natural breaks mostly parallel to bedding. Some at high angle to LCA
D	TNDD026	915.5	955	REW	1	39.5	3	FO						60-90									Irregular			RO												M.Cawood	Similar amount of breaks as above but irregular and rough
D	TNDD026	955	987	REW	1	32	3	FO						60-90									Planar			RO												N.McMillan	Predominantly flat/planar fracture surfaces. May be smooth but generally rough.
D	TNDD026	987	987.7	REW	1	0.7	3	FO						0-30									Undulating			RO												N.McMillan	Irregular to undulating fracture surfaces.
D	TNDD026	987.7	990.5	REW	1	2.8	3	JN						60-90									Irregular			RO												N.McMillan	Average to hard rock
D	TNDD026	990.5	994.35	REW	1	3.85	3	JN						30-60																								N.McMillan	Inconsistent fracture breaks. Predominantly joint fractures.
D	TNDD026	994.35	999.2	REW	1	4.85	3	JN						60-90									Irregular			RO												N.McMillan	
D	TNDD026	999.2	1004	REW	1	4.8	3	JN						0-30									Irregular			RO												N.McMillan	Joint fractures parallel to core axis increase with some flat/perpendicular to core axis.
D	TNDD026	1004	1016.8	REW	1	12.8	3	JN						60-90									Irregular			RO												N.McMillan	
D	TNDD026	1016.8	1018.5	REW	1	1.7	3	JN						0-30									Irregular			RO												N.McMillan	May break along stylolite fractures.
D	TNDD026	1018.5	1038.8	REW	1	20.3	3	JN						60-90									Irregular			RO												N.McMillan	May break along stylolite fractures.
D	TNDD026	1038.8	1041.6	REW	1	2.8	3	FL																														N.McMillan	
D	TNDD026	1041.6	1062.52	REW	1	20.92	3	JN						30-60									Irregular			RO												N.McMillan	30-60 fractures increase.
D	TNDD026	1062.52	1064.05	REW	1	1.53	3	FL																														N.McMillan	
D	TNDD026	1064.05	1068.3	REW	1	4.25	3	JN						60-90									Irregular			RO												N.McMillan	Rare steep/parallel to core axis
D	TNDD026	1068.3	1069.75	REW	1	1.45	3	FL																														N.McMillan	
D	TNDD026	1069.75	1087	REW	1	17.25	3	JN						60-90									Irregular			RO												N.McMillan	Rare planar fracture breaks - rem bedding?
D	TNDD026	1087	1089.6	REW	1	2.6	3	JN						30-60									Irregular			RO												N.McMillan	Rare planar fracture breaks - rem bedding?
D	TNDD026	1089.6	1089.88	REW	1	0.28	3	BC																														N.McMillan	
D	TNDD026	1089.88	1092.55	REW	1	2.67	3	JN						60-90									Irregular			RO												N.McMillan	
D	TNDD026	1092.55	1092.84	REW	1	0.29	3	BC																														N.McMillan	
D	TNDD026	1092.84	1097.6	REW	1	4.76	3	JN						0-30									Irregular			RO												N.McMillan	Both 0-30 and 60-90 joint fractures.
D	TNDD026	1097.6	1098.02	REW	1	0.42	3	FL																														N.McMillan	
D	TNDD026	1098.02	1102.12	REW	1	4.1	3	JN						60-90									Irregular			RO												N.McMillan	
D	TNDD027	0	1.9	REW	1	1.9	0																															N.McMillan	Strongly altered core. Broken core and tabarite.
D	TNDD027	1.9	10.24	REW	1	8.34	2	BC	FO			35			30-60									Planar			RO			PC								N.McMillan	A combination of broken and more competent core with fractures. Core is strœngly weathered/altered including on fracture surfaces. Fractures are predom on bedding planes but alteration can obscure this.
D	TNDD027	10.24	37.23	REW	1	26.99	3	JN	FO	JN	50	10	10	60-90	30-60	0-30							Irregular	Planar	Undulating	RO	RO	RO	SA	SA	SA							N.McMillan	Fracture surface may be stained/altered.
D	TNDD027	37.23	37.6	REW	1	0.37	3		BC																					SA								N.McMillan	
D	TNDD027	37.6	70.14	REW	1	32.54	3	JN	FO		45	13		60-90	30-60								Irregular	Planar		RO	VRO		CL	CL								N.McMillan	
D	TNDD027	70.14	72.08	REW	1	1.94	3	JN			21			30-60									Irregular			RO			PC									N.McMillan	Irregular fracture breaks with rare breaks along bedding planes. Weathering and alteration along fracture breaks. Vugs?
D	TNDD027	72.08	76.5	REW	1	4.42	2	FL			90			60-90									Irregular			RO			CC			hem			1.5			N.McMillan	Fault zone. Intervals of broken rubble and more competent core with fracture breaks. Hematite weathered/alteration on surfaces.
D	TNDD027	76.5	83.5	REW	1	7	3	FO			20			60-90									Irregular			RO			PC									N.McMillan	Predominately competent core with some intervals of broken core coated/stained with iron oxides. Fracture breaks are irregular.
D	TNDD027	83.5	88.4	REW	1	4.9	3	JN	FO		5	1					55	55		190	190		Irregular	Planar		RO	SM		CL	CL								N.McMillan	A combination of planar fracture breaks along bedding planes and bedding parallel but irregular stylolites.
D	TNDD027	88.4	111.4	REW	1	23	3	FO	JN	JN	12	11	9		60-90	0-30	55			195			Planar	Irregular	Irregular	RO	SM	RO	CL	CL	CL							N.McMillan	A combination of planar smooth-rough bedding fractures; irregular low angle to core axis fractures and "flatter" high angle to core axis fractures.
D	TNDD027	111.4	114.27	REW	1	2.87	3	JN	JN		5	2		0-30	60-90								Undulating	Irregular		VRO	RO		CC	CL								N.McMillan	Irregular fractires at vey low angles to core bedding axis. Iron oxide coating on fracture surfaces which also seem to be associated with carbonate veining. Other flatter high angle fractures.
D	TNDD027	114.27	120.8	REW	1	6.53	2	FO	JN		11	4			0-30		60			275			Planar	Irregular		RO	RO		CL	CL								N.McMillan	A combination of irregular-planar rough bedding breaks and rarer low angle fracture breaks.
D	TNDD027	120.8	122.3	REW	1	1.5	3	FO	JN		5	3			0-30		64			0			Planar	Irregular		RO	RO		CL	PC								N.McMillan	
D	TNDD027	122.3	122.45	REW	1	0.15	3	BC																					CC									N.McMillan	
D	TNDD027	122.45	166.15	REW	1	43.7	3	FO	JN	JN	45	20	15	30-60	30-60	0-30							Planar	Irregular	Undulating	SM	RO	RO	CL	CL	PC							N.McMillan	Generally breaks along bedding planes which may be along stylolites so flat/planar and more irregular. With irregular low angle to core axis irregular fractures.
D	TNDD027	166.15	170.8	REW	1	4.65	3		JN			12			60-90									Irregular			VRO			CL								N.McMillan	Irregular fracture breaks which may be along stylolites.
D	TNDD027	170.8	201.5	REW	1	30.7	3	FO	FO	JN	45	25	10	30-60	30-60	0-30							Planar	Irregular	Planar	SM	RO	RO	CL	CL	CL							N.McMillan	Generally breaks along bedding planes which may be along stylolites so flat/planar and more irregular. With irregular low angle to core axis irregular fractures.
D	TNDD027	201.5	207.03	REW	1	5.53	2	JN	FO		7	5		30-60	30-60								Planar	Planar		RO	SM		PC	CL								N.McMillan	Joint fractures may be planar or irregular with some vein infill/coating. Bedding fractures may be rough or smooth-rough.
D	TNDD027	207.03	226.2	REW	1	19.17	3	FO	FO	JN	24	18	5	60-90	60-90	30-60							Planar	Irregular	Planar	RO	VRO	RO	CL	CL	PC							N.McMillan	Predom planar/irregular bedding breaks - mostly along mud interbeds. Some stylolite breaks and low angle fracture breaks.
D	TNDD027	226.2	323.65	REW	1	97.45	3	FO	JN	JN	10	6	5	60-90	60-90	0-30							Undulating	Irregular	Irregular	RO	RO	RO	CL	CL	CL							N.McMillan	Fracture breaks along wavy/itregular bedding breaks. Some low angle fractures and irregular high angle fractures.
D	TNDD027	323.65	376	REW	1	52.35	3	FO	JN		70	8		60-90	0-30								Undulating	Planar		RO	RO		CL	CL								N.McMillan	Irregular/undulating or planar bedding fractures may be along stylolites. Some low angled fractures
D	TNDD027	376	395.89	REW	1	19.89	3	FO			30			60-90									Planar			RO			CL									N.McMillan	Generally planar fracture surfaces (60 - 90)
D	TNDD027	408.1	420.12	REW	1	12.02	3	JN			15			60-90									Irregular			RO			CL									N.McMillan	Generally planar and some irregular fracture breaks. Not necessarily along bedding planes.
D	TNDD027	432.1	469.85	REW	1	37.75	2	FO	JN		50	10		60-90	0-30								Planar	Planar		RO	RO		CL	CL								N.McMillan	Flat planar bedding breaks. Low angled fractures - may be rough to smooth fracture surfaces - some along veins.
D	TNDD027	469.85	475.54	REW	1	5.69	3	FO			20			60-90									Undulating			RO			CL									N.McMillan	Undulating to planar fracture surfaces - rough to smooth faces. May break along vein surfecase which are also along bedding planes.
D	TNDD027	475.54	479.01	REW	1	3.47	3	FO	JN		6	3		60-90	60-90								Planar	Irregular		RO	RO		CL	CL								N.McMillan	Planar and irregular fracture surfaces. Minor interval (<5cm) of broken core.
D	TNDD027	479.01	479.06	REW	1	0.05	1																															N.McMillan	
D	TNDD027	479.06	498.9	REW	1	19.84	3	FO			30			60-90									Planar			RO			CL									N.McMillan	Mostly fractured along bedding planes - may be planar but with irregaulr/rough fracture surfaces.
D	TNDD027	498.9	498.93	REW	1	0.03	1	BC																														N.McMillan	
D	TNDD027	498.93	525.09	REW	1	26.16	2	FO			30			60-90									Irregular			RO			CL									N.McMillan	Irregular fractures along bedding planes.
D	TNDD027	525.09	525.16	REW	1	0.07	2	BC																														N.McMillan	
D	TNDD027	525.16	560	REW	1	34.84	2	FO	JN		40	4		60-90	60-90								Irregular	Stepped		RO	RO		CL	CL								N.McMillan	Irregular/planar breaks along bedding planes. Rarer stepped breaks.
D	TNDD027	560	567.92	REW	1	7.92	2	FO	JN		12	3		60-90	30-60								Planar	Irregular		RO	RO		CL	CL								N.McMillan	Broken along bedding planes and irregular joint fractures.
D	TNDD027	567.92	568.04	REW	1	0.12	1	BC																														N.McMillan	
D	TNDD027	568.04	569.3	REW	1	1.26	2	FO			2			60-90									Irregular			RO			CL									N.McMillan	
D	TNDD027	569.3	569.41	REW	1	0.11	1	BC																														N.McMillan	
D	TNDD027	569.41	594.87	REW	1	25.46	2	FO	JN		45	5		60-90	30-60								Irregular	Planar		RO	RO		CL	CL								N.McMillan	Irregular breaks along bedding planes.
D	TNDD027	594.87	594.99	REW	1	0.12	1	BC																														N.McMillan	
D	TNDD027	594.99	595.8	REW	1	0.81	2	FO			3			60-90									Planar			RO			CL									N.McMillan	
D	TNDD027	595.8	595.85	REW	1	0.05	1	BC																														N.McMillan	
D	TNDD027	595.85	639.33	REW	1	43.48	2	FO	JN		90	4		60-90	30-60								Planar	Irregular		RO	RO		CL	CL								N.McMillan	Probably breaking along bedding planes but difficult to see due to how dark the core is. Planar to irregular breaks generally rough. Some irregular joint fractures.
D	TNDD027	639.33	641	REW	1	1.67	2	FL			6			60-90									Irregular			RO			CL									N.McMillan	Possble fault zone. Significant veining and associated breccia. No obvious offset.
D	TNDD027	641	654.98	REW	1	13.98	2	FO	JN		40	7		60-90	60-90								Planar	Irregular		RO	RO		CL	CL								N.McMillan	Fractures generally along bedding planes and some irregular joint breaks.
D	TNDD027	654.98	655.25	REW	1	0.27	0	BC																														N.McMillan	FAULT ZONE
D	TNDD027	655.77	674.04	REW	1	18.27	2	FO	JN		25	15		60-90	60-90								Planar	Irregular		RO	RO		CL	CL								N.McMillan	Predom planar bedding breaks.
D	TNDD027	674.04	674.47	REW	1	0.43	2	FL			4			60-90									Planar			K			CL									N.McMillan	
D	TNDD027	674.47	679.02	REW	1	4.55	2	JN	FO		10	5		60-90	60-90								Irregular	Planar		RO	RO		CL	CL								N.McMillan	Planar fractures may have smooth-rough surface.
D	TNDD027	679.02	679.94	REW	1	0.92	2	FL			5			30-60									Irregular			RO			CL									N.McMillan	
D	TNDD027	679.94	681.73	REW	1	1.79	3	JN	FO		3	3		0-30	60-90								Planar	Planar		RO	RO		CL	CL								N.McMillan	
D	TNDD027	681.73	681.82	REW	1	0.09	2	BC																														N.McMillan	
D	TNDD027	681.82	691.87	REW	1	10.05	3	FO	JN	FO	6	10	3	60-90	60-90	30-60							Planar	Irregular	Planar	RO	RO	VRO	CL	CL	CL							N.McMillan	A combination of fractures along bedding planes (30-60 and 60-90) and irregular joint fractures.
D	TNDD027	691.87	698	REW	1	6.13	3	FO			22			60-90									Irregular			RO			CL									N.McMillan	Broken along irregular bedding planes.
D	TNDD027	698	704.13	REW	1	6.13	3	JN	JN		30	7		60-90	30-60								Irregular	Irregular		RO	VRO		CL	CL								N.McMillan	
D	TNDD027	704.13	720.9	REW	1	16.77	3	JN	JN		35	5		60-90	30-60								Irregular	Irregular		VRO	VRO		CL	CL								N.McMillan	Some fractures cross cut veining but do not appear to break along veins.
D	TNDD027	720.9	724.16	REW	1	3.26	3	FO			19			60-90									Undulating			RO			CL									N.McMillan	Planar to undulating breaks with rough to smooth surfaces.
D	TNDD027	724.16	728.27	REW	1	4.11	2	FL			11			0-30									Irregular			RO			CL									N.McMillan	
D	TNDD027	728.27	736.63	REW	1	8.36	3	FO			60			60-90									Undulating			RO			CL									N.McMillan	Planar to undulating and rough-smooth surface fratures. Minor intervals of friable/fissile clays.
D	TNDD027	736.63	754	REW	1	17.37	3	JN			23			60-90									Irregular			RO			CL									N.McMillan	Planar to irregular fracture breaks.
D	TNDD027	754	786.9	REW	1	32.9	3	JN	JN	JN	35	11	3	60-90	60-90	0-30							Irregular	Planar	Irregular	RO	RO	VRO	CL	CL	CL							N.McMillan	Fractures
D	TNDD027	786.9	789	REW	1	2.1	2	FL			7			30-60									Irregular			VRO			PC									N.McMillan	
D	TNDD027	789	814.98	REW	1	25.98	3	JN	JN	FO	20	20	15	30-60	60-90	30-60							Irregular	Irregular	Planar	VRO	RO	RO	CL	CL	CL							N.McMillan	Joint breaks are irregular-planar with rough to very rough surface. Foliation breaks are planar-undulating.
D	TNDD027	814.98	815.15	REW	1	0.17	1	BC																														N.McMillan	Possible broken core.
D	TNDD027	815.15	836	REW	1	20.85	3	FO	JN	JN	30	15	5	60-90	60-90	30-60							Planar	Irregular	Irregular	RO	VRO	RO	CL	PC	CL							N.McMillan	Fractures along bedding planes - generally smooth to smooth-rough. Some breaks along stylolites.
D	TNDD027	836	896.5	REW	1	60.5	3	JN	JN	JN	60	25	5	60-90	30-60	0-30							Irregular	Planar	Planar	RO	RO	RO	CL	CL	CL							N.McMillan	
D	TNDD028	0	1.3	REW	1	1.3	0																															Contractor	
D	TNDD028	1.3	3.5	REW	1	2.2	2																						CC									Contractor	Moderately weathered broken ground.
D	TNDD028	3.5	21.8	REW	1	18.3	3	JN			2			60-90									Planar			RO			PC									Contractor	
D	TNDD028	21.8	41.68	REW	1	19.88	4	FL	JN		1	1		30-60	0-30								Planar	Planar		SM	SM		CL	SA								Contractor	
D	TNDD028	41.68	41.69	REW	1	0.01	4	CON			1			30-60									Planar			SM			CL									Contractor	Contact between breccia and dolomitic siltstone. Contact is not broken
D	TNDD028	41.69	58	REW	1	16.31	4	FO	JN	JN	24	5	4	30-60	60-90	0-30							Planar	Planar	Planar	SM	SM	SM	CL	CL	ST							Contractor	
D	TNDD028	58	62.6	REW	1	4.6	4	JN	VN		6	30		30-60	30-60								Planar	Undulating		SM	SM		CL	CL								Contractor	
D	TNDD028	62.6	124.7	REW	1	62.1	4	FO	JN	JN	90	50	8	30-60	60-90	60-90							Planar	Planar	Planar	SM	SM	SM	CL	CL	CL							Contractor	
D	TNDD028	124.7	135.9	REW	1	11.2	4	VN			90			30-60									Irregular			SM			CL									Contractor	
D	TNDD028	135.9	150	REW	1	14.1	4	FO	JN		25	8		30-60	60-90								Planar	Planar		SM	SM		CL	CL								Contractor	
D	TNDD028	150	156	REW	1	6	4	JN	FO		5	3		60-90	30-60								Planar	Planar		SM	SM		CL	CL								Contractor	
D	TNDD028	156	159	REW	1	3	4	JN	VN		3	10		0-30	30-60								Undulating	Planar		RO	SM		CL	CL								Contractor	
D	TNDD028	159	167	REW	1	8	4	FO	JN		25	2		30-60	0-30								Planar	Undulating		SM	RO		CL	CL								Contractor	
D	TNDD028	167	170	REW	1	3	4	BC	JN		90	10			30-60									Planar			SM		CL	CL								Contractor	smal lzone of broken ground. a couple of joints along lca
D	TNDD028	170	173.5	REW	1	3.5	4	JN	VN		10	40		60-90	0-30								Stepped	Irregular		RO	SM		CL	CL								Contractor	
D	TNDD028	173.5	187	REW	1	13.5	4	JN	FO	JN	20	30	3	30-60	30-60	0-30							Planar	Planar	Undulating	SM	SM	RO	CL	CL	CL							Contractor	
D	TNDD028	187	194	REW	1	7	4	FO			7			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	194	211	REW	1	17	4	FO	JN		15	4		30-60	30-60								Planar	Undulating		SM	SM		CL	CL								D. Woolford	
D	TNDD028	211	238	REW	1	27	4	FO	JN		25	4		30-60	30-60								Planar	Undulating		SM	SM		CL	CL								D. Woolford	
D	TNDD028	238	243	REW	1	5	4	JN	FO		1	5		0-30	30-60								Undulating	Planar		SM	RO		CL	CL								D. Woolford	
D	TNDD028	243	262	REW	1	19	4	JN	JN	FO	5	17	25	0-30	30-60	30-60							Planar	Undulating	Planar	SM	SM	SM	CL	CL	CL							D. Woolford	
D	TNDD028	262	278	REW	1	16	4	FO	JN	JN	30	12	2	30-60	30-60	0-30							Planar	Undulating	Planar	SM	SM	SM	CL	CL	CL							D. Woolford	
D	TNDD028	278	290.61	REW	1	12.61	4	FO	JN		25	7		30-60	30-60								Planar	Planar		SM	SM		CL	CL								D. Woolford	
D	TNDD028	290.61	313.37	REW	1	22.76	4	FO	JN	CON	50	3	1	30-60	30-60	30-60							Planar	Planar	Planar	SM	SM	SM	CL	CL	CL							D. Woolford	
D	TNDD028	313.37	319	REW	1	5.63	4	JN			2			0-30									Undulating			SM			CL									D. Woolford	
D	TNDD028	319	332	REW	1	13	4	VN			25			60-90									Planar			SM			IN			car			2			D. Woolford	
D	TNDD028	332	345	REW	1	13	4	VN	FO		7	14		0-30	30-60								Planar	Planar		SM	SM		IN	CL		car			3			D. Woolford	
D	TNDD028	345	357	REW	1	12	4	FO			10			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	357	369	REW	1	12	4	FO			5			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	369	397	REW	1	28	4	VN			50			30-60									Planar			SM			IN			car			2			D. Woolford	
D	TNDD028	397	512	REW	1	115	3	FO			70			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	512	556	REW	1	44	3	VN			30			0-30									Planar			SM			IN			car			2			D. Woolford	
D	TNDD028	556	569	REW	1	13	3	FO			5			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	569	573	REW	1	4	3	VN			17			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	573	582	REW	1	9	3	FO			8			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	582	651.5	REW	1	69.5	4	FO			15			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	651.5	651.7	REW	1	0.2	1	FL			1			30-60									Planar			SM			CL									D. Woolford	
D	TNDD028	651.7	700	REW	1	48.3	3	FO	JN		50	10		30-60	30-60								Planar	Planar		SM	SM		CL	CL								D. Woolford	Irregularly spaced zones of crumbly foliated breaks. Upto 50mm thick
D	TNDD028	700	748.82	REW	1	48.82	3	VN	FO		70	25		30-60	30-60								Planar	Planar		SM	SM		IN	CL		car			2			D. Woolford	
D	TNDD028	748.82	749.4	REW	1	0.58	1	BC																					CL									N.McMillan	Intervals of broken/fissile and friable clay and competent core.
D	TNDD028	749.4	750.49	REW	1	1.09	3	FO	JN		4	3		30-60	30-60								Undulating	Planar		SM	RO		CL	CL								N.McMillan	Joints may be planar to irregular.
D	TNDD028	750.49	750.69	REW	1	0.2	1	BC																														N.McMillan	Broken fissile and friable clay.
D	TNDD028	750.69	751.65	REW	1	0.96	3	FO	JN		5	3		0-30	0-30								Planar	Planar		SM	K		CC	PC								N.McMillan	A combination of smooth and slickenside fracture surfaces. Joints are planar to irregular.
D	TNDD028	751.65	751.92	REW	1	0.27	1	BC																														N.McMillan	Fissile/friable broken muds.
D	TNDD028	751.92	754.15	REW	1	2.23	3	FO			10			0-30									Undulating			SM			CL									N.McMillan	Fracture surfaces are smooth to "mirror-like"
D	TNDD028	754.15	757.25	REW	1	3.1	3	FO	JN		9	2		30-60	30-60								Planar	Irregular		RO	RO		CL	CL								N.McMillan	
D	TNDD028	757.25	768.5	REW	1	11.25	3	FO	SH	JN	9	7	9	0-30	60-90	30-60							Planar	Irregular	Planar	SM	RO	RO	CL	CL	PC							N.McMillan	Joint fractures may break along veins.
D	TNDD028	768.5	777.7	REW	1	9.2	3	FO	JN		13	12		0-30	60-90								Undulating	Irregular		RO	RO		CL	CL								N.McMillan	Foliation breaks are undulating/irregular.
D	TNDD028	777.7	780.9	REW	1	3.2	3	FO	JN		4	3		60-90	30-60								Irregular	Irregular		RO	RO		CL	CL								N.McMillan	Joints are planar to irregular.
D	TNDD028	780.9	786.57	REW	1	5.67	3	FO			11			0-30									Undulating			RO			CL									N.McMillan	Fracture surfaces may be rough to smooth.
D	TNDD028	786.57	786.63	REW	1	0.06	1	BC																														N.McMillan	
D	TNDD028	786.63	788.05	REW	1	1.42	3	FO	JN		3	1		0-30	60-90								Undulating	Planar		RO	RO		CL	CL								N.McMillan	
D	TNDD028	788.05	788.2	REW	1	0.15	1	BC																														N.McMillan	
D	TNDD028	788.2	799.4	REW	1	11.2	3	FO	FO		20	3		60-90	60-90								Undulating	Irregular		RO	RO		CL	CL								N.McMillan	Foliation surfaces are planar/undulating and may be rough-smooth or and rarely smooth.
D	TNDD028	799.4	816.06	REW	1	16.66	3	FO	FO	JN	16	15	3	0-30	30-60	60-90							Undulating	Undulating	Irregular	RO	RO	RO	CL	CL	CL							N.McMillan	Planar to undulating fracture surfaces. May be smooth-rough to rough.
D	TNDD028	816.06	816.44	REW	1	0.38	3	BC																														N.McMillan	Broken core may be related to drilling.
D	TNDD028	816.44	819.36	REW	1	2.92	3	FO	FO		10	3		60-90	30-60								Undulating	Irregular		SM	RO		CL	CL								N.McMillan	Bedding may be planar/undulating or irregular.
D	TNDD028	819.36	820.05	REW	1	0.69	1	BC																														N.McMillan	
D	TNDD028	820.05	821.45	REW	1	1.4	3	JN	FO		6	3		30-60	30-60								Planar	Planar		RO	RO		CL	CL								N.McMillan	
D	TNDD028	821.45	821.62	REW	1	0.17	1	BC																														N.McMillan	
D	TNDD028	821.62	824.1	REW	1	2.48	3	FO	FO		7	4		0-30	30-60								Undulating	Undulating		RO	SM		CL	CL								N.McMillan	
D	TNDD028	824.1	824.2	REW	1	0.1	1	BC																														N.McMillan	
D	TNDD028	824.2	825.76	REW	1	1.56	3	FO			5			60-90									Planar			SM			CL									N.McMillan	
D	TNDD028	825.76	829.53	REW	1	3.77	3	FL	FO		4	2		60-90	0-30								Irregular	Irregular		RO	RO		CL	CL								N.McMillan	Fault zone
D	TNDD028	829.53	829.69	REW	1	0.16	1	BC																														N.McMillan	
D	TNDD028	829.69	832.75	REW	1	3.06	3	FO	JN		7	1		30-60	60-90								Curved	Irregular		RO	RO		CL	CL								N.McMillan	
D	TNDD028	832.75	834.8	REW	1	2.05	3	JN			2			0-30									Irregular			RO			CL									N.McMillan	
D	TNDD028	834.8	841.7	REW	1	6.9	3	FO	JN		10	3		30-60	60-90								Irregular	Irregular		RO	RO		CL	CL								N.McMillan	
D	TNDD028	841.7	848.9	REW	1	7.2	3	JN	FO		8	12		60-90	30-60								Irregular	Irregular		RO	RO		CL	CL								N.McMillan	Bedding fractures are planar/irregular rough-smooth.
D	TNDD028	848.9	849.5	REW	1	0.6	3	BC																														N.McMillan	
D	TNDD028	849.5	861.08	REW	1	11.58	3	FO	JN	JN	15	7	3	30-60	60-90	30-60							Planar	Irregular	Planar	RO	RO	RO	CL	CL	CL							N.McMillan	
D	TNDD028	861.08	865.87	REW	1	4.79	3	FO	JN	JN	6	4	3	0-30	60-90	30-60							Planar	Irregular	Planar	RO	RO	RO	CL	CL	CL							N.McMillan	
D	TNDD028	865.87	867.9	REW	1	2.03	3	BC																														N.McMillan	
D	TNDD028	867.9	873.57	REW	1	5.67	3	FO	FO		7	7		30-60	30-60								Undulating	Planar		RO	RO		CL	CL								N.McMillan	Bedding fractures may be undulating due to dol nods.
D	TNDD028	873.57	873.84	REW	1	0.27	2	BC																														N.McMillan	
D	TNDD028	873.84	885.56	REW	1	11.72	3	FO	JN	JN	17	3	3	30-60	0-30	60-90							Undulating	Planar	Irregular	RO	RO	RO	CL	CL	CL							N.McMillan	
D	TNDD028	885.56	885.72	REW	1	0.16	3	BC																														N.McMillan	
D	TNDD028	885.72	891.15	REW	1	5.43	3	FO			10			30-60									Undulating			RO			CL									N.McMillan	
D	TNDD028	891.15	891.37	REW	1	0.22	2	BC																														N.McMillan	
D	TNDD028	891.37	892.05	REW	1	0.68	3	FO			5			30-60									Planar			SM			CL									N.McMillan	
D	TNDD028	892.05	892.13	REW	1	0.08	2	BC																														N.McMillan	
D	TNDD028	892.13	893.58	REW	1	1.45	3	FO			7			0-30									Planar			SM			CL									N.McMillan	Average to soft rock.
D	TNDD028	893.58	901	REW	1	7.42	3	JN	JN		11	2		60-90	60-90								Irregular	Planar		VRO	RO		CL	CL								N.McMillan	
D	TNDD028	901	917.61	REW	1	16.61	3	FO	JN		21	4		30-60	60-90								Planar	Irregular		RO	RO		CL	CL								N.McMillan	
D	TNDD028	917.61	918.2	REW	1	0.59	3																						CL									N.McMillan	FAULT. No fractures.
D	TNDD028	918.2	919.6	REW	1	1.4	3	JN			3			60-90									Irregular			RO			CL									N.McMillan	
D	TNDD028	919.6	923.26	REW	1	3.66	3	FO	FO		3	2		0-30	30-60								Planar	Undulating		SM	RO		CL	CL								N.McMillan	
D	TNDD028	923.26	924.99	REW	1	1.73	3	JN			4			60-90									Irregular			SM			CL									N.McMillan	
D	TNDD028	924.99	925.26	REW	1	0.27	2	BC																														N.McMillan	
D	TNDD028	925.26	930	REW	1	4.74	3	JN	BC	FO	5		4	60-90		30-60							Irregular		Planar	RO		RO	CL		CL							N.McMillan	
D	TNDD028	930	930.39	REW	1	0.39	3	BC																														N.McMillan	Possibly drilling related.
D	TNDD028	930.39	934.6	REW	1	4.21	3	JN	FO		9	3		60-90	30-60								Irregular	Planar		RO	RO		CL	CL								N.McMillan	
D	TNDD028	934.6	940.78	REW	1	6.18	3	JN	FO		7	4		60-90	0-30								Stepped	Undulating		RO	RO		PC	CL								N.McMillan	
D	TNDD028	940.78	943.8	REW	1	3.02	3	JN			4			60-90									Irregular			RO			CL									N.McMillan	
D	TNDD028	943.8	945.54	REW	1	1.74	3	FO			3			30-60									Planar			SM			CL									N.McMillan	
D	TNDD028	945.54	945.59	REW	1	0.05	2	BC																														N.McMillan	
D	TNDD028	945.59	961.04	REW	1	15.45	3	FO	JN		23	4		0-30	60-90								Planar	Irregular		SM	RO		CL	PC								N.McMillan	Foliation break surface is smooth-rough.
D	TNDD028	961.04	961.06	REW	1	0.02	0	BC																														N.McMillan	
D	TNDD028	961.06	961.27	REW	1	0.21	3	FO			2			30-60									Undulating			SM			CL									N.McMillan	
D	TNDD028	961.27	961.43	REW	1	0.16	1	BC																														N.McMillan	
D	TNDD028	961.43	964.11	REW	1	2.68	3	FO	JN		6	3		0-30	60-90								Undulating	Irregular		SM	RO		CL	CL								N.McMillan	Minor intervals of softer (2) green mud.
D	TNDD028	964.11	975.2	REW	1	11.09	3	FO	FO	JN	20	8	7	0-30	0-30	60-90							Planar	Undulating	Irregular	SM	SM	RO	CL	CL	PC							N.McMillan	Smooth to rough fracture surfaces.
D	TNDD028	975.2	975.5	REW	1	0.3	2	BC																														N.McMillan	
D	TNDD028	975.5	981.41	REW	1	5.91	3	FO	JN		18	6		0-30	60-90								Undulating	Irregular		SM	RO		CL	CL								N.McMillan	
D	TNDD028	981.41	981.8	REW	1	0.39	3	BC																														N.McMillan	
D	TNDD028	981.8	984.88	REW	1	3.08	3	JN	JN		9	2		60-90	60-90								Planar	Irregular		RO	RO		CL	CL								N.McMillan	
D	TNDD028	984.88	984.94	REW	1	0.06	1	BC																														N.McMillan	
D	TNDD028	984.94	1010.53	REW	1	25.59	3	FO	FO	JN	23	2	8	0-30	0-30	60-90							Planar	Undulating	Planar	SM	RO	RO	CL	CL	CL							N.McMillan	
D	TNDD028	1010.53	1011.1	REW	1	0.57	2																															N.McMillan	
D	TNDD028	1011.1	1011.69	REW	1	0.59	3	BC																														N.McMillan	Predominantly broken.
D	TNDD028	1011.69	1013.12	REW	1	1.43	3	FO	JN		7	2		0-30	60-90								Planar	Planar		SM	RO		CL	PC								N.McMillan	
D	TNDD028	1013.12	1013.34	REW	1	0.22	2	BC																														N.McMillan	
D	TNDD028	1013.34	1019.14	REW	1	5.8	3	FO	JN	JN	14	3	3	0-30	60-90	60-90							Planar	Planar	Irregular	SM	RO	SM	CL	PC	PC							N.McMillan	
D	TNDD028	1019.14	1019.17	REW	1	0.03	2	BC																														N.McMillan	
D	TNDD028	1019.17	1020.7	REW	1	1.53	3	FO	JN		2	2		0-30	60-90								Planar	Irregular		SM	RO		CL	CL								N.McMillan	
D	TNDD028	1020.7	1020.8	REW	1	0.1	2	BC																														N.McMillan	
D	TNDD028	1020.8	1026.67	REW	1	5.87	3	JN	FO		6	5		60-90	0-30								Irregular	Undulating		RO	RO		CL	CL								N.McMillan	
D	TNDD028	1026.67	1026.71	REW	1	0.04	2	BC																														N.McMillan	
D	TNDD028	1026.71	1027.71	REW	1	1	3	JN	FO		3	3		60-90	30-60								Irregular	Planar		RO	SM		CL	CL								N.McMillan	
D	TNDD028	1027.71	1028.3	REW	1	0.59	3	BC																														N.McMillan	Average to soft rock.
D	TNDD028	1028.3	1032.55	REW	1	4.25	3	JN	FO		7	3		60-90	0-30								Irregular	Planar		RO	SM		PC	CL								N.McMillan	
D	TNDD028	1032.55	1032.6	REW	1	0.05	3	BC																														N.McMillan	
D	TNDD028	1032.6	1036.75	REW	1	4.15	3	JN	FO		5	2		60-90	0-30								Irregular	Planar		RO	SM		PC	CL								N.McMillan	
D	TNDD028	1036.75	1040.12	REW	1	3.37	3	FL			2			60-90									Irregular			RO			PC									N.McMillan	
D	TNDD028	1040.12	1043.2	REW	1	3.08	3	FO	JN		4	3		0-30	60-90								Planar	Irregular		RO	RO		CL	PC								N.McMillan	Some joints are partially coated/veins.
D	TNDD028	1043.2	1043.9	REW	1	0.7	3	FL			1			0-30									Planar			RO			CL									N.McMillan	
D	TNDD028	1043.9	1047.27	REW	1	3.37	3	JN	FO	BC	3	3		60-90	0-30								Irregular	Undulating		RO	RO		PC	CL								N.McMillan	
D	TNDD028	1047.27	1047.34	REW	1	0.07	3	BC																														N.McMillan	
D	TNDD028	1047.34	1060.32	REW	1	12.98	3	JN	FO	FO	12	4	2	60-90	0-30	0-30							Irregular	Planar	Undulating	RO	RO	RO	PC	CL	CL							N.McMillan	Some jont fractures associated with veins.
D	TNDD028	1060.32	1060.47	REW	1	0.15	2	BC																														N.McMillan	
D	TNDD028	1060.47	1062.19	REW	1	1.72	3	JN	FO		1	2		60-90	60-90								Irregular	Irregular		RO	RO		CL	CC								N.McMillan	Mud on foliation fracture surface.
D	TNDD028	1062.19	1062.39	REW	1	0.2	2	BC																														N.McMillan	
D	TNDD028	1062.39	1063.78	REW	1	1.39	2	JN			2			60-90									Irregular			RO			PC									N.McMillan	
D	TNDD028	1063.78	1063.93	REW	1	0.15	2	BC																														N.McMillan	
D	TNDD028	1063.93	1066.29	REW	1	2.36	3	JN			5			60-90									Irregular			RO			PC									N.McMillan	
D	TNDD028	1066.29	1066.36	REW	1	0.07	2	BC																														N.McMillan	
D	TNDD028	1066.36	1067	REW	1	0.64	3	JN	FO		1	1		60-90	0-30								Irregular	Planar		RO	RO		CL	CL								N.McMillan	
D	TNDD028	1067	1068.23	REW	1	1.23	3	BC	JN	FO		4	2		60-90	0-30								Irregular	Planar		RO	RO		CL	CL							N.McMillan	Broken core may be soft rock (2).
D	TNDD028	1068.23	1071.3	REW	1	3.07	3	JN	FO		4	1		60-90	0-30								Irregular	Undulating		RO	SM		CL	CL								N.McMillan	
D	TNDD028	1071.3	1071.36	REW	1	0.06	2	BC																														N.McMillan	
D	TNDD028	1071.36	1073.76	REW	1	2.4	3	JN			5			60-90									Irregular			RO			CL									N.McMillan	Fractures may be broken along veins.
D	TNDD028	1073.76	1073.9	REW	1	0.14	2	BC																														N.McMillan	
D	TNDD028	1073.9	1076.44	REW	1	2.54	3	JN	FO		4	2		60-90	0-30								Irregular	Irregular		RO	RO		CL	CL								N.McMillan	Fractures may be broken on veins.
D	TNDD028	1076.44	1076.65	REW	1	0.21	2	BC																														N.McMillan	
D	TNDD028	1076.65	1077.78	REW	1	1.13	3	JN	FO		6	2		60-90	0-30								Irregular	Planar		RO	RO		CL	CL								N.McMillan	
D	TNDD028	1077.78	1078.34	REW	1	0.56	2	BC																														N.McMillan	
D	TNDD028	1078.34	1079.58	REW	1	1.24	3	JN	FO		4	3		60-90	0-30								Irregular	Undulating		RO	SM		CL	CL								N.McMillan	
D	TNDD028	1079.58	1080.51	REW	1	0.93	3	BC																														N.McMillan	
D	TNDD028	1080.51	1083.53	REW	1	3.02	3	JN	FO		9	7		60-90	30-60								Irregular	Planar		RO	RO		CL	CL								N.McMillan	
D	TNDD028	1083.53	1083.74	REW	1	0.21	3	BC																														N.McMillan	
D	TNDD028	1083.74	1090	REW	1	6.26	3	JN	JN		25	3		60-90	0-30								Irregular	Undulating		RO	SM		CL	CL								N.McMillan	
D	TNDD028	1090	1095.39	REW	1	5.39	3	FO	BC	JN	24		3	0-30		60-90							Undulating		Irregular	SM		RO	CL		CL							N.McMillan	Minor interval of broken core. Fracture surfaces are undulating to planar.
D	TNDD028	1095.39	1095.64	REW	1	0.25	3	BC																														N.McMillan	
D	TNDD028	1095.64	1100.7	REW	1	5.06	3	FO	BC	JN	20		4	0-30		60-90							Undulating		Irregular	SM		RO	CL		CL							N.McMillan	Minor intervals of broken core and bedding fractures.
D	TNDD028	1100.7	1101.4	REW	1	0.7	3	FL			1			60-90									Irregular			RO			CL									N.McMillan	
D	TNDD028	1101.4	1101.76	REW	1	0.36	3	BC																														N.McMillan	
D	TNDD028	1101.76	1102.12	REW	1	0.36	3	FO	JN		23	2		0-30	0-30								Planar	Planar		SM	RO		CL	CL								N.McMillan	Fractures are planar to undulating. Smooth-rough faces.
D	TNDD028	1102.12	1135.48	REW	1	33.36	4	JN	FO		35	8		60-90	0-30								Irregular	Planar		RO	RO		CL	CL								N.McMillan	Some joint fractures are along veins.
EOF
